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VILLA A68
Material Schedule
PROCUREMENT & EXECUTION · OPTIONS 1 AND 2
Room-by-room approved finishes for the ground floor, upper floor, exterior and outdoor areas. Descriptions reproduce the approved design; undefined technical details are not assumed.
ISSUE  01 · 02 October 2026
STATUS  Design intent schedule
SCOPE  61 room and external-area schedules
Approval notes
1. Reference codes are Villa A68 schedule identifiers, not manufacturer or product codes.
1. Descriptions reproduce the approved design specification; no substitute material has been introduced.
1. Where no manufacturer is fixed, items state "Supplier/Product Code to be selected" — material type, colour and finish remain as specified.
1. All finishes require an approved physical sample and shop drawing before purchase.
1. Final manufacturer, batch, technical build-up, fire rating, slip rating and wet-area system remain subject to approval where not stated.


Schedule reference key
	FAMILY
	MATERIAL GROUP
	APPROVAL BASIS
	STATUS

	ST-01 / ST-02
	Beige marble / dark emperador
	Approved natural-stone design intent
	Sample required

	ST-03 / ST-04
	Travertine / limestone
	Approved natural-stone design intent
	Sample required

	ST-05 / TL-01
	Sintered stone, quartz / porcelain
	Approved engineered-surface intent
	Sample required

	JN-01 / JN-02
	Smoked walnut / oak, teak and wood-effect
	Approved joinery design intent
	Shop drawing required

	WF-01
	Paint, plaster, micro-cement and render
	Approved colour and finish family
	Mock-up required

	MT-01 / GL-01
	Brass, bronze / clear or fluted glass
	Approved metal and glazing intent
	Sample required

	TX-01 / LT-01
	Textiles / decorative and architectural lighting
	Approved visual intent
	Cut sheet required

	LS-01 / FL-01
	Landscape planting / safety surfacing
	Approved landscape intent
	Submittal required




OPTION 1 · HIGH-END MODERN LUXURY
Main Entrance & Lobby
Ground floor  ·  4.20 m lobby width · 1.30 m opening to the living wing · stair and guest WC off the same space
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	ST-02 / ST-01 / MT-01
	[image: ] Dark Emperador
[image: ] Beige marble
	Floor / paving
	90×90 cm polished beige marble, straight set, with a central medallion in dark emperador framed by 5 cm brushed brass inlay lines.
	90 cm · 5 cm
	Main Entrance & Lobby — Flooring

	WF-01 / MT-01
	[image: ] Warm white paint
[image: ] Brushed brass
	Walls / paint
	Warm off-white polished plaster; one wall in vertical fluted cream stone as the console backdrop. Slim brass reveal at skirting level.
	TBC by sample/shop drawing
	Main Entrance & Lobby — Walls

	MT-01 / GL-01 / LT-01
	[image: ] Brushed brass
[image: ] Clear glass
	Ceiling
	Circular recessed drop with perimeter cove (3000 K indirect), trimless pinhole spots, and a vertical cascading brass-and-glass pendant on the medallion axis.
	3000 K
	Main Entrance & Lobby — Ceiling & lighting

	ST-01 / JN-02
	[image: ] Beige marble
[image: ] Natural oak / wood
	Joinery / woodwork
	Full-height flush cloak cupboard, push-to-open, finished in the wall colour so it reads as wall. Floating marble console, 2.20 m.
	2.20 m
	Main Entrance & Lobby — Joinery

	MT-01 / GL-01 / LS-01
	[image: ] Brushed brass
[image: ] Clear glass
	Special finish / equipment
	Arched brushed-brass mirror, paired alabaster-glass sconces, one sculptural planter. Nothing else — the lobby stays a threshold, not a room.
	TBC by sample/shop drawing
	Main Entrance & Lobby — Decorative

	ST-01
	[image: ] Beige marble
	Flooring
	Natural beige marble (Crema Marfil / Botticino type, warm cream), honed-polished satin, bookmatched in principal rooms. Supplier/Product Code to be selected.
	1200×600 mm slabs · 20 mm thick
	Main Entrance & Lobby — full floor area

	WF-01
	[image: ] Warm white paint
	Walls
	Gypsum skim plaster, smooth level-5 finish ready for paint
	Plaster 10–13 mm
	Main Entrance & Lobby — all walls except feature wall

	WF-01
	[image: ] Warm white paint
	Wall paint
	Wall paint: warm white / greige washable matt emulsion (Jotun Fenomastic or equal), 2 coats on primer. Supplier/Product Code to be selected.
	—
	Main Entrance & Lobby — all painted walls

	ST-02 / ST-03 / ST-01
	[image: ] Dark Emperador
[image: ] Travertine
	Feature wall
	Bookmatched Silver Travertine / Dark Emperador marble slab cladding. Supplier/Product Code to be selected.
	20 mm slabs, full-height bookmatch
	Main Entrance & Lobby — entrance feature wall

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Gypsum board ceiling, warm white matt paint, perimeter shadow-gap with 2700K LED cove, trimless downlights. Supplier/Product Code to be selected.
	12.5 mm board · 2.9–3.0 m FFL
	Main Entrance & Lobby — full ceiling

	WF-01 / MT-01
	[image: ] Warm white paint
[image: ] Brushed brass
	Skirting
	Recessed shadow-gap skirting, brushed brass (pvd or solid), satin lacquered trim / flush painted MDF
	80 mm high · 10 mm reveal
	Main Entrance & Lobby — all wall perimeters

	JN-01
	[image: ] Smoked walnut
	Joinery
	Smoked walnut veneer on MR-MDF, matt lacquer 10% sheen. Supplier/Product Code to be selected.
	18–22 mm core · 0.6 mm veneer
	Main Entrance & Lobby — built-in units and wall panelling

	JN-01 / LT-01
	[image: ] Smoked walnut
[image: ] 2700K LED
	Doors
	Full-height flush door, smoked walnut veneer, concealed frame and hinges, magnetic lock. Supplier/Product Code to be selected.
	900×2700 mm · 50 mm leaf
	Main Entrance & Lobby — entry door(s)

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Metal finishes
	Brushed brass (PVD or solid), satin lacquered — door handles, inlays, light fittings, joinery pulls. Supplier/Product Code to be selected.
	—
	Main Entrance & Lobby — all visible metalwork


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 1 · HIGH-END MODERN LUXURY
Formal Guest Lounge
Ground floor  ·  9.50 m long × 5.65 m deep — south wing, direct off the entrance, as dimensioned on the approved plan
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	ST-02 / MT-01 / LT-01
	[image: ] Dark Emperador
[image: ] Brushed brass
	Special finish / equipment
	1.60 m wide linear gas fireplace recessed into the panelled feature wall, framed in honed dark emperador with a brushed-brass shadow reveal and a floating stone hearth shelf. Flue routed in the existing partition depth — no structural change.
	1.60 m
	Formal Guest Lounge — Fireplace

	ST-02 / MT-01 / TX-01
	[image: ] Dark Emperador
[image: ] Brushed brass
	Special finish / equipment
	Custom modular sofas along three walls, 90 cm deep, deep taupe velvet, tailored no-skirt profile with brushed-brass capped legs. Two dark emperador cube side tables at the corners.
	90 cm
	Formal Guest Lounge — Furniture

	MT-01 / TX-01
	[image: ] Brushed brass
[image: ] Textiles
	Walls / paint
	Full-height upholstered fabric panels in warm sand, framed by 20 mm brushed-brass vertical profiles in a tall repeating rhythm — the room's signature treatment.
	20 mm
	Formal Guest Lounge — Feature wall

	MT-01 / GL-01 / LT-01
	[image: ] Brushed brass
[image: ] Clear glass
	Ceiling
	Stepped perimeter cove with warm indirect light, a large cascading brass-and-glass chandelier centred, and paired wall sconces between the panels.
	TBC by sample/shop drawing
	Formal Guest Lounge — Ceiling & lighting

	TX-01
	[image: ] Textiles
	Doors / window treatment
	Sheer linen inner layer plus heavy cream blackout drapery, both on a recessed ceiling track — no visible rod.
	TBC by sample/shop drawing
	Formal Guest Lounge — Curtains

	ST-01 / TX-01
	[image: ] Beige marble
[image: ] Textiles
	Floor / paving
	Polished beige marble with a 4×6 m cream low-pile rug sized so every seat's front legs land on it.
	6 m
	Formal Guest Lounge — Flooring

	ST-01
	[image: ] Beige marble
	Flooring
	Natural beige marble (Crema Marfil / Botticino type, warm cream), honed-polished satin, bookmatched in principal rooms. Supplier/Product Code to be selected.
	1200×600 mm slabs · 20 mm thick
	Formal Guest Lounge — full floor area

	WF-01
	[image: ] Warm white paint
	Walls
	Gypsum skim plaster, smooth level-5 finish ready for paint
	Plaster 10–13 mm
	Formal Guest Lounge — all walls except feature wall

	WF-01
	[image: ] Warm white paint
	Wall paint
	Wall paint: warm white / greige washable matt emulsion (Jotun Fenomastic or equal), 2 coats on primer. Supplier/Product Code to be selected.
	—
	Formal Guest Lounge — all painted walls

	ST-02 / ST-03 / ST-01
	[image: ] Dark Emperador
[image: ] Travertine
	Feature wall
	Bookmatched Silver Travertine / Dark Emperador marble slab cladding. Supplier/Product Code to be selected.
	20 mm slabs, full-height bookmatch
	Formal Guest Lounge — fireplace / TV wall

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Gypsum board ceiling, warm white matt paint, perimeter shadow-gap with 2700K LED cove, trimless downlights. Supplier/Product Code to be selected.
	12.5 mm board · 2.9–3.0 m FFL
	Formal Guest Lounge — full ceiling

	WF-01 / MT-01
	[image: ] Warm white paint
[image: ] Brushed brass
	Skirting
	Recessed shadow-gap skirting, brushed brass (pvd or solid), satin lacquered trim / flush painted MDF
	80 mm high · 10 mm reveal
	Formal Guest Lounge — all wall perimeters

	JN-01
	[image: ] Smoked walnut
	Joinery
	Smoked walnut veneer on MR-MDF, matt lacquer 10% sheen. Supplier/Product Code to be selected.
	18–22 mm core · 0.6 mm veneer
	Formal Guest Lounge — built-in units and wall panelling

	JN-01 / LT-01
	[image: ] Smoked walnut
[image: ] 2700K LED
	Doors
	Full-height flush door, smoked walnut veneer, concealed frame and hinges, magnetic lock. Supplier/Product Code to be selected.
	900×2700 mm · 50 mm leaf
	Formal Guest Lounge — entry door(s)

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Metal finishes
	Brushed brass (PVD or solid), satin lacquered — door handles, inlays, light fittings, joinery pulls. Supplier/Product Code to be selected.
	—
	Formal Guest Lounge — all visible metalwork

	ST-02 / ST-03 / ST-01 / MT-01
	[image: ] Dark Emperador
[image: ] Travertine
	Fireplace
	Linear built-in fireplace with bookmatched silver travertine / dark emperador marble slab cladding surround and brushed brass (pvd or solid), satin lacquered trim. Supplier/Product Code to be selected.
	1500–1800 mm firebox
	Formal Guest Lounge — fireplace wall


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 1 · HIGH-END MODERN LUXURY
Main Family Living Room
Ground floor  ·  9.41 × 6.90 m — north-west, open to the kitchen
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	ST-01 / JN-01 / MT-01 / LT-01
	[image: ] Beige marble
[image: ] Smoked walnut
	Walls / paint
	Full-width book-matched beige marble with a recessed screen niche framed in a 20 mm brass reveal; 3.60 m floating smoked-walnut console with a shadow-gap LED beneath.
	20 mm · 3.60 m
	Main Family Living Room — TV feature wall

	ST-01 / LT-01
	[image: ] Beige marble
[image: ] 2700K LED
	Special finish / equipment
	A 1.80 m linear gas fireplace sits directly under the screen niche inside the same marble plane, so TV, fire and console read as one architectural composition rather than three added objects. Stone returns 60 cm above the opening; heat break and flue concealed within the wall build-up.
	1.80 m · 60 cm
	Main Family Living Room — Fireplace integration

	JN-02
	[image: ] Natural oak / wood
	Walls / paint
	Vertical oak slat panelling (40 mm slats / 20 mm gaps) on dark acoustic backing along the long internal wall — controls echo in a room this size.
	40 mm · 20 mm
	Main Family Living Room — Accent wall

	ST-03 / ST-01 / MT-01 / TX-01
	[image: ] Travertine
[image: ] Beige marble
	Special finish / equipment
	Cream bouclé four-seat sofa, four taupe velvet lounge chairs, travertine-and-brass coffee table; second bay with two facing taupe sofas and a marble-top table.
	TBC by sample/shop drawing
	Main Family Living Room — Furniture

	ST-01 / MT-01 / LT-01
	[image: ] Beige marble
[image: ] Brushed brass
	Ceiling
	Stepped cove with brass reveal, two matching brass-and-alabaster globe chandeliers (one per bay), wall-grazing spots on the marble, two brass floor lamps.
	TBC by sample/shop drawing
	Main Family Living Room — Ceiling & lighting

	MT-01 / TX-01
	[image: ] Brushed brass
[image: ] Textiles
	Special finish / equipment
	Cream silk-blend rugs per cluster, sheer linen with cream blackout drapery on recessed track, bronze and cream silk cushions.
	TBC by sample/shop drawing
	Main Family Living Room — Textiles

	ST-01
	[image: ] Beige marble
	Flooring
	Natural beige marble (Crema Marfil / Botticino type, warm cream), honed-polished satin, bookmatched in principal rooms. Supplier/Product Code to be selected.
	1200×600 mm slabs · 20 mm thick
	Main Family Living Room — full floor area

	WF-01
	[image: ] Warm white paint
	Walls
	Gypsum skim plaster, smooth level-5 finish ready for paint
	Plaster 10–13 mm
	Main Family Living Room — all walls except feature wall

	WF-01
	[image: ] Warm white paint
	Wall paint
	Wall paint: warm white / greige washable matt emulsion (Jotun Fenomastic or equal), 2 coats on primer. Supplier/Product Code to be selected.
	—
	Main Family Living Room — all painted walls

	ST-02 / ST-03 / ST-01
	[image: ] Dark Emperador
[image: ] Travertine
	Feature wall
	Bookmatched Silver Travertine / Dark Emperador marble slab cladding. Supplier/Product Code to be selected.
	20 mm slabs, full-height bookmatch
	Main Family Living Room — fireplace / TV wall

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Gypsum board ceiling, warm white matt paint, perimeter shadow-gap with 2700K LED cove, trimless downlights. Supplier/Product Code to be selected.
	12.5 mm board · 2.9–3.0 m FFL
	Main Family Living Room — full ceiling

	WF-01 / MT-01
	[image: ] Warm white paint
[image: ] Brushed brass
	Skirting
	Recessed shadow-gap skirting, brushed brass (pvd or solid), satin lacquered trim / flush painted MDF
	80 mm high · 10 mm reveal
	Main Family Living Room — all wall perimeters

	JN-01
	[image: ] Smoked walnut
	Joinery
	Smoked walnut veneer on MR-MDF, matt lacquer 10% sheen. Supplier/Product Code to be selected.
	18–22 mm core · 0.6 mm veneer
	Main Family Living Room — built-in units and wall panelling

	JN-01 / LT-01
	[image: ] Smoked walnut
[image: ] 2700K LED
	Doors
	Full-height flush door, smoked walnut veneer, concealed frame and hinges, magnetic lock. Supplier/Product Code to be selected.
	900×2700 mm · 50 mm leaf
	Main Family Living Room — entry door(s)

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Metal finishes
	Brushed brass (PVD or solid), satin lacquered — door handles, inlays, light fittings, joinery pulls. Supplier/Product Code to be selected.
	—
	Main Family Living Room — all visible metalwork

	ST-02 / ST-03 / ST-01 / MT-01
	[image: ] Dark Emperador
[image: ] Travertine
	Fireplace
	Linear built-in fireplace with bookmatched silver travertine / dark emperador marble slab cladding surround and brushed brass (pvd or solid), satin lacquered trim. Supplier/Product Code to be selected.
	1500–1800 mm firebox
	Main Family Living Room — fireplace wall


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 1 · HIGH-END MODERN LUXURY
Dining Area
Ground floor  ·  5.65 m deep × 4.20 m — north-east of the guest lounge, on the kitchen side, exactly as drawn
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	ST-01 / JN-01 / MT-01
	[image: ] Beige marble
[image: ] Smoked walnut
	Countertops / stone
	Custom 1.80 m round table, solid beige marble top on a sculpted smoked-walnut pedestal; eight cream leather chairs with walnut frames and brass sabots.
	1.80 m
	Dining Area — Table & seating

	ST-01 / JN-01 / GL-01 / LT-01
	[image: ] Beige marble
[image: ] Smoked walnut
	Joinery / woodwork
	Full-height smoked-walnut buffet and crockery unit with fluted-glass doors, internal LED, marble top returning 10 cm up the wall.
	10 cm
	Dining Area — Joinery

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Special finish / equipment
	Round multi-tier brass chandelier with alabaster diffusers, hung 80 cm above the table, on a dedicated dimmer. Cove light for ambience only.
	80 cm
	Dining Area — Lighting

	WF-01 / MT-01 / LT-01
	[image: ] Warm white paint
[image: ] Brushed brass
	Walls / paint
	Cream plaster with a large antique-bronze mirror panel opposite the window to double daylight and widen the zone visually.
	TBC by sample/shop drawing
	Dining Area — Walls

	ST-01
	[image: ] Beige marble
	Flooring
	Natural beige marble (Crema Marfil / Botticino type, warm cream), honed-polished satin, bookmatched in principal rooms. Supplier/Product Code to be selected.
	1200×600 mm slabs · 20 mm thick
	Dining Area — full floor area

	WF-01
	[image: ] Warm white paint
	Walls
	Gypsum skim plaster, smooth level-5 finish ready for paint
	Plaster 10–13 mm
	Dining Area — all walls except feature wall

	WF-01
	[image: ] Warm white paint
	Wall paint
	Wall paint: warm white / greige washable matt emulsion (Jotun Fenomastic or equal), 2 coats on primer. Supplier/Product Code to be selected.
	—
	Dining Area — all painted walls

	ST-02 / ST-03 / ST-01
	[image: ] Dark Emperador
[image: ] Travertine
	Feature wall
	Bookmatched Silver Travertine / Dark Emperador marble slab cladding. Supplier/Product Code to be selected.
	20 mm slabs, full-height bookmatch
	Dining Area — dining feature wall

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Gypsum board ceiling, warm white matt paint, perimeter shadow-gap with 2700K LED cove, trimless downlights. Supplier/Product Code to be selected.
	12.5 mm board · 2.9–3.0 m FFL
	Dining Area — full ceiling

	WF-01 / MT-01
	[image: ] Warm white paint
[image: ] Brushed brass
	Skirting
	Recessed shadow-gap skirting, brushed brass (pvd or solid), satin lacquered trim / flush painted MDF
	80 mm high · 10 mm reveal
	Dining Area — all wall perimeters

	JN-01
	[image: ] Smoked walnut
	Joinery
	Smoked walnut veneer on MR-MDF, matt lacquer 10% sheen. Supplier/Product Code to be selected.
	18–22 mm core · 0.6 mm veneer
	Dining Area — built-in units and wall panelling

	JN-01 / LT-01
	[image: ] Smoked walnut
[image: ] 2700K LED
	Doors
	Full-height flush door, smoked walnut veneer, concealed frame and hinges, magnetic lock. Supplier/Product Code to be selected.
	900×2700 mm · 50 mm leaf
	Dining Area — entry door(s)

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Metal finishes
	Brushed brass (PVD or solid), satin lacquered — door handles, inlays, light fittings, joinery pulls. Supplier/Product Code to be selected.
	—
	Dining Area — all visible metalwork

	ST-01 / JN-01 / JN-02
	[image: ] Beige marble
[image: ] Smoked walnut
	Countertops / stone
	Dining table top in beige marble (matching floor family), honed, eased 2 mm edge; walnut/oak sideboard. Supplier/Product Code to be selected.
	20–30 mm
	Dining Area — table & sideboard


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 1 · HIGH-END MODERN LUXURY
Kitchen
Ground floor  ·  North band of the 12.00 m frontage — open to the living and dining areas, sink under the north window, service door to the maid's room
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	JN-01
	[image: ] Smoked walnut
	Joinery / woodwork
	Handleless floor-to-ceiling matte cream lacquer for the tall run; smoked-walnut veneer for the island and low units. Appliances fully integrated behind panels except one statement oven column.
	TBC by sample/shop drawing
	Kitchen — Cabinetry

	ST-01 / ST-05
	[image: ] Beige marble
[image: ] Quartz
	Floor / paving
	Beige marble-effect sintered stone counters (durability over natural marble at the worktop), full-height book-matched splashback behind the hob.
	TBC by sample/shop drawing
	Kitchen — Surfaces

	MT-01
	[image: ] Brushed brass
	Countertops / stone
	Waterfall edge with a 35 cm overhang for three brass-and-leather stools; recessed brass power module in the top.
	35 cm
	Kitchen — Island

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Special finish / equipment
	Three slim brass pendants over the island, under-cabinet task LED, toe-kick glow for night use. All 3000 K to match the living wing.
	3000 K
	Kitchen — Lighting

	ST-01
	[image: ] Beige marble
	Flooring
	Natural beige marble (Crema Marfil / Botticino type, warm cream), honed-polished satin, bookmatched in principal rooms. Supplier/Product Code to be selected.
	1200×600 mm slabs · 20 mm thick
	Kitchen — full floor area

	WF-01
	[image: ] Warm white paint
	Walls
	Gypsum skim plaster, smooth level-5 finish ready for paint
	Plaster 10–13 mm
	Kitchen — all walls except feature wall

	WF-01
	[image: ] Warm white paint
	Wall paint
	Wall paint: warm white / greige washable matt emulsion (Jotun Fenomastic or equal), 2 coats on primer. Supplier/Product Code to be selected.
	—
	Kitchen — all painted walls

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Gypsum board ceiling, warm white matt paint, perimeter shadow-gap with 2700K LED cove, trimless downlights. Supplier/Product Code to be selected.
	12.5 mm board · 2.9–3.0 m FFL
	Kitchen — full ceiling

	WF-01 / MT-01
	[image: ] Warm white paint
[image: ] Brushed brass
	Skirting
	Recessed shadow-gap skirting, brushed brass (pvd or solid), satin lacquered trim / flush painted MDF
	80 mm high · 10 mm reveal
	Kitchen — all wall perimeters

	JN-01
	[image: ] Smoked walnut
	Joinery
	Smoked walnut veneer on MR-MDF, matt lacquer 10% sheen. Supplier/Product Code to be selected.
	18–22 mm core · 0.6 mm veneer
	Kitchen — built-in units and wall panelling

	JN-01 / LT-01
	[image: ] Smoked walnut
[image: ] 2700K LED
	Doors
	Full-height flush door, smoked walnut veneer, concealed frame and hinges, magnetic lock. Supplier/Product Code to be selected.
	900×2700 mm · 50 mm leaf
	Kitchen — entry door(s)

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Metal finishes
	Brushed brass (PVD or solid), satin lacquered — door handles, inlays, light fittings, joinery pulls. Supplier/Product Code to be selected.
	—
	Kitchen — all visible metalwork

	JN-01
	[image: ] Smoked walnut
	Kitchen cabinets
	Smoked walnut veneer tall units + warm taupe matt lacquer base units, handleless J-profile, soft-close hinges & drawers. Supplier/Product Code to be selected.
	18 mm carcass · 600 mm base depth
	Kitchen — base, wall, tall units and island

	ST-01 / ST-05
	[image: ] Beige marble
[image: ] Quartz
	Kitchen countertop
	Beige / Calacatta-tone marble or sintered stone, honed. Supplier/Product Code to be selected.
	20 mm + 40 mm mitred edge / waterfall island
	Kitchen — worktops and island

	ST-01 / ST-05
	[image: ] Beige marble
[image: ] Quartz
	Backsplash
	Full-height slab in matching beige / calacatta-tone marble or sintered stone. Supplier/Product Code to be selected.
	Slab to underside of wall units
	Kitchen — cooking and sink walls


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 1 · HIGH-END MODERN LUXURY
Staircase
Ground floor  ·  2.15 m wide flight · 20 risers · 2.81 m landing
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	ST-01 / MT-01 / LT-01
	[image: ] Beige marble
[image: ] Brushed brass
	Floor / paving
	Beige marble treads with a 15 mm brushed-brass nosing inlay; closed risers in matte cream to keep the flight light.
	15 mm
	Staircase — Treads & risers

	JN-01 / GL-01
	[image: ] Smoked walnut
[image: ] Clear glass
	Metal / fittings
	Frameless 12 mm clear laminated glass panels in a slim recessed stainless channel, with a smoked-walnut cap handrail on the wall side — contemporary, clean and fully transparent to the lobby.
	12 mm
	Staircase — Balustrade

	MT-01 / GL-01 / LT-01
	[image: ] Brushed brass
[image: ] Clear glass
	Special finish / equipment
	Continuous LED washing the underside of the handrail plus a vertical cascading brass-and-glass feature in the void, visible from the lobby.
	TBC by sample/shop drawing
	Staircase — Lighting

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Walls / paint
	Warm greige limewash plaster with one large sculptural artwork; the understair volume becomes flush concealed storage.
	TBC by sample/shop drawing
	Staircase — Wall & understair

	ST-01
	[image: ] Beige marble
	Staircase treads
	Solid beige marble treads & risers, honed, 3 anti-slip grooves to nosing. Supplier/Product Code to be selected.
	Tread 300 mm · riser 160–170 mm · 20–30 mm
	Staircase — all flights and landings

	GL-01
	[image: ] Clear glass
	Balustrade
	Clear frameless laminated toughened glass in recessed floor channel, no handrail rods. Supplier/Product Code to be selected.
	12+12 mm laminated · 1100 mm high
	Staircase — open side of flights and landing

	MT-01
	[image: ] Brushed brass
	Handrail
	Brushed brass (PVD or solid), satin lacquered slim wall-mounted handrail. Supplier/Product Code to be selected.
	Ø40 mm
	Staircase — wall side

	LT-01
	[image: ] 2700K LED
	Stair lighting
	Recessed 2700K LED step lights / under-tread LED strip. Supplier/Product Code to be selected.
	—
	Staircase — every 2nd step

	WF-01
	[image: ] Warm white paint
	Walls
	Gypsum skim plaster, smooth level-5 finish
	—
	Staircase — stairwell walls

	WF-01
	[image: ] Warm white paint
	Wall paint
	Wall paint: warm white / greige washable matt emulsion (Jotun Fenomastic or equal), 2 coats on primer. Supplier/Product Code to be selected.
	—
	Staircase — stairwell walls

	ST-02 / ST-03 / ST-01
	[image: ] Dark Emperador
[image: ] Travertine
	Feature wall
	Bookmatched Silver Travertine / Dark Emperador marble slab cladding. Supplier/Product Code to be selected.
	20 mm slabs, full-height bookmatch
	Staircase — double-height stair wall

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Gypsum board ceiling, warm white matt paint, perimeter shadow-gap with 2700K LED cove, trimless downlights; feature pendant to double-height void. Supplier/Product Code to be selected.
	—
	Staircase — soffit and void

	ST-01
	[image: ] Beige marble
	Skirting
	Stringer skirting in matching solid beige marble treads & risers
	100 mm
	Staircase — wall stringer


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 1 · HIGH-END MODERN LUXURY
Guest WCs
Ground floor  ·  Guest WC 2.40 × 1.20 m off the lobby · second WC 1.82 m wide on the maid's-room side, both as drawn
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	ST-02 / JN-01
	[image: ] Dark Emperador
[image: ] Smoked walnut
	Special finish / equipment
	Full-height book-matched dark emperador on the vanity wall, honed beige stone elsewhere, floating smoked-walnut vanity with an integrated stone basin.
	TBC by sample/shop drawing
	Guest WCs — Guest powder room

	ST-03 / JN-02 / MT-01 / LT-01
	[image: ] Travertine
[image: ] Natural oak / wood
	Special finish / equipment
	Honed travertine walls and floor, light oak vanity, stone vessel basin, round brass-framed backlit mirror.
	TBC by sample/shop drawing
	Guest WCs — Second WC

	LT-01
	[image: ] 2700K LED
	Special finish / equipment
	Backlit mirrors, a lit niche for accessories, and perimeter cove — no downlight directly over the mirror.
	TBC by sample/shop drawing
	Guest WCs — Lighting

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Metal / fittings
	Brushed-brass wall-mounted tapware, concealed cistern with a brass flush plate, wall-hung pan.
	TBC by sample/shop drawing
	Guest WCs — Fittings

	ST-01
	[image: ] Beige marble
	Bathroom floor
	Beige marble, honed anti-slip (R10) finish. Supplier/Product Code to be selected.
	600×600 mm · laid to falls
	Guest WCs — full floor

	ST-01
	[image: ] Beige marble
	Bathroom walls
	Beige marble full-height cladding, honed. Supplier/Product Code to be selected.
	1200×600 mm · 15–20 mm
	Guest WCs — full-height wet walls

	WF-01
	[image: ] Warm white paint
	Wall paint
	Moisture- and mould-resistant matt emulsion, warm white, 2 coats on primer. Supplier/Product Code to be selected.
	—
	Guest WCs — non-tiled wall areas

	ST-02 / ST-03 / ST-01
	[image: ] Dark Emperador
[image: ] Travertine
	Feature wall
	Bookmatched Silver Travertine / Dark Emperador marble slab cladding behind vanity with backlit mirror. Supplier/Product Code to be selected.
	20 mm slabs, full-height bookmatch
	Guest WCs — vanity wall

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Moisture-resistant (MR) gypsum ceiling, anti-mould warm white matt paint, IP44 trimless downlights. Supplier/Product Code to be selected.
	12.5 mm MR board
	Guest WCs — full ceiling

	JN-01 / LT-01
	[image: ] Smoked walnut
[image: ] 2700K LED
	Vanity
	Wall-hung vanity, smoked walnut veneer on mr-mdf, matt lacquer 10% sheen, soft-close drawers, LED under-glow. Supplier/Product Code to be selected.
	550 mm deep
	Guest WCs — vanity wall

	ST-01
	[image: ] Beige marble
	Countertop
	Beige marble top with integrated moulded basin, honed. Supplier/Product Code to be selected.
	20 mm
	Guest WCs — vanity

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Sanitaryware
	Wall-hung rimless WC with concealed cistern, white gloss; brushed brass (pvd or solid), satin lacquered flush plate & mixers. Supplier/Product Code to be selected.
	—
	Guest WCs — WC and basin

	MT-01
	[image: ] Brushed brass
	Metal finishes
	Brushed brass (PVD or solid), satin lacquered — taps, shower set, towel rail, accessories. Supplier/Product Code to be selected.
	—
	Guest WCs — all fittings

	JN-01 / LT-01
	[image: ] Smoked walnut
[image: ] 2700K LED
	Doors
	Full-height flush door, smoked walnut veneer, concealed frame and hinges, magnetic lock, moisture-resistant core. Supplier/Product Code to be selected.
	800×2700 mm
	Guest WCs — entry door


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 1 · HIGH-END MODERN LUXURY
Corridors & Transitional Areas
Ground floor  ·  Lobby-to-wing links and the service passage
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	ST-01 / MT-01
	[image: ] Beige marble
[image: ] Brushed brass
	Floor / paving
	Continuous beige marble with a 5 cm brass inlay strip marking the transition between the guest wing and the family wing.
	5 cm
	Corridors & Transitional Areas — Flooring

	JN-01 / WF-01 / MT-01
	[image: ] Smoked walnut
[image: ] Warm white paint
	Doors / window treatment
	Full-height flush smoked-walnut doors with vertical brass handles; service doors painted flush to the wall so they disappear.
	TBC by sample/shop drawing
	Corridors & Transitional Areas — Doors

	LT-01
	[image: ] 2700K LED
	Special finish / equipment
	Linear ceiling cove plus discreet pinhole spots grazing the wall — deliberately dimmer than the rooms it serves.
	TBC by sample/shop drawing
	Corridors & Transitional Areas — Lighting

	SP-01
	[image: ] Dark bronze / special
	Special finish / equipment
	One console with a single sculptural object and one framed abstract per run. Restraint is the point.
	TBC by sample/shop drawing
	Corridors & Transitional Areas — Art

	ST-01
	[image: ] Beige marble
	Flooring
	Natural beige marble (Crema Marfil / Botticino type, warm cream), honed-polished satin, bookmatched in principal rooms. Supplier/Product Code to be selected.
	1200×600 mm slabs · 20 mm thick
	Corridors & Transitional Areas — full floor area

	WF-01
	[image: ] Warm white paint
	Walls
	Gypsum skim plaster, smooth level-5 finish ready for paint
	Plaster 10–13 mm
	Corridors & Transitional Areas — all walls except feature wall

	WF-01
	[image: ] Warm white paint
	Wall paint
	Wall paint: warm white / greige washable matt emulsion (Jotun Fenomastic or equal), 2 coats on primer. Supplier/Product Code to be selected.
	—
	Corridors & Transitional Areas — all painted walls

	ST-02 / ST-03 / ST-01
	[image: ] Dark Emperador
[image: ] Travertine
	Feature wall
	Bookmatched Silver Travertine / Dark Emperador marble slab cladding. Supplier/Product Code to be selected.
	20 mm slabs, full-height bookmatch
	Corridors & Transitional Areas — end wall of corridor

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Gypsum board ceiling, warm white matt paint, perimeter shadow-gap with 2700K LED cove, trimless downlights. Supplier/Product Code to be selected.
	12.5 mm board · 2.9–3.0 m FFL
	Corridors & Transitional Areas — full ceiling

	WF-01 / MT-01
	[image: ] Warm white paint
[image: ] Brushed brass
	Skirting
	Recessed shadow-gap skirting, brushed brass (pvd or solid), satin lacquered trim / flush painted MDF
	80 mm high · 10 mm reveal
	Corridors & Transitional Areas — all wall perimeters

	JN-01
	[image: ] Smoked walnut
	Joinery
	Smoked walnut veneer on MR-MDF, matt lacquer 10% sheen. Supplier/Product Code to be selected.
	18–22 mm core · 0.6 mm veneer
	Corridors & Transitional Areas — built-in units and wall panelling

	JN-01 / LT-01
	[image: ] Smoked walnut
[image: ] 2700K LED
	Doors
	Full-height flush door, smoked walnut veneer, concealed frame and hinges, magnetic lock. Supplier/Product Code to be selected.
	900×2700 mm · 50 mm leaf
	Corridors & Transitional Areas — entry door(s)

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Metal finishes
	Brushed brass (PVD or solid), satin lacquered — door handles, inlays, light fittings, joinery pulls. Supplier/Product Code to be selected.
	—
	Corridors & Transitional Areas — all visible metalwork


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 1 · HIGH-END MODERN LUXURY
Maid's Room, Service WC & Boiler
Ground floor  ·  Maid's room on the north-east corner as drawn · service WC 1.82 m · boiler 1.60 m recess off the stair core
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	JN-02
	[image: ] Natural oak / wood
	Special finish / equipment
	Single bed with an upholstered head panel, full-height oak-veneer wardrobe with an open shelf bay, 1.10 m desk, blackout roller blind on the drawn window.
	1.10 m
	Maid's Room, Service WC & Boiler — Maid's room

	ST-03 / TL-01 / LT-01
	[image: ] Travertine
[image: ] Marble-look porcelain
	Special finish / equipment
	Travertine-look porcelain to full height, wall-hung pan with a concealed cistern, compact stone-top vanity — plumbing kept exactly on the drawn wet wall.
	TBC by sample/shop drawing
	Maid's Room, Service WC & Boiler — Service WC

	SP-01
	[image: ] Dark bronze / special
	Special finish / equipment
	Stacked washer-dryer in a ventilated niche behind flush doors, with the boiler recess off the stair core retained in its drawn position and given a louvred access panel.
	TBC by sample/shop drawing
	Maid's Room, Service WC & Boiler — Laundry & boiler

	TL-01 / WF-01 / LT-01
	[image: ] Marble-look porcelain
[image: ] Warm white paint
	Walls / paint
	Warm greige paint, matte beige porcelain floor, one cove plus recessed spots at 3000 K to match the rest of the ground floor.
	3000 K
	Maid's Room, Service WC & Boiler — Finishes & lighting

	ST-01
	[image: ] Beige marble
	Flooring
	Natural beige marble (Crema Marfil / Botticino type, warm cream), honed-polished satin, bookmatched in principal rooms. Supplier/Product Code to be selected.
	1200×600 mm slabs · 20 mm thick
	Maid's Room, Service WC & Boiler — full floor area

	WF-01
	[image: ] Warm white paint
	Walls
	Gypsum skim plaster, smooth level-5 finish ready for paint
	Plaster 10–13 mm
	Maid's Room, Service WC & Boiler — all walls except feature wall

	WF-01
	[image: ] Warm white paint
	Wall paint
	Wall paint: warm white / greige washable matt emulsion (Jotun Fenomastic or equal), 2 coats on primer. Supplier/Product Code to be selected.
	—
	Maid's Room, Service WC & Boiler — all painted walls

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Gypsum board ceiling, warm white matt paint, perimeter shadow-gap with 2700K LED cove, trimless downlights. Supplier/Product Code to be selected.
	12.5 mm board · 2.9–3.0 m FFL
	Maid's Room, Service WC & Boiler — full ceiling

	WF-01 / MT-01
	[image: ] Warm white paint
[image: ] Brushed brass
	Skirting
	Recessed shadow-gap skirting, brushed brass (pvd or solid), satin lacquered trim / flush painted MDF
	80 mm high · 10 mm reveal
	Maid's Room, Service WC & Boiler — all wall perimeters

	JN-01
	[image: ] Smoked walnut
	Joinery
	Smoked walnut veneer on MR-MDF, matt lacquer 10% sheen. Supplier/Product Code to be selected.
	18–22 mm core · 0.6 mm veneer
	Maid's Room, Service WC & Boiler — built-in units and wall panelling

	JN-01 / LT-01
	[image: ] Smoked walnut
[image: ] 2700K LED
	Doors
	Full-height flush door, smoked walnut veneer, concealed frame and hinges, magnetic lock. Supplier/Product Code to be selected.
	900×2700 mm · 50 mm leaf
	Maid's Room, Service WC & Boiler — entry door(s)

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Metal finishes
	Brushed brass (PVD or solid), satin lacquered — door handles, inlays, light fittings, joinery pulls. Supplier/Product Code to be selected.
	—
	Maid's Room, Service WC & Boiler — all visible metalwork

	ST-01
	[image: ] Beige marble
	Bathroom floor
	Beige marble, honed anti-slip (R10) finish. Supplier/Product Code to be selected.
	600×600 mm · laid to falls
	Maid's Room, Service WC & Boiler (service WC) — full floor

	ST-01
	[image: ] Beige marble
	Bathroom walls
	Beige marble full-height cladding, honed. Supplier/Product Code to be selected.
	1200×600 mm · 15–20 mm
	Maid's Room, Service WC & Boiler (service WC) — full-height wet walls

	WF-01
	[image: ] Warm white paint
	Wall paint
	Moisture- and mould-resistant matt emulsion, warm white, 2 coats on primer. Supplier/Product Code to be selected.
	—
	Maid's Room, Service WC & Boiler (service WC) — non-tiled wall areas

	ST-02 / ST-03 / ST-01
	[image: ] Dark Emperador
[image: ] Travertine
	Feature wall
	Bookmatched Silver Travertine / Dark Emperador marble slab cladding behind vanity with backlit mirror. Supplier/Product Code to be selected.
	20 mm slabs, full-height bookmatch
	Maid's Room, Service WC & Boiler (service WC) — vanity wall

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Moisture-resistant (MR) gypsum ceiling, anti-mould warm white matt paint, IP44 trimless downlights. Supplier/Product Code to be selected.
	12.5 mm MR board
	Maid's Room, Service WC & Boiler (service WC) — full ceiling

	JN-01 / LT-01
	[image: ] Smoked walnut
[image: ] 2700K LED
	Vanity
	Wall-hung vanity, smoked walnut veneer on mr-mdf, matt lacquer 10% sheen, soft-close drawers, LED under-glow. Supplier/Product Code to be selected.
	550 mm deep
	Maid's Room, Service WC & Boiler (service WC) — vanity wall

	ST-01 / GL-01 / LT-01
	[image: ] Beige marble
[image: ] Clear glass
	Shower area
	Beige marble walls, fluted marble niche, 10 mm low-iron frameless glass screen; linear drain with tile insert; concealed thermostatic mixer & ceiling rain head. Supplier/Product Code to be selected.
	Screen 10 mm · drain 800 mm
	Maid's Room, Service WC & Boiler (service WC) — walk-in shower

	ST-01
	[image: ] Beige marble
	Countertop
	Beige marble top with integrated moulded basin, honed. Supplier/Product Code to be selected.
	20 mm
	Maid's Room, Service WC & Boiler (service WC) — vanity

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Sanitaryware
	Wall-hung rimless WC with concealed cistern, white gloss; brushed brass (pvd or solid), satin lacquered flush plate & mixers. Supplier/Product Code to be selected.
	—
	Maid's Room, Service WC & Boiler (service WC) — WC and basin

	MT-01
	[image: ] Brushed brass
	Metal finishes
	Brushed brass (PVD or solid), satin lacquered — taps, shower set, towel rail, accessories. Supplier/Product Code to be selected.
	—
	Maid's Room, Service WC & Boiler (service WC) — all fittings

	JN-01 / LT-01
	[image: ] Smoked walnut
[image: ] 2700K LED
	Doors
	Full-height flush door, smoked walnut veneer, concealed frame and hinges, magnetic lock, moisture-resistant core. Supplier/Product Code to be selected.
	800×2700 mm
	Maid's Room, Service WC & Boiler (service WC) — entry door


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 1 · HIGH-END MODERN LUXURY
Central Upper Lobby
Upper floor  ·  3.75 m × 2.50 m clear circulation · four bedroom doors and the stair void
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	ST-01 / MT-01 / TX-01
	[image: ] Beige marble
[image: ] Brushed brass
	Floor / paving
	The same 90×90 cm polished beige marble as the ground floor, straight set, with a 3 cm brushed brass inlay border tracing the lobby perimeter. A hand-loomed greige silk-wool runner softens the centre.
	90 cm · 3 cm
	Central Upper Lobby — Flooring

	JN-01 / WF-01 / MT-01
	[image: ] Smoked walnut
[image: ] Warm white paint
	Walls / paint
	Warm cream polished plaster with slim vertical panel reveals. All four bedroom doors are full-height smoked walnut, flush with the panelling, with recessed brushed brass pulls — identical detailing so the lobby reads calm.
	TBC by sample/shop drawing
	Central Upper Lobby — Walls & doors

	GL-01 / LT-01
	[image: ] Clear glass
[image: ] 2700K LED
	Ceiling
	Stepped gypsum perimeter with continuous 3000 K cove, trimless pinhole spots on the doors, one small sculptural glass pendant on axis, plus a dedicated 3000 K under-cabinet LED strip and a backlit open niche in the pantry. Night circuit at 5% on the cove and niche only.
	3000 K · 3000 K · 5%
	Central Upper Lobby — Ceiling & lighting

	ST-05 / JN-01 / MT-01 / LT-01
	[image: ] Quartz
[image: ] Smoked walnut
	Joinery / woodwork
	A 1.60 m full-height built-in dry pantry, flush with the wall panelling: handleless beige-taupe lacquer and smoked-walnut lower cabinets with concealed pull-out storage, a 20 mm honed beige sintered-stone worktop with matching full-height splashback, a small undermount sink with a slim brushed-brass mixer, walnut upper cabinets on push-to-open, and a backlit open niche between them for the coffee machine, kettle and crockery. Brushed-brass sockets and USB points are recessed in the niche splashback, with a shadow-gap toe kick and brass reveals framing the unit.
	1.60 m · 20 mm
	Central Upper Lobby — Preparation pantry

	ST-01 / JN-01 / WF-01 / MT-01 / TX-01
	[image: ] Beige marble
[image: ] Smoked walnut
	Special finish / equipment
	Beige marble · smoked walnut · cream plaster · brushed brass · greige silk-wool.
	TBC by sample/shop drawing
	Central Upper Lobby — Materials

	ST-01
	[image: ] Beige marble
	Flooring
	Natural beige marble (Crema Marfil / Botticino type, warm cream), honed-polished satin, bookmatched in principal rooms. Supplier/Product Code to be selected.
	1200×600 mm slabs · 20 mm thick
	Central Upper Lobby — full floor area

	WF-01
	[image: ] Warm white paint
	Walls
	Gypsum skim plaster, smooth level-5 finish ready for paint
	Plaster 10–13 mm
	Central Upper Lobby — all walls except feature wall

	WF-01
	[image: ] Warm white paint
	Wall paint
	Wall paint: warm white / greige washable matt emulsion (Jotun Fenomastic or equal), 2 coats on primer. Supplier/Product Code to be selected.
	—
	Central Upper Lobby — all painted walls

	ST-02 / ST-03 / ST-01
	[image: ] Dark Emperador
[image: ] Travertine
	Feature wall
	Bookmatched Silver Travertine / Dark Emperador marble slab cladding. Supplier/Product Code to be selected.
	20 mm slabs, full-height bookmatch
	Central Upper Lobby — pantry wall

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Gypsum board ceiling, warm white matt paint, perimeter shadow-gap with 2700K LED cove, trimless downlights. Supplier/Product Code to be selected.
	12.5 mm board · 2.9–3.0 m FFL
	Central Upper Lobby — full ceiling

	WF-01 / MT-01
	[image: ] Warm white paint
[image: ] Brushed brass
	Skirting
	Recessed shadow-gap skirting, brushed brass (pvd or solid), satin lacquered trim / flush painted MDF
	80 mm high · 10 mm reveal
	Central Upper Lobby — all wall perimeters

	JN-01
	[image: ] Smoked walnut
	Joinery
	Smoked walnut veneer on MR-MDF, matt lacquer 10% sheen. Supplier/Product Code to be selected.
	18–22 mm core · 0.6 mm veneer
	Central Upper Lobby — built-in units and wall panelling

	JN-01 / LT-01
	[image: ] Smoked walnut
[image: ] 2700K LED
	Doors
	Full-height flush door, smoked walnut veneer, concealed frame and hinges, magnetic lock. Supplier/Product Code to be selected.
	900×2700 mm · 50 mm leaf
	Central Upper Lobby — entry door(s)

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Metal finishes
	Brushed brass (PVD or solid), satin lacquered — door handles, inlays, light fittings, joinery pulls. Supplier/Product Code to be selected.
	—
	Central Upper Lobby — all visible metalwork

	JN-01
	[image: ] Smoked walnut
	Kitchen cabinets
	Built-in pantry, warm beige/taupe matt lacquer lower & upper units with smoked walnut veneer on mr-mdf, matt lacquer 10% sheen open niche. Supplier/Product Code to be selected.
	600 / 350 mm deep
	Central Upper Lobby — pantry wall

	ST-01
	[image: ] Beige marble
	Kitchen countertop
	Beige marble (matching floor family), honed, eased 2 mm edge with small undermount sink. Supplier/Product Code to be selected.
	20 mm
	Central Upper Lobby — pantry

	LT-01
	[image: ] 2700K LED
	Backsplash
	Matching stone slab with under-cabinet LED. Supplier/Product Code to be selected.
	Full height between units
	Central Upper Lobby — pantry


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 1 · HIGH-END MODERN LUXURY
Staircase Landing & Feature Wall
Upper floor  ·  Stair 2.15 m wide arriving on the east side of the lobby
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	ST-04 / LT-01
	[image: ] Limestone
[image: ] 2700K LED
	Walls / paint
	Full-height vertically fluted cream limestone, 60 mm pitch, grazed from a concealed slot at ceiling level so the flutes read as light and shadow rather than as texture alone.
	60 mm
	Staircase Landing & Feature Wall — Feature wall

	GL-01
	[image: ] Clear glass
	Metal / fittings
	Frameless 12 mm clear laminated glass in a recessed stainless channel with a slim capping rail, continuing the ground-floor stair detail without change. No vertical rods.
	12 mm
	Staircase Landing & Feature Wall — Balustrade

	ST-01 / MT-01 / LT-01
	[image: ] Beige marble
[image: ] Brushed brass
	Floor / paving
	20 mm beige marble treads with a 10 mm brushed brass nosing insert; concealed LED under each nosing on a separate low-level night circuit.
	20 mm · 10 mm
	Staircase Landing & Feature Wall — Treads & landing

	MT-01 / GL-01 / LT-01
	[image: ] Brushed brass
[image: ] Clear glass
	Special finish / equipment
	One cascading brass-and-glass rod chandelier in the void, set so the lowest element is visible from the ground-floor lobby and the mass sits at eye level on the landing.
	TBC by sample/shop drawing
	Staircase Landing & Feature Wall — Decorative lighting

	JN-01
	[image: ] Smoked walnut
	Special finish / equipment
	A recessed walnut niche with a lit sculpture, and a slim stone-topped console on the return wall.
	TBC by sample/shop drawing
	Staircase Landing & Feature Wall — Accents

	ST-01
	[image: ] Beige marble
	Staircase treads
	Solid beige marble treads & risers, honed, 3 anti-slip grooves to nosing. Supplier/Product Code to be selected.
	Tread 300 mm · riser 160–170 mm · 20–30 mm
	Staircase Landing & Feature Wall — all flights and landings

	GL-01
	[image: ] Clear glass
	Balustrade
	Clear frameless laminated toughened glass in recessed floor channel, no handrail rods. Supplier/Product Code to be selected.
	12+12 mm laminated · 1100 mm high
	Staircase Landing & Feature Wall — open side of flights and landing

	MT-01
	[image: ] Brushed brass
	Handrail
	Brushed brass (PVD or solid), satin lacquered slim wall-mounted handrail. Supplier/Product Code to be selected.
	Ø40 mm
	Staircase Landing & Feature Wall — wall side

	LT-01
	[image: ] 2700K LED
	Stair lighting
	Recessed 2700K LED step lights / under-tread LED strip. Supplier/Product Code to be selected.
	—
	Staircase Landing & Feature Wall — every 2nd step

	WF-01
	[image: ] Warm white paint
	Walls
	Gypsum skim plaster, smooth level-5 finish
	—
	Staircase Landing & Feature Wall — stairwell walls

	WF-01
	[image: ] Warm white paint
	Wall paint
	Wall paint: warm white / greige washable matt emulsion (Jotun Fenomastic or equal), 2 coats on primer. Supplier/Product Code to be selected.
	—
	Staircase Landing & Feature Wall — stairwell walls

	ST-02 / ST-03 / ST-01
	[image: ] Dark Emperador
[image: ] Travertine
	Feature wall
	Bookmatched Silver Travertine / Dark Emperador marble slab cladding. Supplier/Product Code to be selected.
	20 mm slabs, full-height bookmatch
	Staircase Landing & Feature Wall — double-height stair wall

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Gypsum board ceiling, warm white matt paint, perimeter shadow-gap with 2700K LED cove, trimless downlights; feature pendant to double-height void. Supplier/Product Code to be selected.
	—
	Staircase Landing & Feature Wall — soffit and void

	ST-01
	[image: ] Beige marble
	Skirting
	Stringer skirting in matching solid beige marble treads & risers
	100 mm
	Staircase Landing & Feature Wall — wall stringer


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 1 · HIGH-END MODERN LUXURY
Master Bedroom One — South-West Suite
Upper floor  ·  4.05 m × 5.40 m (4.10 m at the bed wall) · private ensuite 1.80 m × 2.90 m · PC window to the west
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	JN-01 / LT-01
	[image: ] Smoked walnut
[image: ] 2700K LED
	Special finish / equipment
	180×200 king centred on the long internal wall, 1.05 m clear to the wardrobe run, a 1.60 m upholstered bench at the foot. Two floating walnut bedside tables, 55 cm, with concealed sockets.
	200 k · 1.05 m · 1.60 m · 55 cm
	Master Bedroom One — South-West Suite — Bed & layout

	MT-01 / TX-01 / LT-01
	[image: ] Brushed brass
[image: ] Textiles
	Walls / paint
	Full-height headboard wall in cream bouclé panels with 15 mm brushed brass vertical reveals, flanked by two backlit alabaster-effect stone panels that act as the room's night light.
	15 mm
	Master Bedroom One — South-West Suite — Headboard / feature wall

	JN-01 / MT-01 / LT-01
	[image: ] Smoked walnut
[image: ] Brushed brass
	Joinery / woodwork
	3.40 m of full-height smoked walnut joinery: two fluted 4-door hinged banks with brass shadow-gap pulls, and a central open dressing niche with a drawer chest, mirror and warm LED wash.
	3.40 m
	Master Bedroom One — South-West Suite — Wardrobes & storage

	ST-01 / JN-01 / MT-01
	[image: ] Beige marble
[image: ] Smoked walnut
	Walls / paint
	65" screen recessed into a warm beige marble slab framed in brass, over a fluted walnut media console with a stone top.
	TBC by sample/shop drawing
	Master Bedroom One — South-West Suite — TV wall

	ST-01 / JN-01 / MT-01 / TX-01
	[image: ] Beige marble
[image: ] Smoked walnut
	Joinery / woodwork
	1.40 m bespoke walnut dressing table with a cream marble top, backlit round brass mirror and a bouclé swivel stool at the west window.
	1.40 m
	Master Bedroom One — South-West Suite — Vanity

	LT-01
	[image: ] 2700K LED
	Ceiling
	Stepped gypsum with a continuous 3000 K cove, trimless spots washing the joinery, a pair of alabaster pendants at the bedheads, and two-way dimming from the door and both bedsides.
	3000 K
	Master Bedroom One — South-West Suite — Ceiling & lighting

	JN-02 / TX-01
	[image: ] Natural oak / wood
[image: ] Textiles
	Floor / paving
	Warm oak herringbone, 90×450 mm, brushed and matt-lacquered. A 2.40×3.00 m hand-tufted greige wool rug under the lower two-thirds of the bed.
	450 mm · 3.00 m
	Master Bedroom One — South-West Suite — Flooring & rug

	TX-01
	[image: ] Textiles
	Doors / window treatment
	Recessed twin track: ivory linen sheer plus a taupe blackout drape in a heavyweight matt weave, wall-to-wall, ceiling-hung.
	TBC by sample/shop drawing
	Master Bedroom One — South-West Suite — Curtains

	ST-01 / JN-01 / JN-02 / MT-01 / TX-01
	[image: ] Beige marble
[image: ] Smoked walnut
	Special finish / equipment
	Cream bouclé · smoked walnut · beige marble · brushed brass · oak · greige wool.
	TBC by sample/shop drawing
	Master Bedroom One — South-West Suite — Materials

	JN-01 / JN-02 / LT-01
	[image: ] Smoked walnut
[image: ] Natural oak / wood
	Flooring
	Engineered smoked walnut / oak plank floor, matt oiled. Supplier/Product Code to be selected.
	190×1900 mm · 15 mm
	Master Bedroom One — South-West Suite — full floor area

	WF-01
	[image: ] Warm white paint
	Walls
	Gypsum skim plaster, smooth level-5 finish ready for paint
	Plaster 10–13 mm
	Master Bedroom One — South-West Suite — all walls except feature wall

	WF-01
	[image: ] Warm white paint
	Wall paint
	Wall paint: warm white / greige washable matt emulsion (Jotun Fenomastic or equal), 2 coats on primer. Supplier/Product Code to be selected.
	—
	Master Bedroom One — South-West Suite — all painted walls

	ST-02 / ST-03 / ST-01
	[image: ] Dark Emperador
[image: ] Travertine
	Feature wall
	Bookmatched Silver Travertine / Dark Emperador marble slab cladding. Supplier/Product Code to be selected.
	20 mm slabs, full-height bookmatch
	Master Bedroom One — South-West Suite — upholstered / timber-panelled headboard wall

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Gypsum board ceiling, warm white matt paint, perimeter shadow-gap with 2700K LED cove, trimless downlights. Supplier/Product Code to be selected.
	12.5 mm board · 2.9–3.0 m FFL
	Master Bedroom One — South-West Suite — full ceiling

	WF-01 / MT-01
	[image: ] Warm white paint
[image: ] Brushed brass
	Skirting
	Recessed shadow-gap skirting, brushed brass (pvd or solid), satin lacquered trim / flush painted MDF
	80 mm high · 10 mm reveal
	Master Bedroom One — South-West Suite — all wall perimeters

	JN-01
	[image: ] Smoked walnut
	Joinery
	Smoked walnut veneer on MR-MDF, matt lacquer 10% sheen. Supplier/Product Code to be selected.
	18–22 mm core · 0.6 mm veneer
	Master Bedroom One — South-West Suite — built-in units and wall panelling

	JN-01 / LT-01
	[image: ] Smoked walnut
[image: ] 2700K LED
	Doors
	Full-height flush door, smoked walnut veneer, concealed frame and hinges, magnetic lock. Supplier/Product Code to be selected.
	900×2700 mm · 50 mm leaf
	Master Bedroom One — South-West Suite — entry door(s)

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Metal finishes
	Brushed brass (PVD or solid), satin lacquered — door handles, inlays, light fittings, joinery pulls. Supplier/Product Code to be selected.
	—
	Master Bedroom One — South-West Suite — all visible metalwork

	JN-01 / LT-01
	[image: ] Smoked walnut
[image: ] 2700K LED
	Wardrobes
	Built-in full-height wardrobes, smoked walnut veneer on mr-mdf, matt lacquer 10% sheen, internal LED, soft-close. Supplier/Product Code to be selected.
	600 mm deep · floor to ceiling
	Master Bedroom One — South-West Suite — wardrobe wall


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 1 · HIGH-END MODERN LUXURY
Master One — Dressing Room
Upper floor  ·  2.60 m × 1.95 m · between the bedroom and the ensuite, on the drawn opening
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	JN-01
	[image: ] Smoked walnut
	Joinery / woodwork
	Full-height smoked walnut units on both long walls: hanging at 1.05 m and 1.90 m, adjustable shelving, and four soft-close drawer banks with leather-lined jewellery trays.
	1.05 m · 1.90 m
	Master One — Dressing Room — Wardrobes

	MT-01 / GL-01
	[image: ] Brushed brass
[image: ] Clear glass
	Special finish / equipment
	Two central bays in fluted reeded glass with brushed brass frames for bags and shoes, each shelf lit from within.
	TBC by sample/shop drawing
	Master One — Dressing Room — Display sections

	LT-01
	[image: ] 2700K LED
	Special finish / equipment
	3000 K LED profile behind every hanging rail and under every shelf, on PIR sensors so the units light as the doors open.
	3000 K
	Master One — Dressing Room — Internal lighting

	ST-01 / JN-01 / MT-01 / TX-01
	[image: ] Beige marble
[image: ] Smoked walnut
	Joinery / woodwork
	1.20 m walnut dressing vanity with a cream marble top, backlit brass mirror and an upholstered bouclé stool at the end of the run.
	1.20 m
	Master One — Dressing Room — Vanity

	ST-01 / WF-01 / MT-01 / TX-01 / LT-01
	[image: ] Beige marble
[image: ] Warm white paint
	Walls / paint
	Beige marble floor with an inset greige wool rug, micro-cement ceiling with a slim perimeter cove, brass shadow-gap pulls throughout.
	TBC by sample/shop drawing
	Master One — Dressing Room — Finishes

	ST-01
	[image: ] Beige marble
	Flooring
	Natural beige marble (Crema Marfil / Botticino type, warm cream), honed-polished satin, bookmatched in principal rooms. Supplier/Product Code to be selected.
	1200×600 mm slabs · 20 mm thick
	Master One — Dressing Room — full floor area

	WF-01
	[image: ] Warm white paint
	Walls
	Gypsum skim plaster, smooth level-5 finish ready for paint
	Plaster 10–13 mm
	Master One — Dressing Room — all walls except feature wall

	WF-01
	[image: ] Warm white paint
	Wall paint
	Wall paint: warm white / greige washable matt emulsion (Jotun Fenomastic or equal), 2 coats on primer. Supplier/Product Code to be selected.
	—
	Master One — Dressing Room — all painted walls

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Gypsum board ceiling, warm white matt paint, perimeter shadow-gap with 2700K LED cove, trimless downlights. Supplier/Product Code to be selected.
	12.5 mm board · 2.9–3.0 m FFL
	Master One — Dressing Room — full ceiling

	WF-01 / MT-01
	[image: ] Warm white paint
[image: ] Brushed brass
	Skirting
	Recessed shadow-gap skirting, brushed brass (pvd or solid), satin lacquered trim / flush painted MDF
	80 mm high · 10 mm reveal
	Master One — Dressing Room — all wall perimeters

	JN-01 / LT-01
	[image: ] Smoked walnut
[image: ] 2700K LED
	Doors
	Full-height flush door, smoked walnut veneer, concealed frame and hinges, magnetic lock. Supplier/Product Code to be selected.
	900×2700 mm · 50 mm leaf
	Master One — Dressing Room — entry door(s)

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Metal finishes
	Brushed brass (PVD or solid), satin lacquered — door handles, inlays, light fittings, joinery pulls. Supplier/Product Code to be selected.
	—
	Master One — Dressing Room — all visible metalwork

	JN-01 / MT-01 / GL-01 / LT-01
	[image: ] Smoked walnut
[image: ] Brushed brass
	Wardrobes
	Full-height wardrobes, smoked walnut veneer on mr-mdf, matt lacquer 10% sheen fronts; bronze-tint glass display doors, integrated LED, leather-look internal drawers. Supplier/Product Code to be selected.
	600 mm deep · floor to ceiling
	Master One — Dressing Room — all wardrobe walls

	ST-01
	[image: ] Beige marble
	Joinery
	Dressing island / vanity with beige marble (matching floor family), honed, eased 2 mm edge top and full-length mirror. Supplier/Product Code to be selected.
	20 mm top
	Master One — Dressing Room — centre / vanity wall


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 1 · HIGH-END MODERN LUXURY
Master Ensuite One
Upper floor  ·  1.80 m × 2.90 m · WC, vanity and walk-in shower, on the drawn wet wall
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	ST-01
	[image: ] Beige marble
	Walls / paint
	Book-matched warm beige marble to full height on all wet walls and floor, 20 mm slab vanity top with an integrated basin.
	20 mm
	Master Ensuite One — Stone

	JN-01 / MT-01 / LT-01
	[image: ] Smoked walnut
[image: ] Brushed brass
	Joinery / woodwork
	Wall-hung smoked walnut vanity, 1.20 m, push-open with a concealed brass finger pull.
	1.20 m
	Master Ensuite One — Joinery

	ST-01 / MT-01 / GL-01
	[image: ] Beige marble
[image: ] Brushed brass
	Special finish / equipment
	Walk-in with a single 10 mm clear glass panel on a brass channel, marble bench, brass rain head and hand shower, linear drain.
	10 mm
	Master Ensuite One — Shower

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Metal / fittings
	Brushed brass PVD throughout · wall-hung WC with concealed cistern and a brass plate.
	TBC by sample/shop drawing
	Master Ensuite One — Fittings

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Special finish / equipment
	Backlit brass-framed mirror, IP-rated warm spots over the shower, a lit niche, and a 5% floor-level night circuit.
	5%
	Master Ensuite One — Lighting

	ST-01
	[image: ] Beige marble
	Bathroom floor
	Beige marble, honed anti-slip (R10) finish. Supplier/Product Code to be selected.
	600×600 mm · laid to falls
	Master Ensuite One — full floor

	ST-01
	[image: ] Beige marble
	Bathroom walls
	Beige marble full-height cladding, honed. Supplier/Product Code to be selected.
	1200×600 mm · 15–20 mm
	Master Ensuite One — full-height wet walls

	WF-01
	[image: ] Warm white paint
	Wall paint
	Moisture- and mould-resistant matt emulsion, warm white, 2 coats on primer. Supplier/Product Code to be selected.
	—
	Master Ensuite One — non-tiled wall areas

	ST-02 / ST-03 / ST-01
	[image: ] Dark Emperador
[image: ] Travertine
	Feature wall
	Bookmatched Silver Travertine / Dark Emperador marble slab cladding behind vanity with backlit mirror. Supplier/Product Code to be selected.
	20 mm slabs, full-height bookmatch
	Master Ensuite One — vanity wall

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Moisture-resistant (MR) gypsum ceiling, anti-mould warm white matt paint, IP44 trimless downlights. Supplier/Product Code to be selected.
	12.5 mm MR board
	Master Ensuite One — full ceiling

	JN-01 / LT-01
	[image: ] Smoked walnut
[image: ] 2700K LED
	Vanity
	Wall-hung vanity, smoked walnut veneer on mr-mdf, matt lacquer 10% sheen, soft-close drawers, LED under-glow. Supplier/Product Code to be selected.
	550 mm deep
	Master Ensuite One — vanity wall

	ST-01 / GL-01 / LT-01
	[image: ] Beige marble
[image: ] Clear glass
	Shower area
	Beige marble walls, fluted marble niche, 10 mm low-iron frameless glass screen; linear drain with tile insert; concealed thermostatic mixer & ceiling rain head. Supplier/Product Code to be selected.
	Screen 10 mm · drain 800 mm
	Master Ensuite One — walk-in shower

	ST-01
	[image: ] Beige marble
	Countertop
	Beige marble top with integrated moulded basin, honed. Supplier/Product Code to be selected.
	20 mm
	Master Ensuite One — vanity

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Sanitaryware
	Wall-hung rimless WC with concealed cistern, white gloss; brushed brass (pvd or solid), satin lacquered flush plate & mixers. Supplier/Product Code to be selected.
	—
	Master Ensuite One — WC and basin

	MT-01
	[image: ] Brushed brass
	Metal finishes
	Brushed brass (PVD or solid), satin lacquered — taps, shower set, towel rail, accessories. Supplier/Product Code to be selected.
	—
	Master Ensuite One — all fittings

	JN-01 / LT-01
	[image: ] Smoked walnut
[image: ] 2700K LED
	Doors
	Full-height flush door, smoked walnut veneer, concealed frame and hinges, magnetic lock, moisture-resistant core. Supplier/Product Code to be selected.
	800×2700 mm
	Master Ensuite One — entry door


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 1 · HIGH-END MODERN LUXURY
Master Bedroom Two — South-East Suite
Upper floor  ·  6.95 m × 5.00 m (5.50 m to the terrace line) · ensuite 1.85 m × 3.05 m · direct access to the 4.90 m × 1.20 m terrace
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	TX-01
	[image: ] Textiles
	Special finish / equipment
	200×200 super king on the north wall, 1.20 m clear both sides, a 1.80 m bouclé bench at the foot. The window bay to the terrace is kept free for the lounge pair so the door swing and sliding track stay unobstructed.
	1.20 m · 1.80 m
	Master Bedroom Two — South-East Suite — Bed & layout

	ST-01 / MT-01 / TX-01 / LT-01
	[image: ] Beige marble
[image: ] Brushed brass
	Walls / paint
	Book-matched warm beige marble, full height, with a low taupe velvet headboard and a continuous brushed brass ledge at 900 mm carrying concealed LED that grazes the stone upward.
	900 mm
	Master Bedroom Two — South-East Suite — Headboard / feature wall

	JN-01 / MT-01 / LT-01
	[image: ] Smoked walnut
[image: ] Brushed brass
	Joinery / woodwork
	4.20 m of full-height fluted walnut wardrobe with brass reveals, including a mirrored dressing bay with internal LED, jewellery drawers and a pull-out valet rail.
	4.20 m
	Master Bedroom Two — South-East Suite — Wardrobes & dressing

	JN-02 / LT-01
	[image: ] Natural oak / wood
[image: ] 2700K LED
	Walls / paint
	75" screen set into a slatted oak feature wall with warm backlighting behind the slats, over a floating oak console.
	TBC by sample/shop drawing
	Master Bedroom Two — South-East Suite — TV wall

	ST-03 / MT-01 / TX-01
	[image: ] Travertine
[image: ] Brushed brass
	Special finish / equipment
	Two curved cream bouclé armchairs with a round travertine table in the bay, and a taupe velvet chaise with a brass reading lamp at the terrace threshold.
	TBC by sample/shop drawing
	Master Bedroom Two — South-East Suite — Lounge & chaise

	MT-01 / GL-01 / LT-01
	[image: ] Brushed brass
[image: ] Clear glass
	Ceiling
	Deep coffer with a brass reveal and 3000 K cove, trimless spots, a brass-and-glass chandelier centred on the bed, and a separate terrace-view scene that drops the interior to 15% so the outside reads.
	3000 K · 15%
	Master Bedroom Two — South-East Suite — Ceiling & lighting

	JN-02 / TX-01
	[image: ] Natural oak / wood
[image: ] Textiles
	Floor / paving
	Wide-plank warm oak, 220 mm, with a 3.00×4.00 m silk-wool rug in greige under the bed and bench.
	220 mm · 4.00 m
	Master Bedroom Two — South-East Suite — Flooring & rug

	TX-01
	[image: ] Textiles
	Doors / window treatment
	Motorised ceiling-recessed twin track across the full terrace elevation: ivory sheer plus heavy taupe blackout, both wall-to-wall.
	TBC by sample/shop drawing
	Master Bedroom Two — South-East Suite — Curtains

	ST-03 / ST-01 / JN-01 / JN-02 / MT-01 / TX-01
	[image: ] Travertine
[image: ] Beige marble
	Special finish / equipment
	Book-matched beige marble · taupe velvet · smoked walnut · oak · travertine · brushed brass.
	TBC by sample/shop drawing
	Master Bedroom Two — South-East Suite — Materials

	JN-01 / JN-02 / LT-01
	[image: ] Smoked walnut
[image: ] Natural oak / wood
	Flooring
	Engineered smoked walnut / oak plank floor, matt oiled. Supplier/Product Code to be selected.
	190×1900 mm · 15 mm
	Master Bedroom Two — South-East Suite — full floor area

	WF-01
	[image: ] Warm white paint
	Walls
	Gypsum skim plaster, smooth level-5 finish ready for paint
	Plaster 10–13 mm
	Master Bedroom Two — South-East Suite — all walls except feature wall

	WF-01
	[image: ] Warm white paint
	Wall paint
	Wall paint: warm white / greige washable matt emulsion (Jotun Fenomastic or equal), 2 coats on primer. Supplier/Product Code to be selected.
	—
	Master Bedroom Two — South-East Suite — all painted walls

	ST-02 / ST-03 / ST-01
	[image: ] Dark Emperador
[image: ] Travertine
	Feature wall
	Bookmatched Silver Travertine / Dark Emperador marble slab cladding. Supplier/Product Code to be selected.
	20 mm slabs, full-height bookmatch
	Master Bedroom Two — South-East Suite — upholstered / timber-panelled headboard wall

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Gypsum board ceiling, warm white matt paint, perimeter shadow-gap with 2700K LED cove, trimless downlights. Supplier/Product Code to be selected.
	12.5 mm board · 2.9–3.0 m FFL
	Master Bedroom Two — South-East Suite — full ceiling

	WF-01 / MT-01
	[image: ] Warm white paint
[image: ] Brushed brass
	Skirting
	Recessed shadow-gap skirting, brushed brass (pvd or solid), satin lacquered trim / flush painted MDF
	80 mm high · 10 mm reveal
	Master Bedroom Two — South-East Suite — all wall perimeters

	JN-01
	[image: ] Smoked walnut
	Joinery
	Smoked walnut veneer on MR-MDF, matt lacquer 10% sheen. Supplier/Product Code to be selected.
	18–22 mm core · 0.6 mm veneer
	Master Bedroom Two — South-East Suite — built-in units and wall panelling

	JN-01 / LT-01
	[image: ] Smoked walnut
[image: ] 2700K LED
	Doors
	Full-height flush door, smoked walnut veneer, concealed frame and hinges, magnetic lock. Supplier/Product Code to be selected.
	900×2700 mm · 50 mm leaf
	Master Bedroom Two — South-East Suite — entry door(s)

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Metal finishes
	Brushed brass (PVD or solid), satin lacquered — door handles, inlays, light fittings, joinery pulls. Supplier/Product Code to be selected.
	—
	Master Bedroom Two — South-East Suite — all visible metalwork

	JN-01 / LT-01
	[image: ] Smoked walnut
[image: ] 2700K LED
	Wardrobes
	Built-in full-height wardrobes, smoked walnut veneer on mr-mdf, matt lacquer 10% sheen, internal LED, soft-close. Supplier/Product Code to be selected.
	600 mm deep · floor to ceiling
	Master Bedroom Two — South-East Suite — wardrobe wall


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 1 · HIGH-END MODERN LUXURY
Master Two — Dressing Room
Upper floor  ·  3.10 m × 2.20 m · U-shaped fit-out linking bedroom and ensuite
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	SP-01
	[image: ] Dark bronze / special
	Special finish / equipment
	U-shaped full-height joinery on three walls with a 1.60 m × 0.80 m island, 1.00 m clear on all sides.
	1.60 m × 0.80 m · 1.00 m
	Master Two — Dressing Room — Layout

	JN-01
	[image: ] Smoked walnut
	Joinery / woodwork
	Smoked walnut carcasses with fluted and plain door mixes, double hanging, long hanging, shoe racks and a dedicated luggage bay above.
	TBC by sample/shop drawing
	Master Two — Dressing Room — Wardrobes

	ST-03 / GL-01 / TX-01
	[image: ] Travertine
[image: ] Clear glass
	Countertops / stone
	Travertine top with 20 mm mitred edge over six velvet-lined drawers, plus a shallow glass-topped display drawer for watches and jewellery.
	20 mm
	Master Two — Dressing Room — Island

	GL-01 / LT-01
	[image: ] Clear glass
[image: ] 2700K LED
	Special finish / equipment
	Backlit reeded glass display bays, LED under every shelf and rail, and two small alabaster pendants over the island, all 3000 K and dimmed.
	3000 K
	Master Two — Dressing Room — Display & lighting

	ST-03 / JN-01 / MT-01 / TX-01
	[image: ] Travertine
[image: ] Smoked walnut
	Joinery / woodwork
	1.40 m seated vanity in walnut with a travertine top, backlit rounded brass mirror and a cream bouclé stool.
	1.40 m
	Master Two — Dressing Room — Vanity

	ST-01
	[image: ] Beige marble
	Flooring
	Natural beige marble (Crema Marfil / Botticino type, warm cream), honed-polished satin, bookmatched in principal rooms. Supplier/Product Code to be selected.
	1200×600 mm slabs · 20 mm thick
	Master Two — Dressing Room — full floor area

	WF-01
	[image: ] Warm white paint
	Walls
	Gypsum skim plaster, smooth level-5 finish ready for paint
	Plaster 10–13 mm
	Master Two — Dressing Room — all walls except feature wall

	WF-01
	[image: ] Warm white paint
	Wall paint
	Wall paint: warm white / greige washable matt emulsion (Jotun Fenomastic or equal), 2 coats on primer. Supplier/Product Code to be selected.
	—
	Master Two — Dressing Room — all painted walls

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Gypsum board ceiling, warm white matt paint, perimeter shadow-gap with 2700K LED cove, trimless downlights. Supplier/Product Code to be selected.
	12.5 mm board · 2.9–3.0 m FFL
	Master Two — Dressing Room — full ceiling

	WF-01 / MT-01
	[image: ] Warm white paint
[image: ] Brushed brass
	Skirting
	Recessed shadow-gap skirting, brushed brass (pvd or solid), satin lacquered trim / flush painted MDF
	80 mm high · 10 mm reveal
	Master Two — Dressing Room — all wall perimeters

	JN-01 / LT-01
	[image: ] Smoked walnut
[image: ] 2700K LED
	Doors
	Full-height flush door, smoked walnut veneer, concealed frame and hinges, magnetic lock. Supplier/Product Code to be selected.
	900×2700 mm · 50 mm leaf
	Master Two — Dressing Room — entry door(s)

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Metal finishes
	Brushed brass (PVD or solid), satin lacquered — door handles, inlays, light fittings, joinery pulls. Supplier/Product Code to be selected.
	—
	Master Two — Dressing Room — all visible metalwork

	JN-01 / MT-01 / GL-01 / LT-01
	[image: ] Smoked walnut
[image: ] Brushed brass
	Wardrobes
	Full-height wardrobes, smoked walnut veneer on mr-mdf, matt lacquer 10% sheen fronts; bronze-tint glass display doors, integrated LED, leather-look internal drawers. Supplier/Product Code to be selected.
	600 mm deep · floor to ceiling
	Master Two — Dressing Room — all wardrobe walls

	ST-01
	[image: ] Beige marble
	Joinery
	Dressing island / vanity with beige marble (matching floor family), honed, eased 2 mm edge top and full-length mirror. Supplier/Product Code to be selected.
	20 mm top
	Master Two — Dressing Room — centre / vanity wall


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 1 · HIGH-END MODERN LUXURY
Master Ensuite Two
Upper floor  ·  1.85 m × 3.05 m · twin basins, WC and shower
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	ST-02 / ST-03 / ST-01
	[image: ] Dark Emperador
[image: ] Travertine
	Walls / paint
	Warm travertine to full height with a 900 mm dark emperador marble band at splashback level; travertine floor with a matching solid stone vanity.
	900 mm
	Master Ensuite Two — Stone

	ST-03 / LT-01
	[image: ] Travertine
[image: ] 2700K LED
	Joinery / woodwork
	2.10 m floating solid travertine vanity with twin integrated basins and an open lower shelf for rolled towels.
	2.10 m
	Master Ensuite Two — Vanity

	MT-01 / GL-01
	[image: ] Brushed brass
[image: ] Clear glass
	Special finish / equipment
	Enclosure in fluted glass with a brushed champagne brass frame, stone bench, rain head plus hand shower.
	TBC by sample/shop drawing
	Master Ensuite Two — Shower

	LT-01
	[image: ] 2700K LED
	Special finish / equipment
	Two backlit rounded mirrors, a warm cove in the ceiling recess, and a discreet dimmed circuit for night use.
	TBC by sample/shop drawing
	Master Ensuite Two — Lighting

	MT-01 / TX-01 / LS-01
	[image: ] Brushed brass
[image: ] Textiles
	Special finish / equipment
	A round stone stool, brass towel bars, folded linen towels and a single planted vessel.
	TBC by sample/shop drawing
	Master Ensuite Two — Accessories

	ST-01
	[image: ] Beige marble
	Bathroom floor
	Beige marble, honed anti-slip (R10) finish. Supplier/Product Code to be selected.
	600×600 mm · laid to falls
	Master Ensuite Two — full floor

	ST-01
	[image: ] Beige marble
	Bathroom walls
	Beige marble full-height cladding, honed. Supplier/Product Code to be selected.
	1200×600 mm · 15–20 mm
	Master Ensuite Two — full-height wet walls

	WF-01
	[image: ] Warm white paint
	Wall paint
	Moisture- and mould-resistant matt emulsion, warm white, 2 coats on primer. Supplier/Product Code to be selected.
	—
	Master Ensuite Two — non-tiled wall areas

	ST-02 / ST-03 / ST-01
	[image: ] Dark Emperador
[image: ] Travertine
	Feature wall
	Bookmatched Silver Travertine / Dark Emperador marble slab cladding behind vanity with backlit mirror. Supplier/Product Code to be selected.
	20 mm slabs, full-height bookmatch
	Master Ensuite Two — vanity wall

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Moisture-resistant (MR) gypsum ceiling, anti-mould warm white matt paint, IP44 trimless downlights. Supplier/Product Code to be selected.
	12.5 mm MR board
	Master Ensuite Two — full ceiling

	JN-01 / LT-01
	[image: ] Smoked walnut
[image: ] 2700K LED
	Vanity
	Wall-hung vanity, smoked walnut veneer on mr-mdf, matt lacquer 10% sheen, soft-close drawers, LED under-glow. Supplier/Product Code to be selected.
	550 mm deep
	Master Ensuite Two — vanity wall

	ST-01 / GL-01 / LT-01
	[image: ] Beige marble
[image: ] Clear glass
	Shower area
	Beige marble walls, fluted marble niche, 10 mm low-iron frameless glass screen; linear drain with tile insert; concealed thermostatic mixer & ceiling rain head. Supplier/Product Code to be selected.
	Screen 10 mm · drain 800 mm
	Master Ensuite Two — walk-in shower

	ST-01
	[image: ] Beige marble
	Countertop
	Beige marble top with integrated moulded basin, honed. Supplier/Product Code to be selected.
	20 mm
	Master Ensuite Two — vanity

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Sanitaryware
	Wall-hung rimless WC with concealed cistern, white gloss; brushed brass (pvd or solid), satin lacquered flush plate & mixers. Supplier/Product Code to be selected.
	—
	Master Ensuite Two — WC and basin

	MT-01
	[image: ] Brushed brass
	Metal finishes
	Brushed brass (PVD or solid), satin lacquered — taps, shower set, towel rail, accessories. Supplier/Product Code to be selected.
	—
	Master Ensuite Two — all fittings

	JN-01 / LT-01
	[image: ] Smoked walnut
[image: ] 2700K LED
	Doors
	Full-height flush door, smoked walnut veneer, concealed frame and hinges, magnetic lock, moisture-resistant core. Supplier/Product Code to be selected.
	800×2700 mm
	Master Ensuite Two — entry door


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 1 · HIGH-END MODERN LUXURY
Bedroom Three — North-West Twin
Upper floor  ·  4.30 m × 4.30 m · 3.50 m opening line · direct access to the 4.85 m terrace
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	SP-01
	[image: ] Dark bronze / special
	Special finish / equipment
	Two 100×200 singles with 700 mm between them, both on one continuous headboard panel. Beds sit on the internal wall so the terrace door and the window wall stay clear.
	700 mm
	Bedroom Three — North-West Twin — Bed & layout

	JN-02 / WF-01 / TX-01 / LT-01
	[image: ] Natural oak / wood
[image: ] Warm white paint
	Walls / paint
	A 3.20 m shared headboard in soft greige linen, 1.10 m high, divided by slim oak battens, with a concealed LED wash above it against the painted panelling.
	3.20 m · 1.10 m
	Bedroom Three — North-West Twin — Headboard / feature wall

	JN-02 / MT-01 / LT-01
	[image: ] Natural oak / wood
[image: ] Brushed brass
	Joinery / woodwork
	2.80 m of full-height light oak wardrobe, handleless with thin brass reveals, plus a 1.20 m integrated oak desk with a lit shelf stack and a cream leather chair.
	2.80 m · 1.20 m
	Bedroom Three — North-West Twin — Wardrobes & study

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Walls / paint
	55" screen on a cream micro-cement panel above the desk run, cabling fully concealed.
	TBC by sample/shop drawing
	Bedroom Three — North-West Twin — TV wall

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Ceiling
	Simple recessed tray with a 3000 K cove, spots on the wardrobe faces, one slim linear brass pendant between the beds and individual reading lights at each bedhead.
	3000 K
	Bedroom Three — North-West Twin — Ceiling & lighting

	JN-02 / TX-01
	[image: ] Natural oak / wood
[image: ] Textiles
	Floor / paving
	Warm oak plank flooring with a soft ivory low-pile rug across the bed zone.
	TBC by sample/shop drawing
	Bedroom Three — North-West Twin — Flooring & rug

	TX-01
	[image: ] Textiles
	Doors / window treatment
	Ivory sheer with a greige blackout drape on a recessed track, sized to clear the terrace door leaf completely when stacked.
	TBC by sample/shop drawing
	Bedroom Three — North-West Twin — Curtains

	JN-02 / WF-01 / MT-01 / TX-01 / LT-01
	[image: ] Natural oak / wood
[image: ] Warm white paint
	Special finish / equipment
	Light oak · greige linen · cream paint · micro-cement · brushed brass · ivory wool.
	TBC by sample/shop drawing
	Bedroom Three — North-West Twin — Materials

	JN-01 / JN-02 / LT-01
	[image: ] Smoked walnut
[image: ] Natural oak / wood
	Flooring
	Engineered smoked walnut / oak plank floor, matt oiled. Supplier/Product Code to be selected.
	190×1900 mm · 15 mm
	Bedroom Three — North-West Twin — full floor area

	WF-01
	[image: ] Warm white paint
	Walls
	Gypsum skim plaster, smooth level-5 finish ready for paint
	Plaster 10–13 mm
	Bedroom Three — North-West Twin — all walls except feature wall

	WF-01
	[image: ] Warm white paint
	Wall paint
	Wall paint: warm white / greige washable matt emulsion (Jotun Fenomastic or equal), 2 coats on primer. Supplier/Product Code to be selected.
	—
	Bedroom Three — North-West Twin — all painted walls

	ST-02 / ST-03 / ST-01
	[image: ] Dark Emperador
[image: ] Travertine
	Feature wall
	Bookmatched Silver Travertine / Dark Emperador marble slab cladding. Supplier/Product Code to be selected.
	20 mm slabs, full-height bookmatch
	Bedroom Three — North-West Twin — upholstered / timber-panelled headboard wall

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Gypsum board ceiling, warm white matt paint, perimeter shadow-gap with 2700K LED cove, trimless downlights. Supplier/Product Code to be selected.
	12.5 mm board · 2.9–3.0 m FFL
	Bedroom Three — North-West Twin — full ceiling

	WF-01 / MT-01
	[image: ] Warm white paint
[image: ] Brushed brass
	Skirting
	Recessed shadow-gap skirting, brushed brass (pvd or solid), satin lacquered trim / flush painted MDF
	80 mm high · 10 mm reveal
	Bedroom Three — North-West Twin — all wall perimeters

	JN-01
	[image: ] Smoked walnut
	Joinery
	Smoked walnut veneer on MR-MDF, matt lacquer 10% sheen. Supplier/Product Code to be selected.
	18–22 mm core · 0.6 mm veneer
	Bedroom Three — North-West Twin — built-in units and wall panelling

	JN-01 / LT-01
	[image: ] Smoked walnut
[image: ] 2700K LED
	Doors
	Full-height flush door, smoked walnut veneer, concealed frame and hinges, magnetic lock. Supplier/Product Code to be selected.
	900×2700 mm · 50 mm leaf
	Bedroom Three — North-West Twin — entry door(s)

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Metal finishes
	Brushed brass (PVD or solid), satin lacquered — door handles, inlays, light fittings, joinery pulls. Supplier/Product Code to be selected.
	—
	Bedroom Three — North-West Twin — all visible metalwork

	JN-01 / LT-01
	[image: ] Smoked walnut
[image: ] 2700K LED
	Wardrobes
	Built-in full-height wardrobes, smoked walnut veneer on mr-mdf, matt lacquer 10% sheen, internal LED, soft-close. Supplier/Product Code to be selected.
	600 mm deep · floor to ceiling
	Bedroom Three — North-West Twin — wardrobe wall


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 1 · HIGH-END MODERN LUXURY
Bedroom Four — North-East Guest Room
Upper floor  ·  4.95 m × 5.00 m (5.10 m structural bay) · window wall to the north-east
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	JN-01
	[image: ] Smoked walnut
	Special finish / equipment
	Two 105×200 singles, convertible to one 210 king by joining the bases — a practical guest arrangement. Shared walnut nightstand between, 800 mm clear to the wardrobe faces.
	210 k · 800 mm
	Bedroom Four — North-East Guest Room — Bed & layout

	WF-01 / TX-01
	[image: ] Warm white paint
[image: ] Textiles
	Walls / paint
	Individual 1.60 m tall channel-tufted headboards in warm sand velvet, set against full-height fluted cream plaster panels with a painted cap rail.
	1.60 m
	Bedroom Four — North-East Guest Room — Headboard / feature wall

	JN-01 / MT-01 / LT-01
	[image: ] Smoked walnut
[image: ] Brushed brass
	Joinery / woodwork
	3.60 m of full-height fluted walnut wardrobe with brass shadow-gap pulls, internal LED, and a dedicated luggage bay for guest use.
	3.60 m
	Bedroom Four — North-East Guest Room — Wardrobes & storage

	ST-03 / MT-01
	[image: ] Travertine
[image: ] Brushed brass
	Joinery / woodwork
	1.20 m travertine-topped console at the window with a backlit rounded brass mirror and an upholstered stool, doubling as a desk.
	1.20 m
	Bedroom Four — North-East Guest Room — Vanity / console

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Ceiling
	Tray ceiling with 3000 K cove, a compact brass drum chandelier centred, brass swing-arm sconces at each bedhead on individual switching, and a low-level night light to the ensuite door.
	3000 K
	Bedroom Four — North-East Guest Room — Ceiling & lighting

	JN-02 / TX-01
	[image: ] Natural oak / wood
[image: ] Textiles
	Floor / paving
	Warm oak plank with a textured camel wool rug running under both beds.
	TBC by sample/shop drawing
	Bedroom Four — North-East Guest Room — Flooring & rug

	TX-01 / LT-01
	[image: ] Textiles
[image: ] 2700K LED
	Doors / window treatment
	Ivory sheer with a sand-coloured blackout drape, pinch-pleat on a concealed track, full wall width.
	TBC by sample/shop drawing
	Bedroom Four — North-East Guest Room — Curtains

	ST-03 / JN-01 / WF-01 / MT-01 / TX-01
	[image: ] Travertine
[image: ] Smoked walnut
	Special finish / equipment
	Sand velvet · fluted cream plaster · walnut · travertine · brushed brass · camel wool.
	TBC by sample/shop drawing
	Bedroom Four — North-East Guest Room — Materials

	JN-01 / JN-02 / LT-01
	[image: ] Smoked walnut
[image: ] Natural oak / wood
	Flooring
	Engineered smoked walnut / oak plank floor, matt oiled. Supplier/Product Code to be selected.
	190×1900 mm · 15 mm
	Bedroom Four — North-East Guest Room — full floor area

	WF-01
	[image: ] Warm white paint
	Walls
	Gypsum skim plaster, smooth level-5 finish ready for paint
	Plaster 10–13 mm
	Bedroom Four — North-East Guest Room — all walls except feature wall

	WF-01
	[image: ] Warm white paint
	Wall paint
	Wall paint: warm white / greige washable matt emulsion (Jotun Fenomastic or equal), 2 coats on primer. Supplier/Product Code to be selected.
	—
	Bedroom Four — North-East Guest Room — all painted walls

	ST-02 / ST-03 / ST-01
	[image: ] Dark Emperador
[image: ] Travertine
	Feature wall
	Bookmatched Silver Travertine / Dark Emperador marble slab cladding. Supplier/Product Code to be selected.
	20 mm slabs, full-height bookmatch
	Bedroom Four — North-East Guest Room — upholstered / timber-panelled headboard wall

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Gypsum board ceiling, warm white matt paint, perimeter shadow-gap with 2700K LED cove, trimless downlights. Supplier/Product Code to be selected.
	12.5 mm board · 2.9–3.0 m FFL
	Bedroom Four — North-East Guest Room — full ceiling

	WF-01 / MT-01
	[image: ] Warm white paint
[image: ] Brushed brass
	Skirting
	Recessed shadow-gap skirting, brushed brass (pvd or solid), satin lacquered trim / flush painted MDF
	80 mm high · 10 mm reveal
	Bedroom Four — North-East Guest Room — all wall perimeters

	JN-01
	[image: ] Smoked walnut
	Joinery
	Smoked walnut veneer on MR-MDF, matt lacquer 10% sheen. Supplier/Product Code to be selected.
	18–22 mm core · 0.6 mm veneer
	Bedroom Four — North-East Guest Room — built-in units and wall panelling

	JN-01 / LT-01
	[image: ] Smoked walnut
[image: ] 2700K LED
	Doors
	Full-height flush door, smoked walnut veneer, concealed frame and hinges, magnetic lock. Supplier/Product Code to be selected.
	900×2700 mm · 50 mm leaf
	Bedroom Four — North-East Guest Room — entry door(s)

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Metal finishes
	Brushed brass (PVD or solid), satin lacquered — door handles, inlays, light fittings, joinery pulls. Supplier/Product Code to be selected.
	—
	Bedroom Four — North-East Guest Room — all visible metalwork

	JN-01 / LT-01
	[image: ] Smoked walnut
[image: ] 2700K LED
	Wardrobes
	Built-in full-height wardrobes, smoked walnut veneer on mr-mdf, matt lacquer 10% sheen, internal LED, soft-close. Supplier/Product Code to be selected.
	600 mm deep · floor to ceiling
	Bedroom Four — North-East Guest Room — wardrobe wall


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 1 · HIGH-END MODERN LUXURY
Shared Bathroom & WCs
Upper floor  ·  Two WCs at 1.80 m × 2.80 m serving the north bedrooms, exactly as drawn
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	ST-03
	[image: ] Travertine
	Walls / paint
	Cream travertine large-format wall and floor tiles, honed, with a stone-clad WC duct.
	TBC by sample/shop drawing
	Shared Bathroom & WCs — Stone

	JN-02
	[image: ] Natural oak / wood
	Joinery / woodwork
	Wall-hung stone vanity with an integrated basin and an open oak shelf below for towels and a basket.
	TBC by sample/shop drawing
	Shared Bathroom & WCs — Vanity

	MT-01 / GL-01
	[image: ] Brushed brass
[image: ] Clear glass
	Special finish / equipment
	Walk-in with a fixed glass panel, brass rain head and hand shower, lit niche, linear drain.
	TBC by sample/shop drawing
	Shared Bathroom & WCs — Shower

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Metal / fittings
	Brushed brass tapware, wall-hung WC with a brass flush plate and concealed cistern.
	TBC by sample/shop drawing
	Shared Bathroom & WCs — Fittings

	LT-01
	[image: ] 2700K LED
	Special finish / equipment
	Slim full-height backlit mirror, warm IP spots, and a floor-level night light.
	TBC by sample/shop drawing
	Shared Bathroom & WCs — Lighting

	ST-01
	[image: ] Beige marble
	Bathroom floor
	Beige marble, honed anti-slip (R10) finish. Supplier/Product Code to be selected.
	600×600 mm · laid to falls
	Shared Bathroom & WCs — full floor

	ST-01
	[image: ] Beige marble
	Bathroom walls
	Beige marble full-height cladding, honed. Supplier/Product Code to be selected.
	1200×600 mm · 15–20 mm
	Shared Bathroom & WCs — full-height wet walls

	WF-01
	[image: ] Warm white paint
	Wall paint
	Moisture- and mould-resistant matt emulsion, warm white, 2 coats on primer. Supplier/Product Code to be selected.
	—
	Shared Bathroom & WCs — non-tiled wall areas

	ST-02 / ST-03 / ST-01
	[image: ] Dark Emperador
[image: ] Travertine
	Feature wall
	Bookmatched Silver Travertine / Dark Emperador marble slab cladding behind vanity with backlit mirror. Supplier/Product Code to be selected.
	20 mm slabs, full-height bookmatch
	Shared Bathroom & WCs — vanity wall

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Moisture-resistant (MR) gypsum ceiling, anti-mould warm white matt paint, IP44 trimless downlights. Supplier/Product Code to be selected.
	12.5 mm MR board
	Shared Bathroom & WCs — full ceiling

	JN-01 / LT-01
	[image: ] Smoked walnut
[image: ] 2700K LED
	Vanity
	Wall-hung vanity, smoked walnut veneer on mr-mdf, matt lacquer 10% sheen, soft-close drawers, LED under-glow. Supplier/Product Code to be selected.
	550 mm deep
	Shared Bathroom & WCs — vanity wall

	ST-01 / GL-01 / LT-01
	[image: ] Beige marble
[image: ] Clear glass
	Shower area
	Beige marble walls, fluted marble niche, 10 mm low-iron frameless glass screen; linear drain with tile insert; concealed thermostatic mixer & ceiling rain head. Supplier/Product Code to be selected.
	Screen 10 mm · drain 800 mm
	Shared Bathroom & WCs — walk-in shower

	ST-01
	[image: ] Beige marble
	Countertop
	Beige marble top with integrated moulded basin, honed. Supplier/Product Code to be selected.
	20 mm
	Shared Bathroom & WCs — vanity

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Sanitaryware
	Wall-hung rimless WC with concealed cistern, white gloss; brushed brass (pvd or solid), satin lacquered flush plate & mixers. Supplier/Product Code to be selected.
	—
	Shared Bathroom & WCs — WC and basin

	MT-01
	[image: ] Brushed brass
	Metal finishes
	Brushed brass (PVD or solid), satin lacquered — taps, shower set, towel rail, accessories. Supplier/Product Code to be selected.
	—
	Shared Bathroom & WCs — all fittings

	JN-01 / LT-01
	[image: ] Smoked walnut
[image: ] 2700K LED
	Doors
	Full-height flush door, smoked walnut veneer, concealed frame and hinges, magnetic lock, moisture-resistant core. Supplier/Product Code to be selected.
	800×2700 mm
	Shared Bathroom & WCs — entry door


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 1 · HIGH-END MODERN LUXURY
North Terrace
Upper floor  ·  4.85 m × 1.80 m · off Bedroom Three
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	ST-03
	[image: ] Travertine
	Floor / paving
	600×1200 mm warm travertine, bush-hammered for slip resistance, laid to a 1:80 fall away from the door threshold.
	1200 mm
	North Terrace — Paving

	ST-03 / JN-02
	[image: ] Travertine
[image: ] Natural oak / wood
	Special finish / equipment
	Built-in teak bench, 3.20 m, with quick-dry cream outdoor cushions, and a solid travertine coffee table.
	3.20 m
	North Terrace — Furniture

	LS-01
	[image: ] Planting
	Special finish / equipment
	Two large ribbed stone planters with standard olive trees underplanted with trailing rosemary; drip irrigation from the roof line.
	TBC by sample/shop drawing
	North Terrace — Planting

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Special finish / equipment
	Concealed warm LED in the soffit and under the bench, plus one portable brass lantern. All on the terrace scene, dimmable.
	TBC by sample/shop drawing
	North Terrace — Lighting

	MT-01 / GL-01
	[image: ] Brushed brass
[image: ] Clear glass
	Metal / fittings
	Clear laminated glass with a brushed brass capping rail, matching the villa's metal finish.
	TBC by sample/shop drawing
	North Terrace — Balustrade

	ST-04 / JN-02
	[image: ] Limestone
[image: ] Natural oak / wood
	Outdoor flooring
	Bush-hammered beige limestone, R11 anti-slip with thermally modified ash / teak-tone hardwood decking zones. Supplier/Product Code to be selected.
	600×600 mm · 20 mm
	North Terrace — full terrace, laid to falls

	WF-01
	[image: ] Warm white paint
	Walls
	Exterior textured acrylic render, warm sand / beige, matt. Supplier/Product Code to be selected.
	—
	North Terrace — parapet and back walls

	MT-01 / GL-01
	[image: ] Brushed brass
[image: ] Clear glass
	Balustrade
	Clear frameless laminated glass, brushed brass (pvd or solid), satin lacquered cap. Supplier/Product Code to be selected.
	12+12 mm · 1100 mm
	North Terrace — open edges

	JN-02 / WF-01
	[image: ] Natural oak / wood
[image: ] Warm white paint
	Ceiling
	Exterior soffit, cement board painted warm white / wood-effect aluminium slats. Supplier/Product Code to be selected.
	—
	North Terrace — covered area

	SP-01
	[image: ] Dark bronze / special
	Skirting
	Matching paver upstand
	100 mm
	North Terrace — wall base

	MT-01
	[image: ] Brushed brass
	Doors
	Thermally broken slim aluminium sliding doors, dark bronze, double-glazed. Supplier/Product Code to be selected.
	Per elevation
	North Terrace — opening to bedroom/lobby

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Metal finishes
	Dark bronze powder-coated aluminium / brushed brass (pvd or solid), satin lacquered lights. Supplier/Product Code to be selected.
	—
	North Terrace — fixtures


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 1 · HIGH-END MODERN LUXURY
Master Terrace
Upper floor  ·  4.90 m × 1.20 m · off Master Bedroom Two
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	ST-03
	[image: ] Travertine
	Floor / paving
	Matching bush-hammered travertine, laid in the same direction as the north terrace.
	TBC by sample/shop drawing
	Master Terrace — Paving

	JN-02 / TX-01
	[image: ] Natural oak / wood
[image: ] Textiles
	Special finish / equipment
	Two curved teak loungers with cream outdoor bouclé-look cushions and a round stone side table, all sized to leave a 700 mm clear walking line to the balustrade.
	700 mm
	Master Terrace — Furniture

	LS-01
	[image: ] Planting
	Special finish / equipment
	A continuous 300 mm linear planter along the balustrade with lavender and ornamental grasses — scent and movement rather than mass.
	300 mm
	Master Terrace — Planting

	LT-01 / LS-01
	[image: ] 2700K LED
[image: ] Planting
	Special finish / equipment
	Recessed soffit downlights on the door line, a concealed strip washing the planter, and wall-grazers between the glazing bays. No fixture above eye level.
	TBC by sample/shop drawing
	Master Terrace — Lighting

	JN-02
	[image: ] Natural oak / wood
	Special finish / equipment
	A slatted teak screen at the shared end gives the master terrace visual separation from the neighbouring elevation without closing the view.
	TBC by sample/shop drawing
	Master Terrace — Privacy

	ST-04 / JN-02
	[image: ] Limestone
[image: ] Natural oak / wood
	Outdoor flooring
	Bush-hammered beige limestone, R11 anti-slip with thermally modified ash / teak-tone hardwood decking zones. Supplier/Product Code to be selected.
	600×600 mm · 20 mm
	Master Terrace — full terrace, laid to falls

	WF-01
	[image: ] Warm white paint
	Walls
	Exterior textured acrylic render, warm sand / beige, matt. Supplier/Product Code to be selected.
	—
	Master Terrace — parapet and back walls

	MT-01 / GL-01
	[image: ] Brushed brass
[image: ] Clear glass
	Balustrade
	Clear frameless laminated glass, brushed brass (pvd or solid), satin lacquered cap. Supplier/Product Code to be selected.
	12+12 mm · 1100 mm
	Master Terrace — open edges

	JN-02 / WF-01
	[image: ] Natural oak / wood
[image: ] Warm white paint
	Ceiling
	Exterior soffit, cement board painted warm white / wood-effect aluminium slats. Supplier/Product Code to be selected.
	—
	Master Terrace — covered area

	SP-01
	[image: ] Dark bronze / special
	Skirting
	Matching paver upstand
	100 mm
	Master Terrace — wall base

	MT-01
	[image: ] Brushed brass
	Doors
	Thermally broken slim aluminium sliding doors, dark bronze, double-glazed. Supplier/Product Code to be selected.
	Per elevation
	Master Terrace — opening to bedroom/lobby

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Metal finishes
	Dark bronze powder-coated aluminium / brushed brass (pvd or solid), satin lacquered lights. Supplier/Product Code to be selected.
	—
	Master Terrace — fixtures


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 1 · HIGH-END MODERN LUXURY
Front façade
Exterior & outdoor  ·  01 · Street elevation
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	ST-04 / LT-01
	[image: ] Limestone
[image: ] 2700K LED
	Walls / paint
	Large-format honed limestone in a warm ivory tone, installed with narrow expressed joints.
	TBC by sample/shop drawing
	Front façade — Primary finish

	JN-01 / WF-01
	[image: ] Smoked walnut
[image: ] Warm white paint
	Special finish / equipment
	Warm greige mineral render to recessed planes; smoked-walnut-effect aluminium fins at vertical accents.
	TBC by sample/shop drawing
	Front façade — Contrast volumes

	MT-01 / GL-01
	[image: ] Brushed brass
[image: ] Clear glass
	Metal / fittings
	Dark bronze window frames, copings and shadow-line trims; existing glass balcony retained.
	TBC by sample/shop drawing
	Front façade — Metalwork

	LT-01
	[image: ] 2700K LED
	Special finish / equipment
	Concealed linear light under the cantilever, narrow-beam façade grazers and shielded balcony downlights, all 2700 K.
	2700 K
	Front façade — Lighting

	ST-04
	[image: ] Limestone
	Outdoor paving
	Bush-hammered beige limestone, R11 anti-slip. Supplier/Product Code to be selected.
	600×600 / 900×600 mm · 20–30 mm
	Front façade — paths, terraces and hard landscape

	ST-04 / WF-01
	[image: ] Limestone
[image: ] Warm white paint
	Outdoor walls
	Natural beige limestone cladding with exterior acrylic render, warm sand, matt. Supplier/Product Code to be selected.
	30 mm stone · render 15 mm
	Front façade — façades, boundary and feature walls

	MT-01
	[image: ] Brushed brass
	Outdoor metal
	Dark bronze powder-coated aluminium (gates, pergola, frames, trims). Supplier/Product Code to be selected.
	—
	Front façade — all exterior metalwork

	JN-02
	[image: ] Natural oak / wood
	Outdoor timber
	Thermally modified ash / teak-tone hardwood decking. Supplier/Product Code to be selected.
	140×21 mm boards
	Front façade — decks, cladding and slatted screens

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Outdoor lighting
	2700K IP65 bollards, step lights, uplights and linear wall-washers, dark bronze. Supplier/Product Code to be selected.
	—
	Front façade — per lighting layout


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 1 · HIGH-END MODERN LUXURY
Main entrance, gates & driveway
Exterior & outdoor  ·  02 · Arrival
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	ST-03 / MT-01
	[image: ] Travertine
[image: ] Brushed brass
	Special finish / equipment
	Book-matched vein-cut travertine lining to walls and soffit, framed by a 20 mm champagne-bronze reveal.
	20 mm
	Main entrance, gates & driveway — Portal

	JN-01 / MT-01 / LT-01
	[image: ] Smoked walnut
[image: ] Brushed brass
	Doors / window treatment
	Full-height walnut pivot door with a slim bronze pull and concealed access control.
	TBC by sample/shop drawing
	Main entrance, gates & driveway — Door

	ST-03 / MT-01
	[image: ] Travertine
[image: ] Brushed brass
	Special finish / equipment
	Travertine-clad solid walls with warm greige bands and dark-bronze vertical slat gates.
	TBC by sample/shop drawing
	Main entrance, gates & driveway — Boundary

	SP-01
	[image: ] Dark bronze / special
	Floor / paving
	Honed beige stone modules with charcoal basalt bands guiding cars and pedestrians independently.
	TBC by sample/shop drawing
	Main entrance, gates & driveway — Paving

	ST-04
	[image: ] Limestone
	Outdoor paving
	Bush-hammered beige limestone, R11 anti-slip. Supplier/Product Code to be selected.
	600×600 / 900×600 mm · 20–30 mm
	Main entrance, gates & driveway — paths, terraces and hard landscape

	ST-04 / WF-01
	[image: ] Limestone
[image: ] Warm white paint
	Outdoor walls
	Natural beige limestone cladding with exterior acrylic render, warm sand, matt. Supplier/Product Code to be selected.
	30 mm stone · render 15 mm
	Main entrance, gates & driveway — façades, boundary and feature walls

	MT-01
	[image: ] Brushed brass
	Outdoor metal
	Dark bronze powder-coated aluminium (gates, pergola, frames, trims). Supplier/Product Code to be selected.
	—
	Main entrance, gates & driveway — all exterior metalwork

	JN-02
	[image: ] Natural oak / wood
	Outdoor timber
	Thermally modified ash / teak-tone hardwood decking. Supplier/Product Code to be selected.
	140×21 mm boards
	Main entrance, gates & driveway — decks, cladding and slatted screens

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Outdoor lighting
	2700K IP65 bollards, step lights, uplights and linear wall-washers, dark bronze. Supplier/Product Code to be selected.
	—
	Main entrance, gates & driveway — per lighting layout


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 1 · HIGH-END MODERN LUXURY
Rear façade & pool terrace
Exterior & outdoor  ·  03 · Garden elevation
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	ST-03 / LT-01
	[image: ] Travertine
[image: ] 2700K LED
	Special finish / equipment
	11.00 × 5.92 m footprint retained; pale grey-green stone interior, flush travertine coping and submerged step lighting.
	5.92 m
	Rear façade & pool terrace — Pool

	ST-03 / LT-01
	[image: ] Travertine
[image: ] 2700K LED
	Special finish / equipment
	Slip-resistant honed travertine continuing to the threshold; linear drainage concealed at the façade.
	TBC by sample/shop drawing
	Rear façade & pool terrace — Terrace

	JN-01 / LT-01
	[image: ] Smoked walnut
[image: ] 2700K LED
	Special finish / equipment
	Walnut-effect aluminium pergola slats with integrated dimmable linear lighting and concealed rainwater management.
	TBC by sample/shop drawing
	Rear façade & pool terrace — Shade

	JN-02
	[image: ] Natural oak / wood
	Special finish / equipment
	Low teak lounge seating, cream performance upholstery, sculptural stone tables and a separate outdoor dining setting.
	TBC by sample/shop drawing
	Rear façade & pool terrace — Furniture

	ST-04
	[image: ] Limestone
	Outdoor paving
	Bush-hammered beige limestone, R11 anti-slip. Supplier/Product Code to be selected.
	600×600 / 900×600 mm · 20–30 mm
	Rear façade & pool terrace — paths, terraces and hard landscape

	ST-04 / WF-01
	[image: ] Limestone
[image: ] Warm white paint
	Outdoor walls
	Natural beige limestone cladding with exterior acrylic render, warm sand, matt. Supplier/Product Code to be selected.
	30 mm stone · render 15 mm
	Rear façade & pool terrace — façades, boundary and feature walls

	MT-01
	[image: ] Brushed brass
	Outdoor metal
	Dark bronze powder-coated aluminium (gates, pergola, frames, trims). Supplier/Product Code to be selected.
	—
	Rear façade & pool terrace — all exterior metalwork

	JN-02
	[image: ] Natural oak / wood
	Outdoor timber
	Thermally modified ash / teak-tone hardwood decking. Supplier/Product Code to be selected.
	140×21 mm boards
	Rear façade & pool terrace — decks, cladding and slatted screens

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Outdoor lighting
	2700K IP65 bollards, step lights, uplights and linear wall-washers, dark bronze. Supplier/Product Code to be selected.
	—
	Rear façade & pool terrace — per lighting layout

	ST-04 / TL-01 / GL-01
	[image: ] Limestone
[image: ] Marble-look porcelain
	Pool finish
	Pool interior in sand-beige glass mosaic / porcelain, coping in honed bush-hammered beige limestone, r11 anti-slip. Supplier/Product Code to be selected.
	11.00×5.92 m pool · coping 600×400×30 mm
	Rear façade & pool terrace — pool shell and coping

	ST-04
	[image: ] Limestone
	Pool deck
	Bush-hammered beige limestone, R11 anti-slip, anti-slip. Supplier/Product Code to be selected.
	600×600 mm · 20 mm
	Rear façade & pool terrace — sun deck


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 1 · HIGH-END MODERN LUXURY
Landscape, walkways & outdoor living
Exterior & outdoor  ·  04 · External rooms
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	LS-01
	[image: ] Planting
	Special finish / equipment
	Multi-stem olive trees, date palms where clearance permits, agave, westringia and ornamental grasses in layered beds.
	TBC by sample/shop drawing
	Landscape, walkways & outdoor living — Planting

	ST-04
	[image: ] Limestone
	Special finish / equipment
	600 × 900 mm anti-slip limestone pavers with gravel drainage margins and flush thresholds.
	900 mm
	Landscape, walkways & outdoor living — Walkways

	LT-01 / LS-01
	[image: ] 2700K LED
[image: ] Planting
	Special finish / equipment
	Low-glare spike lights to specimen trees, recessed step lights and shielded bollards along circulation routes.
	TBC by sample/shop drawing
	Landscape, walkways & outdoor living — Garden light

	JN-01 / MT-01
	[image: ] Smoked walnut
[image: ] Brushed brass
	Special finish / equipment
	Existing plan position retained; stone counter, walnut-effect weatherproof cabinetry and a bronze-framed pergola define the outdoor dining room.
	TBC by sample/shop drawing
	Landscape, walkways & outdoor living — BBQ zone

	ST-04
	[image: ] Limestone
	Outdoor paving
	Bush-hammered beige limestone, R11 anti-slip. Supplier/Product Code to be selected.
	600×600 / 900×600 mm · 20–30 mm
	Landscape, walkways & outdoor living — paths, terraces and hard landscape

	ST-04 / WF-01
	[image: ] Limestone
[image: ] Warm white paint
	Outdoor walls
	Natural beige limestone cladding with exterior acrylic render, warm sand, matt. Supplier/Product Code to be selected.
	30 mm stone · render 15 mm
	Landscape, walkways & outdoor living — façades, boundary and feature walls

	MT-01
	[image: ] Brushed brass
	Outdoor metal
	Dark bronze powder-coated aluminium (gates, pergola, frames, trims). Supplier/Product Code to be selected.
	—
	Landscape, walkways & outdoor living — all exterior metalwork

	JN-02
	[image: ] Natural oak / wood
	Outdoor timber
	Thermally modified ash / teak-tone hardwood decking. Supplier/Product Code to be selected.
	140×21 mm boards
	Landscape, walkways & outdoor living — decks, cladding and slatted screens

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Outdoor lighting
	2700K IP65 bollards, step lights, uplights and linear wall-washers, dark bronze. Supplier/Product Code to be selected.
	—
	Landscape, walkways & outdoor living — per lighting layout

	ST-04 / WF-01 / LS-01
	[image: ] Limestone
[image: ] Warm white paint
	Softscape
	Natural lawn, olive / palm feature trees, low hedges, raised planters in render / limestone, drip irrigation. Supplier/Product Code to be selected.
	—
	Landscape, walkways & outdoor living — planting beds and lawn


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 1 · HIGH-END MODERN LUXURY
Swimming pool & sun deck
Exterior & outdoor  ·  11.00 × 5.92 m · depth −0.50 to −1.60 m
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	ST-03
	[image: ] Travertine
	Walls / paint
	Pale grey-green honed stone mosaic interior producing a soft green-blue water colour; 400 mm flush travertine coping with a 10 mm shadow gap.
	400 mm · 10 mm
	Swimming pool & sun deck — Finish

	LT-01
	[image: ] 2700K LED
	Special finish / equipment
	Full-width submerged entry steps at the shallow (−0.50 m) end with a 400 mm sun ledge for children and shallow seating.
	0.50 m · 400 mm
	Swimming pool & sun deck — Entry

	ST-03 / JN-02 / MT-01
	[image: ] Travertine
[image: ] Natural oak / wood
	Special finish / equipment
	Six teak loungers with cream performance cushions, low travertine side tables and two bronze-framed parasols along the villa-side deck.
	TBC by sample/shop drawing
	Swimming pool & sun deck — Furniture

	LT-01
	[image: ] 2700K LED
	Special finish / equipment
	Warm 2700 K submerged niche lights on the long wall, recessed deck markers at 2.5 m centres, no glare-visible fittings from the living room.
	2700 K · 2.5 m
	Swimming pool & sun deck — Lighting

	LT-01 / LS-01
	[image: ] 2700K LED
[image: ] Planting
	Special finish / equipment
	Skimmer line and equipment kept on the north edge nearest the plant space; anti-slip R11 finish to all wet paving; safety cover point discreetly recessed.
	TBC by sample/shop drawing
	Swimming pool & sun deck — Technical

	ST-04
	[image: ] Limestone
	Outdoor paving
	Bush-hammered beige limestone, R11 anti-slip. Supplier/Product Code to be selected.
	600×600 / 900×600 mm · 20–30 mm
	Swimming pool & sun deck — paths, terraces and hard landscape

	ST-04 / WF-01
	[image: ] Limestone
[image: ] Warm white paint
	Outdoor walls
	Natural beige limestone cladding with exterior acrylic render, warm sand, matt. Supplier/Product Code to be selected.
	30 mm stone · render 15 mm
	Swimming pool & sun deck — façades, boundary and feature walls

	MT-01
	[image: ] Brushed brass
	Outdoor metal
	Dark bronze powder-coated aluminium (gates, pergola, frames, trims). Supplier/Product Code to be selected.
	—
	Swimming pool & sun deck — all exterior metalwork

	JN-02
	[image: ] Natural oak / wood
	Outdoor timber
	Thermally modified ash / teak-tone hardwood decking. Supplier/Product Code to be selected.
	140×21 mm boards
	Swimming pool & sun deck — decks, cladding and slatted screens

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Outdoor lighting
	2700K IP65 bollards, step lights, uplights and linear wall-washers, dark bronze. Supplier/Product Code to be selected.
	—
	Swimming pool & sun deck — per lighting layout

	ST-04 / TL-01 / GL-01
	[image: ] Limestone
[image: ] Marble-look porcelain
	Pool finish
	Pool interior in sand-beige glass mosaic / porcelain, coping in honed bush-hammered beige limestone, r11 anti-slip. Supplier/Product Code to be selected.
	11.00×5.92 m pool · coping 600×400×30 mm
	Swimming pool & sun deck — pool shell and coping

	ST-04
	[image: ] Limestone
	Pool deck
	Bush-hammered beige limestone, R11 anti-slip, anti-slip. Supplier/Product Code to be selected.
	600×600 mm · 20 mm
	Swimming pool & sun deck — sun deck


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 1 · HIGH-END MODERN LUXURY
Built-in BBQ pavilion
Exterior & outdoor  ·  North-west corner · approx. 4.50 × 4.50 m
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	ST-03
	[image: ] Travertine
	Countertops / stone
	L-shaped 60 mm honed travertine worktop: 1.40 m preparation run, built-in gas grill, side burner and a raised 1.10 m bar edge with four cushioned stools.
	60 mm · 1.40 m · 1.10 m
	Built-in BBQ pavilion — Counter

	LT-01
	[image: ] 2700K LED
	Special finish / equipment
	Undermount sink with hot and cold supply, outdoor refrigerator and ice drawer, concealed waste bin pull-out, dedicated 16 A circuits and a gas isolation valve.
	16 A
	Built-in BBQ pavilion — Services

	JN-01
	[image: ] Smoked walnut
	Joinery / woodwork
	Walnut-effect marine-grade cabinetry with soft-close doors, a ventilated charcoal store and a lockable cleaning cupboard.
	TBC by sample/shop drawing
	Built-in BBQ pavilion — Storage

	JN-02 / MT-01 / LT-01
	[image: ] Natural oak / wood
[image: ] Brushed brass
	Special finish / equipment
	Dark bronze frame with wood-effect aluminium slats, concealed rainwater downpipe within one column, and dimmable warm linear light to the counter.
	TBC by sample/shop drawing
	Built-in BBQ pavilion — Canopy

	ST-03 / MT-01 / LS-01
	[image: ] Travertine
[image: ] Brushed brass
	Special finish / equipment
	The existing outdoor shower point on the plan is retained and finished in matching travertine with a bronze mixer, screened by planting from the cooking zone.
	TBC by sample/shop drawing
	Built-in BBQ pavilion — Adjacency

	ST-04
	[image: ] Limestone
	Outdoor paving
	Bush-hammered beige limestone, R11 anti-slip. Supplier/Product Code to be selected.
	600×600 / 900×600 mm · 20–30 mm
	Built-in BBQ pavilion — paths, terraces and hard landscape

	ST-04 / WF-01
	[image: ] Limestone
[image: ] Warm white paint
	Outdoor walls
	Natural beige limestone cladding with exterior acrylic render, warm sand, matt. Supplier/Product Code to be selected.
	30 mm stone · render 15 mm
	Built-in BBQ pavilion — façades, boundary and feature walls

	MT-01
	[image: ] Brushed brass
	Outdoor metal
	Dark bronze powder-coated aluminium (gates, pergola, frames, trims). Supplier/Product Code to be selected.
	—
	Built-in BBQ pavilion — all exterior metalwork

	JN-02
	[image: ] Natural oak / wood
	Outdoor timber
	Thermally modified ash / teak-tone hardwood decking. Supplier/Product Code to be selected.
	140×21 mm boards
	Built-in BBQ pavilion — decks, cladding and slatted screens

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Outdoor lighting
	2700K IP65 bollards, step lights, uplights and linear wall-washers, dark bronze. Supplier/Product Code to be selected.
	—
	Built-in BBQ pavilion — per lighting layout

	ST-05
	[image: ] Quartz
	Outdoor countertop
	Flamed / leathered dark granite or exterior sintered stone, UV stable. Supplier/Product Code to be selected.
	30 mm
	Built-in BBQ pavilion — BBQ counter with sink & fridge

	JN-02 / MT-01
	[image: ] Natural oak / wood
[image: ] Brushed brass
	Outdoor cabinets
	Marine-grade stainless steel carcasses with dark bronze / wood-effect HPL doors. Supplier/Product Code to be selected.
	—
	Built-in BBQ pavilion — base units

	JN-02 / MT-01
	[image: ] Natural oak / wood
[image: ] Brushed brass
	Canopy
	Architectural canopy, dark bronze aluminium with wood-effect slat soffit. Supplier/Product Code to be selected.
	Per drawing
	Built-in BBQ pavilion — over BBQ


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 1 · HIGH-END MODERN LUXURY
Garden lounge & lounge deck
Exterior & outdoor  ·  North-east corner · raised deck approx. 3.06 × 3.50 m plus terrace
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	JN-02 / TX-01
	[image: ] Natural oak / wood
[image: ] Textiles
	Special finish / equipment
	Custom modular teak sofa in an L to the two closed sides, two swivel lounge chairs, cream and taupe performance fabrics with bouclé-textured scatter cushions.
	TBC by sample/shop drawing
	Garden lounge & lounge deck — Seating

	ST-03 / JN-01
	[image: ] Travertine
[image: ] Smoked walnut
	Countertops / stone
	Two solid travertine coffee tables at 320 mm and a pair of drum side tables in smoked walnut-effect composite.
	320 mm
	Garden lounge & lounge deck — Tables

	JN-02 / MT-01 / TX-01 / LT-01
	[image: ] Natural oak / wood
[image: ] Brushed brass
	Special finish / equipment
	Bronze-framed pergola with fixed wood-effect slats angled to block midday sun; linen-look outdoor curtains on concealed tracks at the west and north edges.
	TBC by sample/shop drawing
	Garden lounge & lounge deck — Shade

	LT-01
	[image: ] 2700K LED
	Special finish / equipment
	Concealed warm cove light in the pergola beam, two dimmable pendants and floor-recessed uplights washing the columns.
	TBC by sample/shop drawing
	Garden lounge & lounge deck — Lighting

	SP-01
	[image: ] Dark bronze / special
	Special finish / equipment
	Ceiling fan integrated into the canopy, discreet weatherproof sockets and a lidded cushion store below the deck.
	TBC by sample/shop drawing
	Garden lounge & lounge deck — Comfort

	ST-04
	[image: ] Limestone
	Outdoor paving
	Bush-hammered beige limestone, R11 anti-slip. Supplier/Product Code to be selected.
	600×600 / 900×600 mm · 20–30 mm
	Garden lounge & lounge deck — paths, terraces and hard landscape

	ST-04 / WF-01
	[image: ] Limestone
[image: ] Warm white paint
	Outdoor walls
	Natural beige limestone cladding with exterior acrylic render, warm sand, matt. Supplier/Product Code to be selected.
	30 mm stone · render 15 mm
	Garden lounge & lounge deck — façades, boundary and feature walls

	MT-01
	[image: ] Brushed brass
	Outdoor metal
	Dark bronze powder-coated aluminium (gates, pergola, frames, trims). Supplier/Product Code to be selected.
	—
	Garden lounge & lounge deck — all exterior metalwork

	JN-02
	[image: ] Natural oak / wood
	Outdoor timber
	Thermally modified ash / teak-tone hardwood decking. Supplier/Product Code to be selected.
	140×21 mm boards
	Garden lounge & lounge deck — decks, cladding and slatted screens

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Outdoor lighting
	2700K IP65 bollards, step lights, uplights and linear wall-washers, dark bronze. Supplier/Product Code to be selected.
	—
	Garden lounge & lounge deck — per lighting layout

	JN-02 / MT-01 / TX-01
	[image: ] Natural oak / wood
[image: ] Brushed brass
	Pergola
	Dark bronze aluminium pergola with wood-effect louvres, outdoor-fabric upholstery in sand / taupe. Supplier/Product Code to be selected.
	Per drawing
	Garden lounge & lounge deck — seating area

	ST-04 / WF-01 / LS-01
	[image: ] Limestone
[image: ] Warm white paint
	Softscape
	Natural lawn, olive / palm feature trees, low hedges, raised planters in render / limestone, drip irrigation. Supplier/Product Code to be selected.
	—
	Garden lounge & lounge deck — planting beds and lawn


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 1 · HIGH-END MODERN LUXURY
Terrace dining under the pergola
Exterior & outdoor  ·  Rear terrace, aligned with the internal dining and kitchen doors
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	ST-03 / JN-01
	[image: ] Travertine
[image: ] Smoked walnut
	Countertops / stone
	3.00 m travertine top on a smoked walnut plinth base, seating ten in woven cream armchairs with quick-dry cushions.
	3.00 m
	Terrace dining under the pergola — Table

	JN-02 / TX-01
	[image: ] Natural oak / wood
[image: ] Textiles
	Special finish / equipment
	Continuation of the wood-slat pergola with integrated retractable fabric layer for full shade in summer.
	TBC by sample/shop drawing
	Terrace dining under the pergola — Shade

	LT-01
	[image: ] 2700K LED
	Special finish / equipment
	Three woven pendants on dimmers over the table, plus wall-recessed step lights along the threshold.
	TBC by sample/shop drawing
	Terrace dining under the pergola — Lighting

	ST-03 / LT-01
	[image: ] Travertine
[image: ] 2700K LED
	Special finish / equipment
	A short travertine buffet ledge against the villa wall with concealed sockets, warming drawer provision and a beverage fridge.
	TBC by sample/shop drawing
	Terrace dining under the pergola — Service

	ST-04
	[image: ] Limestone
	Outdoor paving
	Bush-hammered beige limestone, R11 anti-slip. Supplier/Product Code to be selected.
	600×600 / 900×600 mm · 20–30 mm
	Terrace dining under the pergola — paths, terraces and hard landscape

	ST-04 / WF-01
	[image: ] Limestone
[image: ] Warm white paint
	Outdoor walls
	Natural beige limestone cladding with exterior acrylic render, warm sand, matt. Supplier/Product Code to be selected.
	30 mm stone · render 15 mm
	Terrace dining under the pergola — façades, boundary and feature walls

	MT-01
	[image: ] Brushed brass
	Outdoor metal
	Dark bronze powder-coated aluminium (gates, pergola, frames, trims). Supplier/Product Code to be selected.
	—
	Terrace dining under the pergola — all exterior metalwork

	JN-02
	[image: ] Natural oak / wood
	Outdoor timber
	Thermally modified ash / teak-tone hardwood decking. Supplier/Product Code to be selected.
	140×21 mm boards
	Terrace dining under the pergola — decks, cladding and slatted screens

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Outdoor lighting
	2700K IP65 bollards, step lights, uplights and linear wall-washers, dark bronze. Supplier/Product Code to be selected.
	—
	Terrace dining under the pergola — per lighting layout

	JN-02 / MT-01 / TX-01
	[image: ] Natural oak / wood
[image: ] Brushed brass
	Pergola
	Dark bronze aluminium pergola with wood-effect louvres, outdoor-fabric upholstery in sand / taupe. Supplier/Product Code to be selected.
	Per drawing
	Terrace dining under the pergola — seating area


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 1 · HIGH-END MODERN LUXURY
Children's play garden
Exterior & outdoor  ·  West lawn · within the 12.60 × 7.80 m tree area
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	JN-02
	[image: ] Natural oak / wood
	Special finish / equipment
	FSC oak play tower with slide, rope climb and two swings on a clean timber frame; a low balance course and a sand/water play table.
	TBC by sample/shop drawing
	Children's play garden — Equipment

	LS-01 / FL-01
	[image: ] Planting
[image: ] EPDM rubber
	Floor / paving
	Sand-beige wet-pour rubber with a 1.5 m critical-fall zone, laid in an organic shape and edged flush with the lawn.
	1.5 m
	Children's play garden — Safety surface

	ST-03 / LS-01
	[image: ] Travertine
[image: ] Planting
	Special finish / equipment
	Curved travertine seat wall with cushions facing the play zone, in direct sight line from the living room glazing; pool access screened by a hedge and a self-closing gate.
	TBC by sample/shop drawing
	Children's play garden — Supervision

	LT-01 / LS-01
	[image: ] 2700K LED
[image: ] Planting
	Special finish / equipment
	Existing trees provide the primary canopy; low-level warm bollards and shielded tree uplights only, no glare at child height.
	TBC by sample/shop drawing
	Children's play garden — Shade & light

	ST-04
	[image: ] Limestone
	Outdoor paving
	Bush-hammered beige limestone, R11 anti-slip. Supplier/Product Code to be selected.
	600×600 / 900×600 mm · 20–30 mm
	Children's play garden — paths, terraces and hard landscape

	ST-04 / WF-01
	[image: ] Limestone
[image: ] Warm white paint
	Outdoor walls
	Natural beige limestone cladding with exterior acrylic render, warm sand, matt. Supplier/Product Code to be selected.
	30 mm stone · render 15 mm
	Children's play garden — façades, boundary and feature walls

	MT-01
	[image: ] Brushed brass
	Outdoor metal
	Dark bronze powder-coated aluminium (gates, pergola, frames, trims). Supplier/Product Code to be selected.
	—
	Children's play garden — all exterior metalwork

	JN-02
	[image: ] Natural oak / wood
	Outdoor timber
	Thermally modified ash / teak-tone hardwood decking. Supplier/Product Code to be selected.
	140×21 mm boards
	Children's play garden — decks, cladding and slatted screens

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Outdoor lighting
	2700K IP65 bollards, step lights, uplights and linear wall-washers, dark bronze. Supplier/Product Code to be selected.
	—
	Children's play garden — per lighting layout

	FL-01
	[image: ] EPDM rubber
	Safety flooring
	Wet-pour EPDM rubber safety surface, sand / sage colours. Supplier/Product Code to be selected.
	40–80 mm (per fall height, EN 1177)
	Children's play garden — whole play zone

	ST-04 / WF-01 / LS-01
	[image: ] Limestone
[image: ] Warm white paint
	Softscape
	Natural lawn, olive / palm feature trees, low hedges, raised planters in render / limestone, drip irrigation. Supplier/Product Code to be selected.
	—
	Children's play garden — planting beds and lawn


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 1 · HIGH-END MODERN LUXURY
Garden, walkways and planters
Exterior & outdoor  ·  Perimeter strips, west lawn and boundary beds per plan
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	LS-01
	[image: ] Planting
	Special finish / equipment
	The three existing mature trees on the west lawn are retained and crown-lifted; date palms and multi-stem olives reinforce the boundary strips shown on the plan.
	TBC by sample/shop drawing
	Garden, walkways and planters — Trees

	LS-01
	[image: ] Planting
	Special finish / equipment
	Structure from clipped myrtle and box near the villa; texture from westringia, lavender, agave, rosemary and ornamental grasses at the perimeter. Drought-tolerant throughout.
	TBC by sample/shop drawing
	Garden, walkways and planters — Planting

	LS-01
	[image: ] Planting
	Special finish / equipment
	Warm-season turf to the west area with a flush stone mowing edge; irrigated by sub-surface drip with a smart controller.
	TBC by sample/shop drawing
	Garden, walkways and planters — Lawn

	ST-04
	[image: ] Limestone
	Floor / paving
	600 × 900 mm anti-slip honed limestone with 10 mm joints and gravel drainage margins; charcoal basalt bands mark thresholds and changes of zone.
	900 mm · 10 mm
	Garden, walkways and planters — Paving

	ST-03 / LS-01
	[image: ] Travertine
[image: ] Planting
	Special finish / equipment
	Large monolithic travertine planters at the terrace corners and pavilion entries, planted with olive standards and trailing rosemary.
	TBC by sample/shop drawing
	Garden, walkways and planters — Planters

	LT-01 / LS-01
	[image: ] 2700K LED
[image: ] Planting
	Special finish / equipment
	One warm 2700 K family throughout: tree uplights, shielded 400 mm bollards on walkways, recessed step lights and grazers on the boundary wall — every source shielded from seated eye level.
	2700 K · 400 mm
	Garden, walkways and planters — Lighting

	ST-04
	[image: ] Limestone
	Outdoor paving
	Bush-hammered beige limestone, R11 anti-slip. Supplier/Product Code to be selected.
	600×600 / 900×600 mm · 20–30 mm
	Garden, walkways and planters — paths, terraces and hard landscape

	ST-04 / WF-01
	[image: ] Limestone
[image: ] Warm white paint
	Outdoor walls
	Natural beige limestone cladding with exterior acrylic render, warm sand, matt. Supplier/Product Code to be selected.
	30 mm stone · render 15 mm
	Garden, walkways and planters — façades, boundary and feature walls

	MT-01
	[image: ] Brushed brass
	Outdoor metal
	Dark bronze powder-coated aluminium (gates, pergola, frames, trims). Supplier/Product Code to be selected.
	—
	Garden, walkways and planters — all exterior metalwork

	JN-02
	[image: ] Natural oak / wood
	Outdoor timber
	Thermally modified ash / teak-tone hardwood decking. Supplier/Product Code to be selected.
	140×21 mm boards
	Garden, walkways and planters — decks, cladding and slatted screens

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Outdoor lighting
	2700K IP65 bollards, step lights, uplights and linear wall-washers, dark bronze. Supplier/Product Code to be selected.
	—
	Garden, walkways and planters — per lighting layout

	ST-04 / WF-01 / LS-01
	[image: ] Limestone
[image: ] Warm white paint
	Softscape
	Natural lawn, olive / palm feature trees, low hedges, raised planters in render / limestone, drip irrigation. Supplier/Product Code to be selected.
	—
	Garden, walkways and planters — planting beds and lawn


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 2 · AFFORDABLE MODERN LUXURY
Main Entrance & Lobby
Ground floor  ·  Entry axis 4.20 m deep · 1.30 m opening to the living wing
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	ST-01 / TL-01
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Floor / paving
	120×120 cm marble-look porcelain, rectified, straight set with 2 mm joints. No inlay medallion, no waterjet cutting — the single biggest saving on this floor.
	120 cm · 2 mm
	Main Entrance & Lobby — Flooring

	JN-02 / WF-01
	[image: ] Natural oak / wood
[image: ] Warm white paint
	Walls / paint
	Premium washable matt paint in warm greige, with one feature wall in a factory-made oak-veneer slat panel system instead of carved fluted stone.
	TBC by sample/shop drawing
	Main Entrance & Lobby — Walls

	MT-01 / GL-01 / LT-01
	[image: ] Brushed brass
[image: ] Clear glass
	Ceiling
	Simple single-step gypsum drop with a continuous cove (3000 K) and standard recessed spots. One catalogue glass-and-black-metal pendant replaces the bespoke brass cascade.
	3000 K
	Main Entrance & Lobby — Ceiling & lighting

	ST-01 / JN-02
	[image: ] Beige marble
[image: ] Natural oak / wood
	Joinery / woodwork
	Modular flush cloak cupboard in melamine carcass with veneer fronts; wall-hung shelf console in the same veneer instead of a solid marble slab.
	TBC by sample/shop drawing
	Main Entrance & Lobby — Joinery

	ST-01 / TL-01
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Flooring
	Marble-look rectified porcelain (warm beige / cream vein), matt-satin. Supplier/Product Code to be selected.
	1200×600 mm · 9–10 mm thick
	Main Entrance & Lobby — full floor area

	WF-01
	[image: ] Warm white paint
	Walls
	Gypsum skim plaster, smooth level-5 finish ready for paint
	Plaster 10–13 mm
	Main Entrance & Lobby — all walls except feature wall

	WF-01
	[image: ] Warm white paint
	Wall paint
	Wall paint: warm white / greige washable matt emulsion (Jotun Fenomastic or equal), 2 coats on primer. Supplier/Product Code to be selected.
	—
	Main Entrance & Lobby — all painted walls

	ST-03 / TL-01
	[image: ] Travertine
[image: ] Marble-look porcelain
	Feature wall
	Large-format travertine-look porcelain slab cladding (stone-effect). Supplier/Product Code to be selected.
	1200×2400 mm slabs · 6–12 mm
	Main Entrance & Lobby — entrance feature wall

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Gypsum board ceiling, warm white matt paint, perimeter shadow-gap with 2700K LED cove, trimless downlights. Supplier/Product Code to be selected.
	12.5 mm board · 2.9–3.0 m FFL
	Main Entrance & Lobby — full ceiling

	WF-01 / MT-01
	[image: ] Warm white paint
[image: ] Brushed brass
	Skirting
	Recessed shadow-gap skirting, brass-effect brushed pvd / powder-coat champagne bronze trim / flush painted MDF
	80 mm high · 10 mm reveal
	Main Entrance & Lobby — all wall perimeters

	JN-02
	[image: ] Natural oak / wood
	Joinery
	Engineered natural oak veneer / oak-effect HPL on MR-MDF, matt. Supplier/Product Code to be selected.
	18 mm core
	Main Entrance & Lobby — built-in units and wall panelling

	JN-02 / LT-01
	[image: ] Natural oak / wood
[image: ] 2700K LED
	Doors
	Full-height flush door, oak-effect laminate / veneer, concealed frame, concealed hinges. Supplier/Product Code to be selected.
	900×2700 mm · 50 mm leaf
	Main Entrance & Lobby — entry door(s)

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Metal finishes
	Brass-effect brushed PVD / powder-coat champagne bronze — door handles, inlays, light fittings, joinery pulls. Supplier/Product Code to be selected.
	—
	Main Entrance & Lobby — all visible metalwork


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 2 · AFFORDABLE MODERN LUXURY
Formal Guest Lounge
Ground floor  ·  9.50 m long × 5.65 m deep — south wing, direct off the entrance
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	ST-01 / TL-01 / JN-02 / MT-01
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Special finish / equipment
	1.60 m linear electric/gas insert in a marble-look porcelain slab surround with an oak-veneer reveal instead of honed emperador and brass. Same visual weight, a fraction of the stone cost.
	1.60 m
	Formal Guest Lounge — Fireplace

	TL-01 / WF-01 / MT-01 / TX-01
	[image: ] Marble-look porcelain
[image: ] Warm white paint
	Walls / paint
	Porcelain slab centre panel flanked by painted MDF grooved panelling in warm sand — the upholstered fabric panels and brass profiles of Option 1 are dropped.
	1 a
	Formal Guest Lounge — Feature wall

	ST-01 / TX-01
	[image: ] Beige marble
[image: ] Textiles
	Special finish / equipment
	Locally made perimeter sofas, 90 cm deep, in a heavy performance weave rather than velvet; two ceramic-top side tables replacing solid marble cubes.
	90 cm
	Formal Guest Lounge — Furniture

	LT-01
	[image: ] 2700K LED
	Ceiling
	Single-step perimeter cove, no stepped profile. Two medium catalogue pendants instead of one large bespoke chandelier, plus dimmable spots.
	TBC by sample/shop drawing
	Formal Guest Lounge — Ceiling & lighting

	TX-01
	[image: ] Textiles
	Doors / window treatment
	Sheer plus lined cream drapery on a recessed track — the one detail kept exactly as Option 1.
	TBC by sample/shop drawing
	Formal Guest Lounge — Curtains

	ST-01 / TL-01
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Flooring
	Marble-look rectified porcelain (warm beige / cream vein), matt-satin. Supplier/Product Code to be selected.
	1200×600 mm · 9–10 mm thick
	Formal Guest Lounge — full floor area

	WF-01
	[image: ] Warm white paint
	Walls
	Gypsum skim plaster, smooth level-5 finish ready for paint
	Plaster 10–13 mm
	Formal Guest Lounge — all walls except feature wall

	WF-01
	[image: ] Warm white paint
	Wall paint
	Wall paint: warm white / greige washable matt emulsion (Jotun Fenomastic or equal), 2 coats on primer. Supplier/Product Code to be selected.
	—
	Formal Guest Lounge — all painted walls

	ST-03 / TL-01
	[image: ] Travertine
[image: ] Marble-look porcelain
	Feature wall
	Large-format travertine-look porcelain slab cladding (stone-effect). Supplier/Product Code to be selected.
	1200×2400 mm slabs · 6–12 mm
	Formal Guest Lounge — fireplace / TV wall

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Gypsum board ceiling, warm white matt paint, perimeter shadow-gap with 2700K LED cove, trimless downlights. Supplier/Product Code to be selected.
	12.5 mm board · 2.9–3.0 m FFL
	Formal Guest Lounge — full ceiling

	WF-01 / MT-01
	[image: ] Warm white paint
[image: ] Brushed brass
	Skirting
	Recessed shadow-gap skirting, brass-effect brushed pvd / powder-coat champagne bronze trim / flush painted MDF
	80 mm high · 10 mm reveal
	Formal Guest Lounge — all wall perimeters

	JN-02
	[image: ] Natural oak / wood
	Joinery
	Engineered natural oak veneer / oak-effect HPL on MR-MDF, matt. Supplier/Product Code to be selected.
	18 mm core
	Formal Guest Lounge — built-in units and wall panelling

	JN-02 / LT-01
	[image: ] Natural oak / wood
[image: ] 2700K LED
	Doors
	Full-height flush door, oak-effect laminate / veneer, concealed frame, concealed hinges. Supplier/Product Code to be selected.
	900×2700 mm · 50 mm leaf
	Formal Guest Lounge — entry door(s)

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Metal finishes
	Brass-effect brushed PVD / powder-coat champagne bronze — door handles, inlays, light fittings, joinery pulls. Supplier/Product Code to be selected.
	—
	Formal Guest Lounge — all visible metalwork

	ST-03 / TL-01 / MT-01
	[image: ] Travertine
[image: ] Marble-look porcelain
	Fireplace
	Linear built-in fireplace with large-format travertine-look porcelain slab cladding (stone-effect) surround and brass-effect brushed pvd / powder-coat champagne bronze trim. Supplier/Product Code to be selected.
	1500–1800 mm firebox
	Formal Guest Lounge — fireplace wall


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 2 · AFFORDABLE MODERN LUXURY
Main Family Living Room
Ground floor  ·  9.41 × 6.90 m — north-west, open to the kitchen
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	ST-01 / TL-01
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Walls / paint
	Two 160×320 cm marble-look porcelain slabs (not book-matched natural marble) with a recessed screen niche and a 1.80 m linear fire beneath, in one plane.
	320 cm · 1.80 m
	Main Family Living Room — Feature wall

	JN-01 / JN-02 / LT-01
	[image: ] Smoked walnut
[image: ] Natural oak / wood
	Joinery / woodwork
	3.60 m floating console in oak-effect laminate with a veneer face and LED shadow gap — visually identical at 2 m, roughly a third of the smoked-walnut cost.
	3.60 m · 2 m
	Main Family Living Room — Joinery

	JN-02 / TX-01
	[image: ] Natural oak / wood
[image: ] Textiles
	Walls / paint
	Prefabricated acoustic slat panels on the long internal wall instead of site-built oak slats on acoustic backing.
	TBC by sample/shop drawing
	Main Family Living Room — Accent wall

	LT-01
	[image: ] 2700K LED
	Ceiling
	Flat ceiling with a single perimeter cove and a linear magnetic track over each cluster; one modest decorative fixture per bay.
	TBC by sample/shop drawing
	Main Family Living Room — Ceiling & lighting

	TX-01
	[image: ] Textiles
	Special finish / equipment
	Cream weave four-seater, four fabric lounge chairs, ceramic-top coffee tables; second bay with two locally made sofas.
	TBC by sample/shop drawing
	Main Family Living Room — Furniture

	ST-01 / TL-01
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Flooring
	Marble-look rectified porcelain (warm beige / cream vein), matt-satin. Supplier/Product Code to be selected.
	1200×600 mm · 9–10 mm thick
	Main Family Living Room — full floor area

	WF-01
	[image: ] Warm white paint
	Walls
	Gypsum skim plaster, smooth level-5 finish ready for paint
	Plaster 10–13 mm
	Main Family Living Room — all walls except feature wall

	WF-01
	[image: ] Warm white paint
	Wall paint
	Wall paint: warm white / greige washable matt emulsion (Jotun Fenomastic or equal), 2 coats on primer. Supplier/Product Code to be selected.
	—
	Main Family Living Room — all painted walls

	ST-03 / TL-01
	[image: ] Travertine
[image: ] Marble-look porcelain
	Feature wall
	Large-format travertine-look porcelain slab cladding (stone-effect). Supplier/Product Code to be selected.
	1200×2400 mm slabs · 6–12 mm
	Main Family Living Room — fireplace / TV wall

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Gypsum board ceiling, warm white matt paint, perimeter shadow-gap with 2700K LED cove, trimless downlights. Supplier/Product Code to be selected.
	12.5 mm board · 2.9–3.0 m FFL
	Main Family Living Room — full ceiling

	WF-01 / MT-01
	[image: ] Warm white paint
[image: ] Brushed brass
	Skirting
	Recessed shadow-gap skirting, brass-effect brushed pvd / powder-coat champagne bronze trim / flush painted MDF
	80 mm high · 10 mm reveal
	Main Family Living Room — all wall perimeters

	JN-02
	[image: ] Natural oak / wood
	Joinery
	Engineered natural oak veneer / oak-effect HPL on MR-MDF, matt. Supplier/Product Code to be selected.
	18 mm core
	Main Family Living Room — built-in units and wall panelling

	JN-02 / LT-01
	[image: ] Natural oak / wood
[image: ] 2700K LED
	Doors
	Full-height flush door, oak-effect laminate / veneer, concealed frame, concealed hinges. Supplier/Product Code to be selected.
	900×2700 mm · 50 mm leaf
	Main Family Living Room — entry door(s)

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Metal finishes
	Brass-effect brushed PVD / powder-coat champagne bronze — door handles, inlays, light fittings, joinery pulls. Supplier/Product Code to be selected.
	—
	Main Family Living Room — all visible metalwork

	ST-03 / TL-01 / MT-01
	[image: ] Travertine
[image: ] Marble-look porcelain
	Fireplace
	Linear built-in fireplace with large-format travertine-look porcelain slab cladding (stone-effect) surround and brass-effect brushed pvd / powder-coat champagne bronze trim. Supplier/Product Code to be selected.
	1500–1800 mm firebox
	Main Family Living Room — fireplace wall


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 2 · AFFORDABLE MODERN LUXURY
Dining Area
Ground floor  ·  5.65 m deep × 4.20 m — north-east of the guest lounge, as drawn
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	ST-05 / JN-01 / TX-01
	[image: ] Quartz
[image: ] Smoked walnut
	Countertops / stone
	1.80 m round table with a sintered-stone top on a veneered MDF pedestal; eight upholstered fabric chairs from a local maker instead of leather and walnut.
	1.80 m
	Dining Area — Table & seating

	TL-01 / JN-02
	[image: ] Marble-look porcelain
[image: ] Natural oak / wood
	Joinery / woodwork
	Low buffet only (no full-height crockery unit), oak-veneer fronts with a porcelain top and a single lit open niche above.
	TBC by sample/shop drawing
	Dining Area — Joinery

	MT-01 / GL-01 / LT-01
	[image: ] Brushed brass
[image: ] Clear glass
	Special finish / equipment
	One three-tier catalogue pendant in matt bronze with opal glass on a dimmer.
	TBC by sample/shop drawing
	Dining Area — Lighting

	WF-01 / MT-01
	[image: ] Warm white paint
[image: ] Brushed brass
	Walls / paint
	Premium paint with one textured wallpaper panel replacing the antique-bronze mirror wall.
	TBC by sample/shop drawing
	Dining Area — Walls

	ST-01 / TL-01
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Flooring
	Marble-look rectified porcelain (warm beige / cream vein), matt-satin. Supplier/Product Code to be selected.
	1200×600 mm · 9–10 mm thick
	Dining Area — full floor area

	WF-01
	[image: ] Warm white paint
	Walls
	Gypsum skim plaster, smooth level-5 finish ready for paint
	Plaster 10–13 mm
	Dining Area — all walls except feature wall

	WF-01
	[image: ] Warm white paint
	Wall paint
	Wall paint: warm white / greige washable matt emulsion (Jotun Fenomastic or equal), 2 coats on primer. Supplier/Product Code to be selected.
	—
	Dining Area — all painted walls

	ST-03 / TL-01
	[image: ] Travertine
[image: ] Marble-look porcelain
	Feature wall
	Large-format travertine-look porcelain slab cladding (stone-effect). Supplier/Product Code to be selected.
	1200×2400 mm slabs · 6–12 mm
	Dining Area — dining feature wall

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Gypsum board ceiling, warm white matt paint, perimeter shadow-gap with 2700K LED cove, trimless downlights. Supplier/Product Code to be selected.
	12.5 mm board · 2.9–3.0 m FFL
	Dining Area — full ceiling

	WF-01 / MT-01
	[image: ] Warm white paint
[image: ] Brushed brass
	Skirting
	Recessed shadow-gap skirting, brass-effect brushed pvd / powder-coat champagne bronze trim / flush painted MDF
	80 mm high · 10 mm reveal
	Dining Area — all wall perimeters

	JN-02
	[image: ] Natural oak / wood
	Joinery
	Engineered natural oak veneer / oak-effect HPL on MR-MDF, matt. Supplier/Product Code to be selected.
	18 mm core
	Dining Area — built-in units and wall panelling

	JN-02 / LT-01
	[image: ] Natural oak / wood
[image: ] 2700K LED
	Doors
	Full-height flush door, oak-effect laminate / veneer, concealed frame, concealed hinges. Supplier/Product Code to be selected.
	900×2700 mm · 50 mm leaf
	Dining Area — entry door(s)

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Metal finishes
	Brass-effect brushed PVD / powder-coat champagne bronze — door handles, inlays, light fittings, joinery pulls. Supplier/Product Code to be selected.
	—
	Dining Area — all visible metalwork

	ST-05 / JN-01 / JN-02
	[image: ] Quartz
[image: ] Smoked walnut
	Countertops / stone
	Dining table top in quartz, warm white with soft grey vein, polished; walnut/oak sideboard. Supplier/Product Code to be selected.
	20–30 mm
	Dining Area — table & sideboard


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 2 · AFFORDABLE MODERN LUXURY
Kitchen
Ground floor  ·  North band of the 12.00 m frontage, open to the living and dining areas, service door to the maid's room
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	JN-02
	[image: ] Natural oak / wood
	Joinery / woodwork
	High-quality modular handleless system: matt cream lacquer-effect tall run, oak-effect melamine island. Appliances integrated except a single visible oven column.
	TBC by sample/shop drawing
	Kitchen — Cabinetry

	TL-01 / ST-05
	[image: ] Marble-look porcelain
[image: ] Quartz
	Floor / paving
	Engineered quartz worktops and a 60 cm porcelain splashback rather than a full-height book-matched slab.
	60 cm
	Kitchen — Surfaces

	SP-01
	[image: ] Dark bronze / special
	Countertops / stone
	Straight square edge instead of a waterfall return, 30 cm overhang, three stools, surface-mounted socket strip.
	30 cm
	Kitchen — Island

	GL-01 / LT-01
	[image: ] Clear glass
[image: ] 2700K LED
	Special finish / equipment
	Three simple opal-glass pendants and under-cabinet LED, all 3000 K.
	3000 K
	Kitchen — Lighting

	ST-01 / TL-01
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Flooring
	Marble-look rectified porcelain (warm beige / cream vein), matt-satin. Supplier/Product Code to be selected.
	1200×600 mm · 9–10 mm thick
	Kitchen — full floor area

	WF-01
	[image: ] Warm white paint
	Walls
	Gypsum skim plaster, smooth level-5 finish ready for paint
	Plaster 10–13 mm
	Kitchen — all walls except feature wall

	WF-01
	[image: ] Warm white paint
	Wall paint
	Wall paint: warm white / greige washable matt emulsion (Jotun Fenomastic or equal), 2 coats on primer. Supplier/Product Code to be selected.
	—
	Kitchen — all painted walls

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Gypsum board ceiling, warm white matt paint, perimeter shadow-gap with 2700K LED cove, trimless downlights. Supplier/Product Code to be selected.
	12.5 mm board · 2.9–3.0 m FFL
	Kitchen — full ceiling

	WF-01 / MT-01
	[image: ] Warm white paint
[image: ] Brushed brass
	Skirting
	Recessed shadow-gap skirting, brass-effect brushed pvd / powder-coat champagne bronze trim / flush painted MDF
	80 mm high · 10 mm reveal
	Kitchen — all wall perimeters

	JN-02
	[image: ] Natural oak / wood
	Joinery
	Engineered natural oak veneer / oak-effect HPL on MR-MDF, matt. Supplier/Product Code to be selected.
	18 mm core
	Kitchen — built-in units and wall panelling

	JN-02 / LT-01
	[image: ] Natural oak / wood
[image: ] 2700K LED
	Doors
	Full-height flush door, oak-effect laminate / veneer, concealed frame, concealed hinges. Supplier/Product Code to be selected.
	900×2700 mm · 50 mm leaf
	Kitchen — entry door(s)

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Metal finishes
	Brass-effect brushed PVD / powder-coat champagne bronze — door handles, inlays, light fittings, joinery pulls. Supplier/Product Code to be selected.
	—
	Kitchen — all visible metalwork

	JN-02
	[image: ] Natural oak / wood
	Kitchen cabinets
	Warm taupe matt lacquer / anti-fingerprint laminate base units + oak-effect tall units, handleless profile, soft-close hinges & drawers. Supplier/Product Code to be selected.
	18 mm carcass · 600 mm base depth
	Kitchen — base, wall, tall units and island

	ST-05
	[image: ] Quartz
	Kitchen countertop
	Quartz, warm white with soft grey vein, polished. Supplier/Product Code to be selected.
	20 mm + 40 mm mitred edge / waterfall island
	Kitchen — worktops and island

	ST-05
	[image: ] Quartz
	Backsplash
	Full-height slab in matching quartz. Supplier/Product Code to be selected.
	Slab to underside of wall units
	Kitchen — cooking and sink walls


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 2 · AFFORDABLE MODERN LUXURY
Staircase
Ground floor  ·  2.15 m wide flight · 20 risers · 2.81 m landing
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	ST-01 / TL-01 / MT-01
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Floor / paving
	Marble-look large-format porcelain stair tiles with a matching bullnose nosing; matte cream risers. No brass inlay.
	TBC by sample/shop drawing
	Staircase — Treads & risers

	JN-02 / GL-01
	[image: ] Natural oak / wood
[image: ] Clear glass
	Metal / fittings
	Frameless clear toughened glass in a satin aluminium base channel with an oak-effect cap handrail — the same glass concept as Option 1, in a standard system rather than a bespoke one.
	TBC by sample/shop drawing
	Staircase — Balustrade

	LT-01
	[image: ] 2700K LED
	Special finish / equipment
	Handrail LED plus one linear multi-drop pendant in the void — one fixture, not a bespoke cascade.
	TBC by sample/shop drawing
	Staircase — Lighting

	WF-01
	[image: ] Warm white paint
	Walls / paint
	Textured paint finish with one large print; understair volume in modular flush storage.
	TBC by sample/shop drawing
	Staircase — Wall & understair

	ST-01 / TL-01
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Staircase treads
	Marble-look porcelain treads with bullnose nosing, matt anti-slip. Supplier/Product Code to be selected.
	Tread 300 mm · riser 160–170 mm · 20–30 mm
	Staircase — all flights and landings

	GL-01
	[image: ] Clear glass
	Balustrade
	Clear frameless laminated toughened glass in recessed floor channel, no handrail rods. Supplier/Product Code to be selected.
	12+12 mm laminated · 1100 mm high
	Staircase — open side of flights and landing

	MT-01
	[image: ] Brushed brass
	Handrail
	Brass-effect brushed PVD / powder-coat champagne bronze slim wall-mounted handrail. Supplier/Product Code to be selected.
	Ø40 mm
	Staircase — wall side

	LT-01
	[image: ] 2700K LED
	Stair lighting
	Recessed 2700K LED step lights / under-tread LED strip. Supplier/Product Code to be selected.
	—
	Staircase — every 2nd step

	WF-01
	[image: ] Warm white paint
	Walls
	Gypsum skim plaster, smooth level-5 finish
	—
	Staircase — stairwell walls

	WF-01
	[image: ] Warm white paint
	Wall paint
	Wall paint: warm white / greige washable matt emulsion (Jotun Fenomastic or equal), 2 coats on primer. Supplier/Product Code to be selected.
	—
	Staircase — stairwell walls

	ST-03 / TL-01
	[image: ] Travertine
[image: ] Marble-look porcelain
	Feature wall
	Large-format travertine-look porcelain slab cladding (stone-effect). Supplier/Product Code to be selected.
	1200×2400 mm slabs · 6–12 mm
	Staircase — double-height stair wall

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Gypsum board ceiling, warm white matt paint, perimeter shadow-gap with 2700K LED cove, trimless downlights; feature pendant to double-height void. Supplier/Product Code to be selected.
	—
	Staircase — soffit and void

	ST-01 / TL-01
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Skirting
	Stringer skirting in matching marble-look porcelain treads with bullnose nosing
	100 mm
	Staircase — wall stringer


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 2 · AFFORDABLE MODERN LUXURY
Guest WCs
Ground floor  ·  Guest WC 2.40 × 1.20 m off the lobby · second WC 1.82 m wide on the service side
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	ST-03 / ST-01 / TL-01
	[image: ] Travertine
[image: ] Beige marble
	Walls / paint
	120×280 cm marble-look and travertine-look porcelain slabs on the feature wall, large-format tile elsewhere. No natural stone.
	280 cm
	Guest WCs — Finishes

	SP-01
	[image: ] Dark bronze / special
	Special finish / equipment
	Standard-size wall-hung units with veneer fronts and integrated ceramic basins rather than carved stone basins.
	TBC by sample/shop drawing
	Guest WCs — Vanities

	LT-01
	[image: ] 2700K LED
	Special finish / equipment
	Backlit mirror plus a single wall light; the lit accessory niche is retained in the guest WC only.
	TBC by sample/shop drawing
	Guest WCs — Lighting

	SP-01
	[image: ] Dark bronze / special
	Metal / fittings
	Matt black or brushed-nickel tapware from a mid-market premium range.
	TBC by sample/shop drawing
	Guest WCs — Fittings

	ST-01 / TL-01
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Bathroom floor
	Marble-look porcelain, matt anti-slip (R10). Supplier/Product Code to be selected.
	600×600 mm · laid to falls
	Guest WCs — full floor

	ST-01 / TL-01
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Bathroom walls
	Marble-look porcelain, satin. Supplier/Product Code to be selected.
	1200×600 mm · 9 mm
	Guest WCs — full-height wet walls

	WF-01
	[image: ] Warm white paint
	Wall paint
	Moisture- and mould-resistant matt emulsion, warm white, 2 coats on primer. Supplier/Product Code to be selected.
	—
	Guest WCs — non-tiled wall areas

	ST-03 / TL-01
	[image: ] Travertine
[image: ] Marble-look porcelain
	Feature wall
	Large-format travertine-look porcelain slab cladding (stone-effect) behind vanity with backlit mirror. Supplier/Product Code to be selected.
	1200×2400 mm slabs · 6–12 mm
	Guest WCs — vanity wall

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Moisture-resistant (MR) gypsum ceiling, anti-mould warm white matt paint, IP44 trimless downlights. Supplier/Product Code to be selected.
	12.5 mm MR board
	Guest WCs — full ceiling

	JN-02 / LT-01
	[image: ] Natural oak / wood
[image: ] 2700K LED
	Vanity
	Wall-hung vanity, engineered natural oak veneer / oak-effect hpl on mr-mdf, matt, soft-close drawers, LED under-glow. Supplier/Product Code to be selected.
	550 mm deep
	Guest WCs — vanity wall

	ST-05
	[image: ] Quartz
	Countertop
	Quartz top with undermount ceramic basin, polished. Supplier/Product Code to be selected.
	20 mm
	Guest WCs — vanity

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Sanitaryware
	Wall-hung rimless WC with concealed cistern, white gloss; brass-effect brushed pvd / powder-coat champagne bronze flush plate & mixers. Supplier/Product Code to be selected.
	—
	Guest WCs — WC and basin

	MT-01
	[image: ] Brushed brass
	Metal finishes
	Brass-effect brushed PVD / powder-coat champagne bronze — taps, shower set, towel rail, accessories. Supplier/Product Code to be selected.
	—
	Guest WCs — all fittings

	JN-02 / LT-01
	[image: ] Natural oak / wood
[image: ] 2700K LED
	Doors
	Full-height flush door, oak-effect laminate / veneer, concealed frame, concealed hinges, moisture-resistant core. Supplier/Product Code to be selected.
	800×2700 mm
	Guest WCs — entry door


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 2 · AFFORDABLE MODERN LUXURY
Corridors & Transitional Areas
Ground floor  ·  Lobby-to-wing links and the service passage
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	TL-01
	[image: ] Marble-look porcelain
	Floor / paving
	Continuous 120×120 cm porcelain, no inlay strip.
	120 cm
	Corridors & Transitional Areas — Flooring

	WF-01
	[image: ] Warm white paint
	Doors / window treatment
	Standard-height veneered flush doors with simple black lever handles; service doors painted flush to the wall.
	TBC by sample/shop drawing
	Corridors & Transitional Areas — Doors

	LT-01
	[image: ] 2700K LED
	Special finish / equipment
	One cove line, spots only where a door needs marking.
	TBC by sample/shop drawing
	Corridors & Transitional Areas — Lighting

	ST-01 / TL-01
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Flooring
	Marble-look rectified porcelain (warm beige / cream vein), matt-satin. Supplier/Product Code to be selected.
	1200×600 mm · 9–10 mm thick
	Corridors & Transitional Areas — full floor area

	WF-01
	[image: ] Warm white paint
	Walls
	Gypsum skim plaster, smooth level-5 finish ready for paint
	Plaster 10–13 mm
	Corridors & Transitional Areas — all walls except feature wall

	WF-01
	[image: ] Warm white paint
	Wall paint
	Wall paint: warm white / greige washable matt emulsion (Jotun Fenomastic or equal), 2 coats on primer. Supplier/Product Code to be selected.
	—
	Corridors & Transitional Areas — all painted walls

	ST-03 / TL-01
	[image: ] Travertine
[image: ] Marble-look porcelain
	Feature wall
	Large-format travertine-look porcelain slab cladding (stone-effect). Supplier/Product Code to be selected.
	1200×2400 mm slabs · 6–12 mm
	Corridors & Transitional Areas — end wall of corridor

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Gypsum board ceiling, warm white matt paint, perimeter shadow-gap with 2700K LED cove, trimless downlights. Supplier/Product Code to be selected.
	12.5 mm board · 2.9–3.0 m FFL
	Corridors & Transitional Areas — full ceiling

	WF-01 / MT-01
	[image: ] Warm white paint
[image: ] Brushed brass
	Skirting
	Recessed shadow-gap skirting, brass-effect brushed pvd / powder-coat champagne bronze trim / flush painted MDF
	80 mm high · 10 mm reveal
	Corridors & Transitional Areas — all wall perimeters

	JN-02
	[image: ] Natural oak / wood
	Joinery
	Engineered natural oak veneer / oak-effect HPL on MR-MDF, matt. Supplier/Product Code to be selected.
	18 mm core
	Corridors & Transitional Areas — built-in units and wall panelling

	JN-02 / LT-01
	[image: ] Natural oak / wood
[image: ] 2700K LED
	Doors
	Full-height flush door, oak-effect laminate / veneer, concealed frame, concealed hinges. Supplier/Product Code to be selected.
	900×2700 mm · 50 mm leaf
	Corridors & Transitional Areas — entry door(s)

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Metal finishes
	Brass-effect brushed PVD / powder-coat champagne bronze — door handles, inlays, light fittings, joinery pulls. Supplier/Product Code to be selected.
	—
	Corridors & Transitional Areas — all visible metalwork


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 2 · AFFORDABLE MODERN LUXURY
Maid's Room, Service WC & Boiler
Ground floor  ·  Maid's room on the north-east corner as drawn · service WC 1.82 m · boiler recess off the stair core
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	JN-02
	[image: ] Natural oak / wood
	Special finish / equipment
	Single bed, oak-effect melamine wardrobe with an open bay, laminate desk, roller blind on the drawn window.
	TBC by sample/shop drawing
	Maid's Room, Service WC & Boiler — Maid's room

	TL-01 / LT-01
	[image: ] Marble-look porcelain
[image: ] 2700K LED
	Special finish / equipment
	Large-format porcelain to 2.10 m, close-coupled WC, compact vanity — plumbing on the drawn wet wall.
	2.10 m
	Maid's Room, Service WC & Boiler — Service WC

	WF-01
	[image: ] Warm white paint
	Special finish / equipment
	Washer and dryer in a ventilated niche behind flush painted doors; boiler recess retained with a louvred panel.
	TBC by sample/shop drawing
	Maid's Room, Service WC & Boiler — Laundry & boiler

	TL-01 / WF-01 / LT-01
	[image: ] Marble-look porcelain
[image: ] Warm white paint
	Walls / paint
	Washable cream paint, matte beige porcelain floor, recessed spots at 3000 K.
	3000 K
	Maid's Room, Service WC & Boiler — Finishes & lighting

	ST-01 / TL-01
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Flooring
	Marble-look rectified porcelain (warm beige / cream vein), matt-satin. Supplier/Product Code to be selected.
	1200×600 mm · 9–10 mm thick
	Maid's Room, Service WC & Boiler — full floor area

	WF-01
	[image: ] Warm white paint
	Walls
	Gypsum skim plaster, smooth level-5 finish ready for paint
	Plaster 10–13 mm
	Maid's Room, Service WC & Boiler — all walls except feature wall

	WF-01
	[image: ] Warm white paint
	Wall paint
	Wall paint: warm white / greige washable matt emulsion (Jotun Fenomastic or equal), 2 coats on primer. Supplier/Product Code to be selected.
	—
	Maid's Room, Service WC & Boiler — all painted walls

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Gypsum board ceiling, warm white matt paint, perimeter shadow-gap with 2700K LED cove, trimless downlights. Supplier/Product Code to be selected.
	12.5 mm board · 2.9–3.0 m FFL
	Maid's Room, Service WC & Boiler — full ceiling

	WF-01 / MT-01
	[image: ] Warm white paint
[image: ] Brushed brass
	Skirting
	Recessed shadow-gap skirting, brass-effect brushed pvd / powder-coat champagne bronze trim / flush painted MDF
	80 mm high · 10 mm reveal
	Maid's Room, Service WC & Boiler — all wall perimeters

	JN-02
	[image: ] Natural oak / wood
	Joinery
	Engineered natural oak veneer / oak-effect HPL on MR-MDF, matt. Supplier/Product Code to be selected.
	18 mm core
	Maid's Room, Service WC & Boiler — built-in units and wall panelling

	JN-02 / LT-01
	[image: ] Natural oak / wood
[image: ] 2700K LED
	Doors
	Full-height flush door, oak-effect laminate / veneer, concealed frame, concealed hinges. Supplier/Product Code to be selected.
	900×2700 mm · 50 mm leaf
	Maid's Room, Service WC & Boiler — entry door(s)

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Metal finishes
	Brass-effect brushed PVD / powder-coat champagne bronze — door handles, inlays, light fittings, joinery pulls. Supplier/Product Code to be selected.
	—
	Maid's Room, Service WC & Boiler — all visible metalwork

	ST-01 / TL-01
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Bathroom floor
	Marble-look porcelain, matt anti-slip (R10). Supplier/Product Code to be selected.
	600×600 mm · laid to falls
	Maid's Room, Service WC & Boiler (service WC) — full floor

	ST-01 / TL-01
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Bathroom walls
	Marble-look porcelain, satin. Supplier/Product Code to be selected.
	1200×600 mm · 9 mm
	Maid's Room, Service WC & Boiler (service WC) — full-height wet walls

	WF-01
	[image: ] Warm white paint
	Wall paint
	Moisture- and mould-resistant matt emulsion, warm white, 2 coats on primer. Supplier/Product Code to be selected.
	—
	Maid's Room, Service WC & Boiler (service WC) — non-tiled wall areas

	ST-03 / TL-01
	[image: ] Travertine
[image: ] Marble-look porcelain
	Feature wall
	Large-format travertine-look porcelain slab cladding (stone-effect) behind vanity with backlit mirror. Supplier/Product Code to be selected.
	1200×2400 mm slabs · 6–12 mm
	Maid's Room, Service WC & Boiler (service WC) — vanity wall

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Moisture-resistant (MR) gypsum ceiling, anti-mould warm white matt paint, IP44 trimless downlights. Supplier/Product Code to be selected.
	12.5 mm MR board
	Maid's Room, Service WC & Boiler (service WC) — full ceiling

	JN-02 / LT-01
	[image: ] Natural oak / wood
[image: ] 2700K LED
	Vanity
	Wall-hung vanity, engineered natural oak veneer / oak-effect hpl on mr-mdf, matt, soft-close drawers, LED under-glow. Supplier/Product Code to be selected.
	550 mm deep
	Maid's Room, Service WC & Boiler (service WC) — vanity wall

	ST-01 / TL-01 / GL-01 / LT-01
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Shower area
	Marble-look porcelain walls, recessed niche, 8 mm clear tempered frameless glass screen; linear drain with tile insert; concealed thermostatic mixer & ceiling rain head. Supplier/Product Code to be selected.
	Screen 10 mm · drain 800 mm
	Maid's Room, Service WC & Boiler (service WC) — walk-in shower

	ST-05
	[image: ] Quartz
	Countertop
	Quartz top with undermount ceramic basin, polished. Supplier/Product Code to be selected.
	20 mm
	Maid's Room, Service WC & Boiler (service WC) — vanity

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Sanitaryware
	Wall-hung rimless WC with concealed cistern, white gloss; brass-effect brushed pvd / powder-coat champagne bronze flush plate & mixers. Supplier/Product Code to be selected.
	—
	Maid's Room, Service WC & Boiler (service WC) — WC and basin

	MT-01
	[image: ] Brushed brass
	Metal finishes
	Brass-effect brushed PVD / powder-coat champagne bronze — taps, shower set, towel rail, accessories. Supplier/Product Code to be selected.
	—
	Maid's Room, Service WC & Boiler (service WC) — all fittings

	JN-02 / LT-01
	[image: ] Natural oak / wood
[image: ] 2700K LED
	Doors
	Full-height flush door, oak-effect laminate / veneer, concealed frame, concealed hinges, moisture-resistant core. Supplier/Product Code to be selected.
	800×2700 mm
	Maid's Room, Service WC & Boiler (service WC) — entry door


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 2 · AFFORDABLE MODERN LUXURY
Central Lobby & Preparation Pantry
Upper floor  ·  3.75 × 2.50 m lobby · 1.60 m pantry run on the lobby wall
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	JN-02
	[image: ] Natural oak / wood
	Joinery / woodwork
	1.60 m run: modular lower cabinets with drawers, upper cabinets, and an open niche between. Beige-taupe matt fronts with an oak-effect accent, soft-close hardware.
	1.60 m
	Central Lobby & Preparation Pantry — Pantry joinery

	ST-05
	[image: ] Quartz
	Countertops / stone
	Engineered quartz top with a 400 mm undermount stainless sink and a black mixer tap. Water and waste run in the adjacent bathroom wall — no new wet wall.
	400 mm
	Central Lobby & Preparation Pantry — Countertop & sink

	SP-01
	[image: ] Dark bronze / special
	Special finish / equipment
	Two twin sockets above the counter for a kettle and coffee machine, one inside the niche, dedicated circuit and a local isolator.
	TBC by sample/shop drawing
	Central Lobby & Preparation Pantry — Electrical

	LT-01
	[image: ] 2700K LED
	Special finish / equipment
	Under-cabinet LED strip plus a warm niche strip on a night circuit.
	TBC by sample/shop drawing
	Central Lobby & Preparation Pantry — Lighting

	ST-01 / TL-01
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Flooring
	Marble-look rectified porcelain (warm beige / cream vein), matt-satin. Supplier/Product Code to be selected.
	1200×600 mm · 9–10 mm thick
	Central Lobby & Preparation Pantry — full floor area

	WF-01
	[image: ] Warm white paint
	Walls
	Gypsum skim plaster, smooth level-5 finish ready for paint
	Plaster 10–13 mm
	Central Lobby & Preparation Pantry — all walls except feature wall

	WF-01
	[image: ] Warm white paint
	Wall paint
	Wall paint: warm white / greige washable matt emulsion (Jotun Fenomastic or equal), 2 coats on primer. Supplier/Product Code to be selected.
	—
	Central Lobby & Preparation Pantry — all painted walls

	ST-03 / TL-01
	[image: ] Travertine
[image: ] Marble-look porcelain
	Feature wall
	Large-format travertine-look porcelain slab cladding (stone-effect). Supplier/Product Code to be selected.
	1200×2400 mm slabs · 6–12 mm
	Central Lobby & Preparation Pantry — pantry wall

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Gypsum board ceiling, warm white matt paint, perimeter shadow-gap with 2700K LED cove, trimless downlights. Supplier/Product Code to be selected.
	12.5 mm board · 2.9–3.0 m FFL
	Central Lobby & Preparation Pantry — full ceiling

	WF-01 / MT-01
	[image: ] Warm white paint
[image: ] Brushed brass
	Skirting
	Recessed shadow-gap skirting, brass-effect brushed pvd / powder-coat champagne bronze trim / flush painted MDF
	80 mm high · 10 mm reveal
	Central Lobby & Preparation Pantry — all wall perimeters

	JN-02
	[image: ] Natural oak / wood
	Joinery
	Engineered natural oak veneer / oak-effect HPL on MR-MDF, matt. Supplier/Product Code to be selected.
	18 mm core
	Central Lobby & Preparation Pantry — built-in units and wall panelling

	JN-02 / LT-01
	[image: ] Natural oak / wood
[image: ] 2700K LED
	Doors
	Full-height flush door, oak-effect laminate / veneer, concealed frame, concealed hinges. Supplier/Product Code to be selected.
	900×2700 mm · 50 mm leaf
	Central Lobby & Preparation Pantry — entry door(s)

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Metal finishes
	Brass-effect brushed PVD / powder-coat champagne bronze — door handles, inlays, light fittings, joinery pulls. Supplier/Product Code to be selected.
	—
	Central Lobby & Preparation Pantry — all visible metalwork

	JN-02
	[image: ] Natural oak / wood
	Kitchen cabinets
	Built-in pantry, warm beige/taupe matt lacquer lower & upper units with engineered natural oak veneer / oak-effect hpl on mr-mdf, matt open niche. Supplier/Product Code to be selected.
	600 / 350 mm deep
	Central Lobby & Preparation Pantry — pantry wall

	ST-05
	[image: ] Quartz
	Kitchen countertop
	Quartz, warm white with soft grey vein, polished with small undermount sink. Supplier/Product Code to be selected.
	20 mm
	Central Lobby & Preparation Pantry — pantry

	LT-01
	[image: ] 2700K LED
	Backsplash
	Matching stone slab with under-cabinet LED. Supplier/Product Code to be selected.
	Full height between units
	Central Lobby & Preparation Pantry — pantry


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 2 · AFFORDABLE MODERN LUXURY
Master Suite One — Bedroom
Upper floor  ·  4.05 × 5.40 m (4.10 m at the bed wall)
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	JN-01 / TX-01
	[image: ] Smoked walnut
[image: ] Textiles
	Walls / paint
	Prefabricated upholstered panel run in warm sand fabric, flanked by veneer-effect panels — no site-built walnut frame.
	TBC by sample/shop drawing
	Master Suite One — Bedroom — Headboard wall

	LT-01
	[image: ] 2700K LED
	Ceiling
	Single-step cove with spots; two catalogue pendants at the bedsides instead of a chandelier.
	TBC by sample/shop drawing
	Master Suite One — Bedroom — Ceiling & lighting

	JN-02 / WF-01
	[image: ] Natural oak / wood
[image: ] Warm white paint
	Floor / paving
	Premium paint plus one textured wallpaper wall; engineered oak-effect laminate flooring rather than solid or engineered oak.
	TBC by sample/shop drawing
	Master Suite One — Bedroom — Walls & floor

	ST-01 / TL-01
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Flooring
	Marble-look rectified porcelain (warm beige / cream vein), matt-satin. Supplier/Product Code to be selected.
	1200×600 mm · 9–10 mm thick
	Master Suite One — Bedroom — full floor area

	WF-01
	[image: ] Warm white paint
	Walls
	Gypsum skim plaster, smooth level-5 finish ready for paint
	Plaster 10–13 mm
	Master Suite One — Bedroom — all walls except feature wall

	WF-01
	[image: ] Warm white paint
	Wall paint
	Wall paint: warm white / greige washable matt emulsion (Jotun Fenomastic or equal), 2 coats on primer. Supplier/Product Code to be selected.
	—
	Master Suite One — Bedroom — all painted walls

	ST-03 / TL-01
	[image: ] Travertine
[image: ] Marble-look porcelain
	Feature wall
	Large-format travertine-look porcelain slab cladding (stone-effect). Supplier/Product Code to be selected.
	1200×2400 mm slabs · 6–12 mm
	Master Suite One — Bedroom — upholstered / timber-panelled headboard wall

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Gypsum board ceiling, warm white matt paint, perimeter shadow-gap with 2700K LED cove, trimless downlights. Supplier/Product Code to be selected.
	12.5 mm board · 2.9–3.0 m FFL
	Master Suite One — Bedroom — full ceiling

	WF-01 / MT-01
	[image: ] Warm white paint
[image: ] Brushed brass
	Skirting
	Recessed shadow-gap skirting, brass-effect brushed pvd / powder-coat champagne bronze trim / flush painted MDF
	80 mm high · 10 mm reveal
	Master Suite One — Bedroom — all wall perimeters

	JN-02
	[image: ] Natural oak / wood
	Joinery
	Engineered natural oak veneer / oak-effect HPL on MR-MDF, matt. Supplier/Product Code to be selected.
	18 mm core
	Master Suite One — Bedroom — built-in units and wall panelling

	JN-02 / LT-01
	[image: ] Natural oak / wood
[image: ] 2700K LED
	Doors
	Full-height flush door, oak-effect laminate / veneer, concealed frame, concealed hinges. Supplier/Product Code to be selected.
	900×2700 mm · 50 mm leaf
	Master Suite One — Bedroom — entry door(s)

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Metal finishes
	Brass-effect brushed PVD / powder-coat champagne bronze — door handles, inlays, light fittings, joinery pulls. Supplier/Product Code to be selected.
	—
	Master Suite One — Bedroom — all visible metalwork

	JN-02 / LT-01
	[image: ] Natural oak / wood
[image: ] 2700K LED
	Wardrobes
	Built-in full-height wardrobes, engineered natural oak veneer / oak-effect hpl on mr-mdf, matt, internal LED, soft-close. Supplier/Product Code to be selected.
	600 mm deep · floor to ceiling
	Master Suite One — Bedroom — wardrobe wall


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 2 · AFFORDABLE MODERN LUXURY
Master Suite One — Dressing
Upper floor  ·  Walk-in dressing bay off the bedroom, as drawn
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	LT-01
	[image: ] 2700K LED
	Joinery / woodwork
	Modular full-height units, matt beige fronts, soft-close drawers, hanging double rails, two open display sections with LED strips.
	TBC by sample/shop drawing
	Master Suite One — Dressing — Wardrobes

	ST-05
	[image: ] Quartz
	Joinery / woodwork
	Wall-hung 1.10 m veneer vanity with a quartz top, drawer bank and a simple round lit mirror.
	1.10 m
	Master Suite One — Dressing — Vanity

	LT-01
	[image: ] 2700K LED
	Special finish / equipment
	In-cabinet LED strips on door sensors, plus one flush ceiling fixture.
	TBC by sample/shop drawing
	Master Suite One — Dressing — Lighting

	ST-01 / TL-01
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Flooring
	Marble-look rectified porcelain (warm beige / cream vein), matt-satin. Supplier/Product Code to be selected.
	1200×600 mm · 9–10 mm thick
	Master Suite One — Dressing — full floor area

	WF-01
	[image: ] Warm white paint
	Walls
	Gypsum skim plaster, smooth level-5 finish ready for paint
	Plaster 10–13 mm
	Master Suite One — Dressing — all walls except feature wall

	WF-01
	[image: ] Warm white paint
	Wall paint
	Wall paint: warm white / greige washable matt emulsion (Jotun Fenomastic or equal), 2 coats on primer. Supplier/Product Code to be selected.
	—
	Master Suite One — Dressing — all painted walls

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Gypsum board ceiling, warm white matt paint, perimeter shadow-gap with 2700K LED cove, trimless downlights. Supplier/Product Code to be selected.
	12.5 mm board · 2.9–3.0 m FFL
	Master Suite One — Dressing — full ceiling

	WF-01 / MT-01
	[image: ] Warm white paint
[image: ] Brushed brass
	Skirting
	Recessed shadow-gap skirting, brass-effect brushed pvd / powder-coat champagne bronze trim / flush painted MDF
	80 mm high · 10 mm reveal
	Master Suite One — Dressing — all wall perimeters

	JN-02 / LT-01
	[image: ] Natural oak / wood
[image: ] 2700K LED
	Doors
	Full-height flush door, oak-effect laminate / veneer, concealed frame, concealed hinges. Supplier/Product Code to be selected.
	900×2700 mm · 50 mm leaf
	Master Suite One — Dressing — entry door(s)

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Metal finishes
	Brass-effect brushed PVD / powder-coat champagne bronze — door handles, inlays, light fittings, joinery pulls. Supplier/Product Code to be selected.
	—
	Master Suite One — Dressing — all visible metalwork

	JN-02 / MT-01 / GL-01 / LT-01
	[image: ] Natural oak / wood
[image: ] Brushed brass
	Wardrobes
	Full-height wardrobes, engineered natural oak veneer / oak-effect hpl on mr-mdf, matt fronts; bronze-tint glass display doors, integrated LED, leather-look internal drawers. Supplier/Product Code to be selected.
	600 mm deep · floor to ceiling
	Master Suite One — Dressing — all wardrobe walls

	ST-05
	[image: ] Quartz
	Joinery
	Dressing island / vanity with quartz, warm white with soft grey vein, polished top and full-length mirror. Supplier/Product Code to be selected.
	20 mm top
	Master Suite One — Dressing — centre / vanity wall


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 2 · AFFORDABLE MODERN LUXURY
Master Suite One — Ensuite
Upper floor  ·  Position and plumbing walls exactly as drawn
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	ST-01 / TL-01
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Floor / paving
	120×280 cm marble-look porcelain on the vanity and shower walls, matching large-format tile elsewhere.
	280 cm
	Master Suite One — Ensuite — Walls & floor

	ST-05
	[image: ] Quartz
	Joinery / woodwork
	1.40 m wall-hung veneer vanity, quartz top with an integrated basin, backlit mirror cabinet.
	1.40 m
	Master Suite One — Ensuite — Vanity

	GL-01 / LT-01
	[image: ] Clear glass
[image: ] 2700K LED
	Special finish / equipment
	Walk-in shower with a frameless fixed glass panel, linear drain, thermostatic mixer; wall-hung WC with a concealed cistern.
	TBC by sample/shop drawing
	Master Suite One — Ensuite — Shower & WC

	ST-01 / TL-01
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Bathroom floor
	Marble-look porcelain, matt anti-slip (R10). Supplier/Product Code to be selected.
	600×600 mm · laid to falls
	Master Suite One — Ensuite — full floor

	ST-01 / TL-01
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Bathroom walls
	Marble-look porcelain, satin. Supplier/Product Code to be selected.
	1200×600 mm · 9 mm
	Master Suite One — Ensuite — full-height wet walls

	WF-01
	[image: ] Warm white paint
	Wall paint
	Moisture- and mould-resistant matt emulsion, warm white, 2 coats on primer. Supplier/Product Code to be selected.
	—
	Master Suite One — Ensuite — non-tiled wall areas

	ST-03 / TL-01
	[image: ] Travertine
[image: ] Marble-look porcelain
	Feature wall
	Large-format travertine-look porcelain slab cladding (stone-effect) behind vanity with backlit mirror. Supplier/Product Code to be selected.
	1200×2400 mm slabs · 6–12 mm
	Master Suite One — Ensuite — vanity wall

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Moisture-resistant (MR) gypsum ceiling, anti-mould warm white matt paint, IP44 trimless downlights. Supplier/Product Code to be selected.
	12.5 mm MR board
	Master Suite One — Ensuite — full ceiling

	JN-02 / LT-01
	[image: ] Natural oak / wood
[image: ] 2700K LED
	Vanity
	Wall-hung vanity, engineered natural oak veneer / oak-effect hpl on mr-mdf, matt, soft-close drawers, LED under-glow. Supplier/Product Code to be selected.
	550 mm deep
	Master Suite One — Ensuite — vanity wall

	ST-01 / TL-01 / GL-01 / LT-01
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Shower area
	Marble-look porcelain walls, recessed niche, 8 mm clear tempered frameless glass screen; linear drain with tile insert; concealed thermostatic mixer & ceiling rain head. Supplier/Product Code to be selected.
	Screen 10 mm · drain 800 mm
	Master Suite One — Ensuite — walk-in shower

	ST-05
	[image: ] Quartz
	Countertop
	Quartz top with undermount ceramic basin, polished. Supplier/Product Code to be selected.
	20 mm
	Master Suite One — Ensuite — vanity

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Sanitaryware
	Wall-hung rimless WC with concealed cistern, white gloss; brass-effect brushed pvd / powder-coat champagne bronze flush plate & mixers. Supplier/Product Code to be selected.
	—
	Master Suite One — Ensuite — WC and basin

	MT-01
	[image: ] Brushed brass
	Metal finishes
	Brass-effect brushed PVD / powder-coat champagne bronze — taps, shower set, towel rail, accessories. Supplier/Product Code to be selected.
	—
	Master Suite One — Ensuite — all fittings

	JN-02 / LT-01
	[image: ] Natural oak / wood
[image: ] 2700K LED
	Doors
	Full-height flush door, oak-effect laminate / veneer, concealed frame, concealed hinges, moisture-resistant core. Supplier/Product Code to be selected.
	800×2700 mm
	Master Suite One — Ensuite — entry door


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 2 · AFFORDABLE MODERN LUXURY
Master Suite Two — Bedroom
Upper floor  ·  6.95 × 5.00 m (5.50 m to the terrace line), with the 4.90 × 1.20 m terrace
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	ST-01 / TL-01 / JN-02
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Walls / paint
	Two marble-look porcelain slabs with an oak-veneer frame, replacing book-matched natural stone.
	TBC by sample/shop drawing
	Master Suite Two — Bedroom — Bedhead wall

	LT-01
	[image: ] 2700K LED
	Ceiling
	Double cove, no coffers; one medium decorative fixture plus bedside wall lights.
	TBC by sample/shop drawing
	Master Suite Two — Bedroom — Ceiling & lighting

	TX-01
	[image: ] Textiles
	Special finish / equipment
	Upholstered bed and bench in performance fabric from a local maker; laminate-topped bedside tables with veneer fronts.
	TBC by sample/shop drawing
	Master Suite Two — Bedroom — Furniture

	ST-01 / TL-01
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Flooring
	Marble-look rectified porcelain (warm beige / cream vein), matt-satin. Supplier/Product Code to be selected.
	1200×600 mm · 9–10 mm thick
	Master Suite Two — Bedroom — full floor area

	WF-01
	[image: ] Warm white paint
	Walls
	Gypsum skim plaster, smooth level-5 finish ready for paint
	Plaster 10–13 mm
	Master Suite Two — Bedroom — all walls except feature wall

	WF-01
	[image: ] Warm white paint
	Wall paint
	Wall paint: warm white / greige washable matt emulsion (Jotun Fenomastic or equal), 2 coats on primer. Supplier/Product Code to be selected.
	—
	Master Suite Two — Bedroom — all painted walls

	ST-03 / TL-01
	[image: ] Travertine
[image: ] Marble-look porcelain
	Feature wall
	Large-format travertine-look porcelain slab cladding (stone-effect). Supplier/Product Code to be selected.
	1200×2400 mm slabs · 6–12 mm
	Master Suite Two — Bedroom — upholstered / timber-panelled headboard wall

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Gypsum board ceiling, warm white matt paint, perimeter shadow-gap with 2700K LED cove, trimless downlights. Supplier/Product Code to be selected.
	12.5 mm board · 2.9–3.0 m FFL
	Master Suite Two — Bedroom — full ceiling

	WF-01 / MT-01
	[image: ] Warm white paint
[image: ] Brushed brass
	Skirting
	Recessed shadow-gap skirting, brass-effect brushed pvd / powder-coat champagne bronze trim / flush painted MDF
	80 mm high · 10 mm reveal
	Master Suite Two — Bedroom — all wall perimeters

	JN-02
	[image: ] Natural oak / wood
	Joinery
	Engineered natural oak veneer / oak-effect HPL on MR-MDF, matt. Supplier/Product Code to be selected.
	18 mm core
	Master Suite Two — Bedroom — built-in units and wall panelling

	JN-02 / LT-01
	[image: ] Natural oak / wood
[image: ] 2700K LED
	Doors
	Full-height flush door, oak-effect laminate / veneer, concealed frame, concealed hinges. Supplier/Product Code to be selected.
	900×2700 mm · 50 mm leaf
	Master Suite Two — Bedroom — entry door(s)

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Metal finishes
	Brass-effect brushed PVD / powder-coat champagne bronze — door handles, inlays, light fittings, joinery pulls. Supplier/Product Code to be selected.
	—
	Master Suite Two — Bedroom — all visible metalwork

	JN-02 / LT-01
	[image: ] Natural oak / wood
[image: ] 2700K LED
	Wardrobes
	Built-in full-height wardrobes, engineered natural oak veneer / oak-effect hpl on mr-mdf, matt, internal LED, soft-close. Supplier/Product Code to be selected.
	600 mm deep · floor to ceiling
	Master Suite Two — Bedroom — wardrobe wall


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 2 · AFFORDABLE MODERN LUXURY
Master Suite Two — Dressing
Upper floor  ·  Dressing area as drawn between bedroom and ensuite
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	SP-01
	[image: ] Dark bronze / special
	Joinery / woodwork
	Modular units on three walls, matt taupe fronts, mix of hanging, drawers and two lit open bays.
	TBC by sample/shop drawing
	Master Suite Two — Dressing — Wardrobes

	ST-05
	[image: ] Quartz
	Special finish / equipment
	Freestanding 1.20 m drawer island with a quartz top instead of a bespoke fitted island.
	1.20 m
	Master Suite Two — Dressing — Central unit

	LT-01
	[image: ] 2700K LED
	Special finish / equipment
	Cabinet LED plus two flush ceiling fixtures.
	TBC by sample/shop drawing
	Master Suite Two — Dressing — Lighting

	ST-01 / TL-01
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Flooring
	Marble-look rectified porcelain (warm beige / cream vein), matt-satin. Supplier/Product Code to be selected.
	1200×600 mm · 9–10 mm thick
	Master Suite Two — Dressing — full floor area

	WF-01
	[image: ] Warm white paint
	Walls
	Gypsum skim plaster, smooth level-5 finish ready for paint
	Plaster 10–13 mm
	Master Suite Two — Dressing — all walls except feature wall

	WF-01
	[image: ] Warm white paint
	Wall paint
	Wall paint: warm white / greige washable matt emulsion (Jotun Fenomastic or equal), 2 coats on primer. Supplier/Product Code to be selected.
	—
	Master Suite Two — Dressing — all painted walls

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Gypsum board ceiling, warm white matt paint, perimeter shadow-gap with 2700K LED cove, trimless downlights. Supplier/Product Code to be selected.
	12.5 mm board · 2.9–3.0 m FFL
	Master Suite Two — Dressing — full ceiling

	WF-01 / MT-01
	[image: ] Warm white paint
[image: ] Brushed brass
	Skirting
	Recessed shadow-gap skirting, brass-effect brushed pvd / powder-coat champagne bronze trim / flush painted MDF
	80 mm high · 10 mm reveal
	Master Suite Two — Dressing — all wall perimeters

	JN-02 / LT-01
	[image: ] Natural oak / wood
[image: ] 2700K LED
	Doors
	Full-height flush door, oak-effect laminate / veneer, concealed frame, concealed hinges. Supplier/Product Code to be selected.
	900×2700 mm · 50 mm leaf
	Master Suite Two — Dressing — entry door(s)

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Metal finishes
	Brass-effect brushed PVD / powder-coat champagne bronze — door handles, inlays, light fittings, joinery pulls. Supplier/Product Code to be selected.
	—
	Master Suite Two — Dressing — all visible metalwork

	JN-02 / MT-01 / GL-01 / LT-01
	[image: ] Natural oak / wood
[image: ] Brushed brass
	Wardrobes
	Full-height wardrobes, engineered natural oak veneer / oak-effect hpl on mr-mdf, matt fronts; bronze-tint glass display doors, integrated LED, leather-look internal drawers. Supplier/Product Code to be selected.
	600 mm deep · floor to ceiling
	Master Suite Two — Dressing — all wardrobe walls

	ST-05
	[image: ] Quartz
	Joinery
	Dressing island / vanity with quartz, warm white with soft grey vein, polished top and full-length mirror. Supplier/Product Code to be selected.
	20 mm top
	Master Suite Two — Dressing — centre / vanity wall


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 2 · AFFORDABLE MODERN LUXURY
Master Suite Two — Ensuite
Upper floor  ·  Position and plumbing walls exactly as drawn
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	ST-03 / TL-01
	[image: ] Travertine
[image: ] Marble-look porcelain
	Floor / paving
	Travertine-look large-format porcelain throughout, one darker feature slab behind the vanity.
	TBC by sample/shop drawing
	Master Suite Two — Ensuite — Walls & floor

	ST-05
	[image: ] Quartz
	Joinery / woodwork
	1.80 m wall-hung double vanity, veneer fronts, quartz top with two integrated basins, full-width backlit mirror.
	1.80 m
	Master Suite Two — Ensuite — Vanity

	GL-01 / LT-01
	[image: ] Clear glass
[image: ] 2700K LED
	Special finish / equipment
	Walk-in shower with fixed glass, ceiling rain head and hand shower; wall-hung WC with concealed cistern.
	TBC by sample/shop drawing
	Master Suite Two — Ensuite — Shower & WC

	ST-01 / TL-01
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Bathroom floor
	Marble-look porcelain, matt anti-slip (R10). Supplier/Product Code to be selected.
	600×600 mm · laid to falls
	Master Suite Two — Ensuite — full floor

	ST-01 / TL-01
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Bathroom walls
	Marble-look porcelain, satin. Supplier/Product Code to be selected.
	1200×600 mm · 9 mm
	Master Suite Two — Ensuite — full-height wet walls

	WF-01
	[image: ] Warm white paint
	Wall paint
	Moisture- and mould-resistant matt emulsion, warm white, 2 coats on primer. Supplier/Product Code to be selected.
	—
	Master Suite Two — Ensuite — non-tiled wall areas

	ST-03 / TL-01
	[image: ] Travertine
[image: ] Marble-look porcelain
	Feature wall
	Large-format travertine-look porcelain slab cladding (stone-effect) behind vanity with backlit mirror. Supplier/Product Code to be selected.
	1200×2400 mm slabs · 6–12 mm
	Master Suite Two — Ensuite — vanity wall

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Moisture-resistant (MR) gypsum ceiling, anti-mould warm white matt paint, IP44 trimless downlights. Supplier/Product Code to be selected.
	12.5 mm MR board
	Master Suite Two — Ensuite — full ceiling

	JN-02 / LT-01
	[image: ] Natural oak / wood
[image: ] 2700K LED
	Vanity
	Wall-hung vanity, engineered natural oak veneer / oak-effect hpl on mr-mdf, matt, soft-close drawers, LED under-glow. Supplier/Product Code to be selected.
	550 mm deep
	Master Suite Two — Ensuite — vanity wall

	ST-01 / TL-01 / GL-01 / LT-01
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Shower area
	Marble-look porcelain walls, recessed niche, 8 mm clear tempered frameless glass screen; linear drain with tile insert; concealed thermostatic mixer & ceiling rain head. Supplier/Product Code to be selected.
	Screen 10 mm · drain 800 mm
	Master Suite Two — Ensuite — walk-in shower

	ST-05
	[image: ] Quartz
	Countertop
	Quartz top with undermount ceramic basin, polished. Supplier/Product Code to be selected.
	20 mm
	Master Suite Two — Ensuite — vanity

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Sanitaryware
	Wall-hung rimless WC with concealed cistern, white gloss; brass-effect brushed pvd / powder-coat champagne bronze flush plate & mixers. Supplier/Product Code to be selected.
	—
	Master Suite Two — Ensuite — WC and basin

	MT-01
	[image: ] Brushed brass
	Metal finishes
	Brass-effect brushed PVD / powder-coat champagne bronze — taps, shower set, towel rail, accessories. Supplier/Product Code to be selected.
	—
	Master Suite Two — Ensuite — all fittings

	JN-02 / LT-01
	[image: ] Natural oak / wood
[image: ] 2700K LED
	Doors
	Full-height flush door, oak-effect laminate / veneer, concealed frame, concealed hinges, moisture-resistant core. Supplier/Product Code to be selected.
	800×2700 mm
	Master Suite Two — Ensuite — entry door


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 2 · AFFORDABLE MODERN LUXURY
Bedroom Three
Upper floor  ·  4.30 × 4.30 m
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	WF-01
	[image: ] Warm white paint
	Walls / paint
	Premium paint with a grooved painted MDF panel behind the bed.
	TBC by sample/shop drawing
	Bedroom Three — Walls

	LT-01
	[image: ] 2700K LED
	Joinery / woodwork
	Modular wardrobe run and a laminate study desk with a veneer face and LED strip.
	TBC by sample/shop drawing
	Bedroom Three — Joinery

	LT-01
	[image: ] 2700K LED
	Special finish / equipment
	Cove plus spots; two simple wall reading lights.
	TBC by sample/shop drawing
	Bedroom Three — Lighting

	ST-01 / TL-01
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Flooring
	Marble-look rectified porcelain (warm beige / cream vein), matt-satin. Supplier/Product Code to be selected.
	1200×600 mm · 9–10 mm thick
	Bedroom Three — full floor area

	WF-01
	[image: ] Warm white paint
	Walls
	Gypsum skim plaster, smooth level-5 finish ready for paint
	Plaster 10–13 mm
	Bedroom Three — all walls except feature wall

	WF-01
	[image: ] Warm white paint
	Wall paint
	Wall paint: warm white / greige washable matt emulsion (Jotun Fenomastic or equal), 2 coats on primer. Supplier/Product Code to be selected.
	—
	Bedroom Three — all painted walls

	ST-03 / TL-01
	[image: ] Travertine
[image: ] Marble-look porcelain
	Feature wall
	Large-format travertine-look porcelain slab cladding (stone-effect). Supplier/Product Code to be selected.
	1200×2400 mm slabs · 6–12 mm
	Bedroom Three — upholstered / timber-panelled headboard wall

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Gypsum board ceiling, warm white matt paint, perimeter shadow-gap with 2700K LED cove, trimless downlights. Supplier/Product Code to be selected.
	12.5 mm board · 2.9–3.0 m FFL
	Bedroom Three — full ceiling

	WF-01 / MT-01
	[image: ] Warm white paint
[image: ] Brushed brass
	Skirting
	Recessed shadow-gap skirting, brass-effect brushed pvd / powder-coat champagne bronze trim / flush painted MDF
	80 mm high · 10 mm reveal
	Bedroom Three — all wall perimeters

	JN-02
	[image: ] Natural oak / wood
	Joinery
	Engineered natural oak veneer / oak-effect HPL on MR-MDF, matt. Supplier/Product Code to be selected.
	18 mm core
	Bedroom Three — built-in units and wall panelling

	JN-02 / LT-01
	[image: ] Natural oak / wood
[image: ] 2700K LED
	Doors
	Full-height flush door, oak-effect laminate / veneer, concealed frame, concealed hinges. Supplier/Product Code to be selected.
	900×2700 mm · 50 mm leaf
	Bedroom Three — entry door(s)

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Metal finishes
	Brass-effect brushed PVD / powder-coat champagne bronze — door handles, inlays, light fittings, joinery pulls. Supplier/Product Code to be selected.
	—
	Bedroom Three — all visible metalwork

	JN-02 / LT-01
	[image: ] Natural oak / wood
[image: ] 2700K LED
	Wardrobes
	Built-in full-height wardrobes, engineered natural oak veneer / oak-effect hpl on mr-mdf, matt, internal LED, soft-close. Supplier/Product Code to be selected.
	600 mm deep · floor to ceiling
	Bedroom Three — wardrobe wall


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 2 · AFFORDABLE MODERN LUXURY
Bedroom Four
Upper floor  ·  4.95 × 5.00 m (5.10 m structural bay)
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	WF-01
	[image: ] Warm white paint
	Walls / paint
	Textured paint or heavy wallpaper on the bed wall instead of fluted plaster.
	TBC by sample/shop drawing
	Bedroom Four — Walls

	TX-01
	[image: ] Textiles
	Special finish / equipment
	Upholstered bed in sand weave, veneer bedside tables, a fabric bench.
	TBC by sample/shop drawing
	Bedroom Four — Furniture

	LT-01
	[image: ] 2700K LED
	Special finish / equipment
	Cove, spots and two pendant drops at the bedsides.
	TBC by sample/shop drawing
	Bedroom Four — Lighting

	ST-01 / TL-01
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Flooring
	Marble-look rectified porcelain (warm beige / cream vein), matt-satin. Supplier/Product Code to be selected.
	1200×600 mm · 9–10 mm thick
	Bedroom Four — full floor area

	WF-01
	[image: ] Warm white paint
	Walls
	Gypsum skim plaster, smooth level-5 finish ready for paint
	Plaster 10–13 mm
	Bedroom Four — all walls except feature wall

	WF-01
	[image: ] Warm white paint
	Wall paint
	Wall paint: warm white / greige washable matt emulsion (Jotun Fenomastic or equal), 2 coats on primer. Supplier/Product Code to be selected.
	—
	Bedroom Four — all painted walls

	ST-03 / TL-01
	[image: ] Travertine
[image: ] Marble-look porcelain
	Feature wall
	Large-format travertine-look porcelain slab cladding (stone-effect). Supplier/Product Code to be selected.
	1200×2400 mm slabs · 6–12 mm
	Bedroom Four — upholstered / timber-panelled headboard wall

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Gypsum board ceiling, warm white matt paint, perimeter shadow-gap with 2700K LED cove, trimless downlights. Supplier/Product Code to be selected.
	12.5 mm board · 2.9–3.0 m FFL
	Bedroom Four — full ceiling

	WF-01 / MT-01
	[image: ] Warm white paint
[image: ] Brushed brass
	Skirting
	Recessed shadow-gap skirting, brass-effect brushed pvd / powder-coat champagne bronze trim / flush painted MDF
	80 mm high · 10 mm reveal
	Bedroom Four — all wall perimeters

	JN-02
	[image: ] Natural oak / wood
	Joinery
	Engineered natural oak veneer / oak-effect HPL on MR-MDF, matt. Supplier/Product Code to be selected.
	18 mm core
	Bedroom Four — built-in units and wall panelling

	JN-02 / LT-01
	[image: ] Natural oak / wood
[image: ] 2700K LED
	Doors
	Full-height flush door, oak-effect laminate / veneer, concealed frame, concealed hinges. Supplier/Product Code to be selected.
	900×2700 mm · 50 mm leaf
	Bedroom Four — entry door(s)

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Metal finishes
	Brass-effect brushed PVD / powder-coat champagne bronze — door handles, inlays, light fittings, joinery pulls. Supplier/Product Code to be selected.
	—
	Bedroom Four — all visible metalwork

	JN-02 / LT-01
	[image: ] Natural oak / wood
[image: ] 2700K LED
	Wardrobes
	Built-in full-height wardrobes, engineered natural oak veneer / oak-effect hpl on mr-mdf, matt, internal LED, soft-close. Supplier/Product Code to be selected.
	600 mm deep · floor to ceiling
	Bedroom Four — wardrobe wall


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 2 · AFFORDABLE MODERN LUXURY
Terraces
Upper floor  ·  Two terraces, 4.85 m and 4.90 m long, depths as drawn
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	ST-03 / TL-01
	[image: ] Travertine
[image: ] Marble-look porcelain
	Floor / paving
	20 mm travertine-look outdoor porcelain on pedestals rather than natural stone slabs.
	20 mm
	Terraces — Paving

	TL-01 / WF-01 / GL-01
	[image: ] Marble-look porcelain
[image: ] Warm white paint
	Metal / fittings
	Rendered and painted parapet with a porcelain coping; no metal or glass balustrade added.
	TBC by sample/shop drawing
	Terraces — Balustrade & parapet

	GL-01 / LT-01 / LS-01
	[image: ] Clear glass
[image: ] 2700K LED
	Special finish / equipment
	Aluminium-and-rope lounge set, fibreglass planters, recessed step lights and one wall wash per terrace.
	TBC by sample/shop drawing
	Terraces — Furniture & lighting

	ST-04 / TL-01 / JN-02
	[image: ] Limestone
[image: ] Marble-look porcelain
	Outdoor flooring
	Limestone-look exterior porcelain, R11 anti-slip with composite wood-effect decking, teak tone zones. Supplier/Product Code to be selected.
	600×600 mm · 20 mm
	Terraces — full terrace, laid to falls

	WF-01
	[image: ] Warm white paint
	Walls
	Exterior textured acrylic render, warm sand / beige, matt. Supplier/Product Code to be selected.
	—
	Terraces — parapet and back walls

	MT-01 / GL-01
	[image: ] Brushed brass
[image: ] Clear glass
	Balustrade
	Clear frameless laminated glass, brass-effect brushed pvd / powder-coat champagne bronze cap. Supplier/Product Code to be selected.
	12+12 mm · 1100 mm
	Terraces — open edges

	JN-02 / WF-01
	[image: ] Natural oak / wood
[image: ] Warm white paint
	Ceiling
	Exterior soffit, cement board painted warm white / wood-effect aluminium slats. Supplier/Product Code to be selected.
	—
	Terraces — covered area

	SP-01
	[image: ] Dark bronze / special
	Skirting
	Matching paver upstand
	100 mm
	Terraces — wall base

	MT-01
	[image: ] Brushed brass
	Doors
	Thermally broken slim aluminium sliding doors, dark bronze, double-glazed. Supplier/Product Code to be selected.
	Per elevation
	Terraces — opening to bedroom/lobby

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Metal finishes
	Dark bronze powder-coated aluminium / brass-effect brushed pvd / powder-coat champagne bronze lights. Supplier/Product Code to be selected.
	—
	Terraces — fixtures


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 2 · AFFORDABLE MODERN LUXURY
Staircase Landing & Feature Wall
Upper floor  ·  Per approved upper floor plan
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	ST-01 / TL-01
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Staircase treads
	Marble-look porcelain treads with bullnose nosing, matt anti-slip. Supplier/Product Code to be selected.
	Tread 300 mm · riser 160–170 mm · 20–30 mm
	Staircase Landing & Feature Wall — all flights and landings

	GL-01
	[image: ] Clear glass
	Balustrade
	Clear frameless laminated toughened glass in recessed floor channel, no handrail rods. Supplier/Product Code to be selected.
	12+12 mm laminated · 1100 mm high
	Staircase Landing & Feature Wall — open side of flights and landing

	MT-01
	[image: ] Brushed brass
	Handrail
	Brass-effect brushed PVD / powder-coat champagne bronze slim wall-mounted handrail. Supplier/Product Code to be selected.
	Ø40 mm
	Staircase Landing & Feature Wall — wall side

	LT-01
	[image: ] 2700K LED
	Stair lighting
	Recessed 2700K LED step lights / under-tread LED strip. Supplier/Product Code to be selected.
	—
	Staircase Landing & Feature Wall — every 2nd step

	WF-01
	[image: ] Warm white paint
	Walls
	Gypsum skim plaster, smooth level-5 finish
	—
	Staircase Landing & Feature Wall — stairwell walls

	WF-01
	[image: ] Warm white paint
	Wall paint
	Wall paint: warm white / greige washable matt emulsion (Jotun Fenomastic or equal), 2 coats on primer. Supplier/Product Code to be selected.
	—
	Staircase Landing & Feature Wall — stairwell walls

	ST-03 / TL-01
	[image: ] Travertine
[image: ] Marble-look porcelain
	Feature wall
	Large-format travertine-look porcelain slab cladding (stone-effect). Supplier/Product Code to be selected.
	1200×2400 mm slabs · 6–12 mm
	Staircase Landing & Feature Wall — double-height stair wall

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Gypsum board ceiling, warm white matt paint, perimeter shadow-gap with 2700K LED cove, trimless downlights; feature pendant to double-height void. Supplier/Product Code to be selected.
	—
	Staircase Landing & Feature Wall — soffit and void

	ST-01 / TL-01
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Skirting
	Stringer skirting in matching marble-look porcelain treads with bullnose nosing
	100 mm
	Staircase Landing & Feature Wall — wall stringer


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 2 · AFFORDABLE MODERN LUXURY
Shared Bathroom & WCs
Upper floor  ·  Per approved upper floor plan
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	ST-01 / TL-01
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Bathroom floor
	Marble-look porcelain, matt anti-slip (R10). Supplier/Product Code to be selected.
	600×600 mm · laid to falls
	Shared Bathroom & WCs — full floor

	ST-01 / TL-01
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Bathroom walls
	Marble-look porcelain, satin. Supplier/Product Code to be selected.
	1200×600 mm · 9 mm
	Shared Bathroom & WCs — full-height wet walls

	WF-01
	[image: ] Warm white paint
	Wall paint
	Moisture- and mould-resistant matt emulsion, warm white, 2 coats on primer. Supplier/Product Code to be selected.
	—
	Shared Bathroom & WCs — non-tiled wall areas

	ST-03 / TL-01
	[image: ] Travertine
[image: ] Marble-look porcelain
	Feature wall
	Large-format travertine-look porcelain slab cladding (stone-effect) behind vanity with backlit mirror. Supplier/Product Code to be selected.
	1200×2400 mm slabs · 6–12 mm
	Shared Bathroom & WCs — vanity wall

	WF-01 / LT-01
	[image: ] Warm white paint
[image: ] 2700K LED
	Ceiling
	Moisture-resistant (MR) gypsum ceiling, anti-mould warm white matt paint, IP44 trimless downlights. Supplier/Product Code to be selected.
	12.5 mm MR board
	Shared Bathroom & WCs — full ceiling

	JN-02 / LT-01
	[image: ] Natural oak / wood
[image: ] 2700K LED
	Vanity
	Wall-hung vanity, engineered natural oak veneer / oak-effect hpl on mr-mdf, matt, soft-close drawers, LED under-glow. Supplier/Product Code to be selected.
	550 mm deep
	Shared Bathroom & WCs — vanity wall

	ST-01 / TL-01 / GL-01 / LT-01
	[image: ] Beige marble
[image: ] Marble-look porcelain
	Shower area
	Marble-look porcelain walls, recessed niche, 8 mm clear tempered frameless glass screen; linear drain with tile insert; concealed thermostatic mixer & ceiling rain head. Supplier/Product Code to be selected.
	Screen 10 mm · drain 800 mm
	Shared Bathroom & WCs — walk-in shower

	ST-05
	[image: ] Quartz
	Countertop
	Quartz top with undermount ceramic basin, polished. Supplier/Product Code to be selected.
	20 mm
	Shared Bathroom & WCs — vanity

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Sanitaryware
	Wall-hung rimless WC with concealed cistern, white gloss; brass-effect brushed pvd / powder-coat champagne bronze flush plate & mixers. Supplier/Product Code to be selected.
	—
	Shared Bathroom & WCs — WC and basin

	MT-01
	[image: ] Brushed brass
	Metal finishes
	Brass-effect brushed PVD / powder-coat champagne bronze — taps, shower set, towel rail, accessories. Supplier/Product Code to be selected.
	—
	Shared Bathroom & WCs — all fittings

	JN-02 / LT-01
	[image: ] Natural oak / wood
[image: ] 2700K LED
	Doors
	Full-height flush door, oak-effect laminate / veneer, concealed frame, concealed hinges, moisture-resistant core. Supplier/Product Code to be selected.
	800×2700 mm
	Shared Bathroom & WCs — entry door


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 2 · AFFORDABLE MODERN LUXURY
Front Façade & Main Entrance
Exterior & outdoor  ·  Existing massing and proportions unchanged
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	ST-04 / TL-01 / WF-01
	[image: ] Limestone
[image: ] Marble-look porcelain
	Walls / paint
	Warm greige textured render across most of the façade, with 60×120 cm stone-look porcelain applied only to the entrance frame and the two ground-floor piers — roughly 20% of the area instead of full limestone.
	120 cm · 20%
	Front Façade & Main Entrance — Cladding strategy

	JN-01 / JN-02
	[image: ] Smoked walnut
[image: ] Natural oak / wood
	Special finish / equipment
	Full-height door in an oak-effect aluminium composite panel rather than solid walnut; same proportions and pivot look.
	TBC by sample/shop drawing
	Front Façade & Main Entrance — Entrance

	SP-01
	[image: ] Dark bronze / special
	Metal / fittings
	Dark powder-coated aluminium window and screen frames, standard profiles.
	TBC by sample/shop drawing
	Front Façade & Main Entrance — Metalwork

	LT-01
	[image: ] 2700K LED
	Special finish / equipment
	Recessed uplights at the piers, one linear grazer over the entrance, 2700 K, on a single dusk sensor.
	2700 K
	Front Façade & Main Entrance — Lighting

	ST-04 / TL-01
	[image: ] Limestone
[image: ] Marble-look porcelain
	Outdoor paving
	Limestone-look exterior porcelain, R11 anti-slip. Supplier/Product Code to be selected.
	600×600 / 900×600 mm · 20–30 mm
	Front Façade & Main Entrance — paths, terraces and hard landscape

	ST-04 / WF-01
	[image: ] Limestone
[image: ] Warm white paint
	Outdoor walls
	Natural beige limestone cladding with exterior acrylic render, warm sand, matt. Supplier/Product Code to be selected.
	30 mm stone · render 15 mm
	Front Façade & Main Entrance — façades, boundary and feature walls

	MT-01
	[image: ] Brushed brass
	Outdoor metal
	Dark bronze powder-coated aluminium (gates, pergola, frames, trims). Supplier/Product Code to be selected.
	—
	Front Façade & Main Entrance — all exterior metalwork

	JN-02
	[image: ] Natural oak / wood
	Outdoor timber
	Composite wood-effect decking, teak tone. Supplier/Product Code to be selected.
	140×21 mm boards
	Front Façade & Main Entrance — decks, cladding and slatted screens

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Outdoor lighting
	2700K IP65 bollards, step lights, uplights and linear wall-washers, dark bronze. Supplier/Product Code to be selected.
	—
	Front Façade & Main Entrance — per lighting layout


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 2 · AFFORDABLE MODERN LUXURY
Rear Façade & Terrace
Exterior & outdoor  ·  As drawn, opening onto the pool terrace
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	ST-03 / TL-01
	[image: ] Travertine
[image: ] Marble-look porcelain
	Floor / paving
	Travertine-look outdoor porcelain, 60×120 cm, laid on sand-cement.
	120 cm
	Rear Façade & Terrace — Paving

	JN-02 / WF-01
	[image: ] Natural oak / wood
[image: ] Warm white paint
	Special finish / equipment
	Painted soffit with a slim slat-effect aluminium band instead of a full timber ceiling.
	TBC by sample/shop drawing
	Rear Façade & Terrace — Soffit

	LT-01
	[image: ] 2700K LED
	Special finish / equipment
	Recessed downlights in the soffit and a continuous LED line at the wall junction.
	TBC by sample/shop drawing
	Rear Façade & Terrace — Lighting

	ST-04 / TL-01
	[image: ] Limestone
[image: ] Marble-look porcelain
	Outdoor paving
	Limestone-look exterior porcelain, R11 anti-slip. Supplier/Product Code to be selected.
	600×600 / 900×600 mm · 20–30 mm
	Rear Façade & Terrace — paths, terraces and hard landscape

	ST-04 / WF-01
	[image: ] Limestone
[image: ] Warm white paint
	Outdoor walls
	Natural beige limestone cladding with exterior acrylic render, warm sand, matt. Supplier/Product Code to be selected.
	30 mm stone · render 15 mm
	Rear Façade & Terrace — façades, boundary and feature walls

	MT-01
	[image: ] Brushed brass
	Outdoor metal
	Dark bronze powder-coated aluminium (gates, pergola, frames, trims). Supplier/Product Code to be selected.
	—
	Rear Façade & Terrace — all exterior metalwork

	JN-02
	[image: ] Natural oak / wood
	Outdoor timber
	Composite wood-effect decking, teak tone. Supplier/Product Code to be selected.
	140×21 mm boards
	Rear Façade & Terrace — decks, cladding and slatted screens

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Outdoor lighting
	2700K IP65 bollards, step lights, uplights and linear wall-washers, dark bronze. Supplier/Product Code to be selected.
	—
	Rear Façade & Terrace — per lighting layout


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 2 · AFFORDABLE MODERN LUXURY
Swimming Pool
Exterior & outdoor  ·  11.00 × 5.92 m — exactly the area allocated on the site plan
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	WF-01 / GL-01
	[image: ] Warm white paint
[image: ] Clear glass
	Walls / paint
	Pale sand-tone glass mosaic or premium pool plaster instead of full stone lining, giving the same water colour.
	TBC by sample/shop drawing
	Swimming Pool — Finish

	TL-01
	[image: ] Marble-look porcelain
	Floor / paving
	20 mm anti-slip porcelain coping with a flush edge; matching porcelain deck.
	20 mm
	Swimming Pool — Coping & deck

	LT-01
	[image: ] 2700K LED
	Special finish / equipment
	Four underwater LEDs plus recessed step lights, 2700 K on the deck.
	2700 K
	Swimming Pool — Lighting

	ST-04 / TL-01
	[image: ] Limestone
[image: ] Marble-look porcelain
	Outdoor paving
	Limestone-look exterior porcelain, R11 anti-slip. Supplier/Product Code to be selected.
	600×600 / 900×600 mm · 20–30 mm
	Swimming Pool — paths, terraces and hard landscape

	ST-04 / WF-01
	[image: ] Limestone
[image: ] Warm white paint
	Outdoor walls
	Natural beige limestone cladding with exterior acrylic render, warm sand, matt. Supplier/Product Code to be selected.
	30 mm stone · render 15 mm
	Swimming Pool — façades, boundary and feature walls

	MT-01
	[image: ] Brushed brass
	Outdoor metal
	Dark bronze powder-coated aluminium (gates, pergola, frames, trims). Supplier/Product Code to be selected.
	—
	Swimming Pool — all exterior metalwork

	JN-02
	[image: ] Natural oak / wood
	Outdoor timber
	Composite wood-effect decking, teak tone. Supplier/Product Code to be selected.
	140×21 mm boards
	Swimming Pool — decks, cladding and slatted screens

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Outdoor lighting
	2700K IP65 bollards, step lights, uplights and linear wall-washers, dark bronze. Supplier/Product Code to be selected.
	—
	Swimming Pool — per lighting layout

	ST-04 / TL-01 / GL-01
	[image: ] Limestone
[image: ] Marble-look porcelain
	Pool finish
	Pool interior in sand-beige glass mosaic / porcelain, coping in honed limestone-look exterior porcelain, r11 anti-slip. Supplier/Product Code to be selected.
	11.00×5.92 m pool · coping 600×400×30 mm
	Swimming Pool — pool shell and coping

	ST-04 / TL-01
	[image: ] Limestone
[image: ] Marble-look porcelain
	Pool deck
	Limestone-look exterior porcelain, R11 anti-slip, anti-slip. Supplier/Product Code to be selected.
	600×600 mm · 20 mm
	Swimming Pool — sun deck


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 2 · AFFORDABLE MODERN LUXURY
BBQ & Outdoor Kitchen
Exterior & outdoor  ·  In the position allocated on the site plan, under an architectural canopy
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	TL-01
	[image: ] Marble-look porcelain
	Countertops / stone
	Blockwork carcass clad in outdoor porcelain with a 20 mm porcelain worktop; built-in gas BBQ, stainless sink and an under-counter fridge.
	20 mm
	BBQ & Outdoor Kitchen — Counter

	JN-02 / WF-01 / MT-01
	[image: ] Natural oak / wood
[image: ] Warm white paint
	Special finish / equipment
	Powder-coated steel frame with a painted soffit and an aluminium slat band, replacing the bronze-framed timber canopy.
	TBC by sample/shop drawing
	BBQ & Outdoor Kitchen — Canopy

	LT-01
	[image: ] 2700K LED
	Special finish / equipment
	Task strip under the canopy edge plus one warm downlight per bay.
	TBC by sample/shop drawing
	BBQ & Outdoor Kitchen — Lighting

	ST-04 / TL-01
	[image: ] Limestone
[image: ] Marble-look porcelain
	Outdoor paving
	Limestone-look exterior porcelain, R11 anti-slip. Supplier/Product Code to be selected.
	600×600 / 900×600 mm · 20–30 mm
	BBQ & Outdoor Kitchen — paths, terraces and hard landscape

	ST-04 / WF-01
	[image: ] Limestone
[image: ] Warm white paint
	Outdoor walls
	Natural beige limestone cladding with exterior acrylic render, warm sand, matt. Supplier/Product Code to be selected.
	30 mm stone · render 15 mm
	BBQ & Outdoor Kitchen — façades, boundary and feature walls

	MT-01
	[image: ] Brushed brass
	Outdoor metal
	Dark bronze powder-coated aluminium (gates, pergola, frames, trims). Supplier/Product Code to be selected.
	—
	BBQ & Outdoor Kitchen — all exterior metalwork

	JN-02
	[image: ] Natural oak / wood
	Outdoor timber
	Composite wood-effect decking, teak tone. Supplier/Product Code to be selected.
	140×21 mm boards
	BBQ & Outdoor Kitchen — decks, cladding and slatted screens

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Outdoor lighting
	2700K IP65 bollards, step lights, uplights and linear wall-washers, dark bronze. Supplier/Product Code to be selected.
	—
	BBQ & Outdoor Kitchen — per lighting layout

	ST-05
	[image: ] Quartz
	Outdoor countertop
	Flamed / leathered dark granite or exterior sintered stone, UV stable. Supplier/Product Code to be selected.
	30 mm
	BBQ & Outdoor Kitchen — BBQ counter with sink & fridge

	JN-02 / MT-01
	[image: ] Natural oak / wood
[image: ] Brushed brass
	Outdoor cabinets
	Marine-grade stainless steel carcasses with dark bronze / wood-effect HPL doors. Supplier/Product Code to be selected.
	—
	BBQ & Outdoor Kitchen — base units

	JN-02 / MT-01
	[image: ] Natural oak / wood
[image: ] Brushed brass
	Canopy
	Architectural canopy, dark bronze aluminium with wood-effect slat soffit. Supplier/Product Code to be selected.
	Per drawing
	BBQ & Outdoor Kitchen — over BBQ


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 2 · AFFORDABLE MODERN LUXURY
Outdoor Lounge
Exterior & outdoor  ·  Raised platform at the north-east of the site plan
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	SP-01
	[image: ] Dark bronze / special
	Special finish / equipment
	Modular aluminium-and-rope lounge with quick-dry cushions in sand; ceramic-top low tables.
	TBC by sample/shop drawing
	Outdoor Lounge — Furniture

	JN-02
	[image: ] Natural oak / wood
	Special finish / equipment
	Powder-coated aluminium pergola with fixed slats instead of a hardwood structure.
	TBC by sample/shop drawing
	Outdoor Lounge — Structure

	TL-01 / JN-02
	[image: ] Marble-look porcelain
[image: ] Natural oak / wood
	Floor / paving
	Wood-effect outdoor porcelain rather than hardwood decking — no annual oiling.
	TBC by sample/shop drawing
	Outdoor Lounge — Deck

	ST-04 / TL-01
	[image: ] Limestone
[image: ] Marble-look porcelain
	Outdoor paving
	Limestone-look exterior porcelain, R11 anti-slip. Supplier/Product Code to be selected.
	600×600 / 900×600 mm · 20–30 mm
	Outdoor Lounge — paths, terraces and hard landscape

	ST-04 / WF-01
	[image: ] Limestone
[image: ] Warm white paint
	Outdoor walls
	Natural beige limestone cladding with exterior acrylic render, warm sand, matt. Supplier/Product Code to be selected.
	30 mm stone · render 15 mm
	Outdoor Lounge — façades, boundary and feature walls

	MT-01
	[image: ] Brushed brass
	Outdoor metal
	Dark bronze powder-coated aluminium (gates, pergola, frames, trims). Supplier/Product Code to be selected.
	—
	Outdoor Lounge — all exterior metalwork

	JN-02
	[image: ] Natural oak / wood
	Outdoor timber
	Composite wood-effect decking, teak tone. Supplier/Product Code to be selected.
	140×21 mm boards
	Outdoor Lounge — decks, cladding and slatted screens

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Outdoor lighting
	2700K IP65 bollards, step lights, uplights and linear wall-washers, dark bronze. Supplier/Product Code to be selected.
	—
	Outdoor Lounge — per lighting layout

	JN-02 / MT-01 / TX-01
	[image: ] Natural oak / wood
[image: ] Brushed brass
	Pergola
	Dark bronze aluminium pergola with wood-effect louvres, outdoor-fabric upholstery in sand / taupe. Supplier/Product Code to be selected.
	Per drawing
	Outdoor Lounge — seating area


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 2 · AFFORDABLE MODERN LUXURY
Outdoor Dining
Exterior & outdoor  ·  Adjacent to the BBQ zone as drawn
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	SP-01
	[image: ] Dark bronze / special
	Countertops / stone
	2.40 m aluminium table with a ceramic top and eight woven dining chairs.
	2.40 m
	Outdoor Dining — Table & seating

	SP-01
	[image: ] Dark bronze / special
	Special finish / equipment
	Extension of the BBQ canopy rather than a separate structure — one build, two uses.
	TBC by sample/shop drawing
	Outdoor Dining — Shade

	LT-01
	[image: ] 2700K LED
	Special finish / equipment
	Two warm pendants under the canopy on a dimmer.
	TBC by sample/shop drawing
	Outdoor Dining — Lighting

	ST-04 / TL-01
	[image: ] Limestone
[image: ] Marble-look porcelain
	Outdoor paving
	Limestone-look exterior porcelain, R11 anti-slip. Supplier/Product Code to be selected.
	600×600 / 900×600 mm · 20–30 mm
	Outdoor Dining — paths, terraces and hard landscape

	ST-04 / WF-01
	[image: ] Limestone
[image: ] Warm white paint
	Outdoor walls
	Natural beige limestone cladding with exterior acrylic render, warm sand, matt. Supplier/Product Code to be selected.
	30 mm stone · render 15 mm
	Outdoor Dining — façades, boundary and feature walls

	MT-01
	[image: ] Brushed brass
	Outdoor metal
	Dark bronze powder-coated aluminium (gates, pergola, frames, trims). Supplier/Product Code to be selected.
	—
	Outdoor Dining — all exterior metalwork

	JN-02
	[image: ] Natural oak / wood
	Outdoor timber
	Composite wood-effect decking, teak tone. Supplier/Product Code to be selected.
	140×21 mm boards
	Outdoor Dining — decks, cladding and slatted screens

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Outdoor lighting
	2700K IP65 bollards, step lights, uplights and linear wall-washers, dark bronze. Supplier/Product Code to be selected.
	—
	Outdoor Dining — per lighting layout

	JN-02 / MT-01 / TX-01
	[image: ] Natural oak / wood
[image: ] Brushed brass
	Pergola
	Dark bronze aluminium pergola with wood-effect louvres, outdoor-fabric upholstery in sand / taupe. Supplier/Product Code to be selected.
	Per drawing
	Outdoor Dining — seating area


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 2 · AFFORDABLE MODERN LUXURY
Children's Play Area
Exterior & outdoor  ·  Dedicated zone in the position shown on the site plan
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	FL-01
	[image: ] EPDM rubber
	Special finish / equipment
	Bonded rubber safety surface in sand tone — the same product family as Option 1, in a plain colour.
	TBC by sample/shop drawing
	Children's Play Area — Surfacing

	JN-02
	[image: ] Natural oak / wood
	Special finish / equipment
	Catalogue climbing frame and swing in timber-effect finish rather than a bespoke oak structure.
	TBC by sample/shop drawing
	Children's Play Area — Equipment

	LT-01 / LS-01
	[image: ] 2700K LED
[image: ] Planting
	Special finish / equipment
	Low hedge screen from the pool deck and two bollard lights.
	TBC by sample/shop drawing
	Children's Play Area — Screening & lighting

	ST-04 / TL-01
	[image: ] Limestone
[image: ] Marble-look porcelain
	Outdoor paving
	Limestone-look exterior porcelain, R11 anti-slip. Supplier/Product Code to be selected.
	600×600 / 900×600 mm · 20–30 mm
	Children's Play Area — paths, terraces and hard landscape

	ST-04 / WF-01
	[image: ] Limestone
[image: ] Warm white paint
	Outdoor walls
	Natural beige limestone cladding with exterior acrylic render, warm sand, matt. Supplier/Product Code to be selected.
	30 mm stone · render 15 mm
	Children's Play Area — façades, boundary and feature walls

	MT-01
	[image: ] Brushed brass
	Outdoor metal
	Dark bronze powder-coated aluminium (gates, pergola, frames, trims). Supplier/Product Code to be selected.
	—
	Children's Play Area — all exterior metalwork

	JN-02
	[image: ] Natural oak / wood
	Outdoor timber
	Composite wood-effect decking, teak tone. Supplier/Product Code to be selected.
	140×21 mm boards
	Children's Play Area — decks, cladding and slatted screens

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Outdoor lighting
	2700K IP65 bollards, step lights, uplights and linear wall-washers, dark bronze. Supplier/Product Code to be selected.
	—
	Children's Play Area — per lighting layout

	FL-01
	[image: ] EPDM rubber
	Safety flooring
	Wet-pour EPDM rubber safety surface, sand / sage colours. Supplier/Product Code to be selected.
	40–80 mm (per fall height, EN 1177)
	Children's Play Area — whole play zone


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
OPTION 2 · AFFORDABLE MODERN LUXURY
Garden, Walkways & Lighting
Exterior & outdoor  ·  Full plot as shown on the site plan
	REF.
	SAMPLE
	ITEM
	MATERIAL · COLOUR · FINISH
	SIZE / THICKNESS
	EXACT LOCATION

	LT-01 / LS-01
	[image: ] 2700K LED
[image: ] Planting
	Special finish / equipment
	Six repeated species: olive, frangipani, clipped ficus hedge, agave, lantana groundcover and buffalo lawn. Fewer semi-mature specimens, more small stock allowed to grow in.
	TBC by sample/shop drawing
	Garden, Walkways & Lighting — Planting

	TL-01
	[image: ] Marble-look porcelain
	Special finish / equipment
	Outdoor porcelain pavers on compacted base with gravel margins instead of continuous natural stone.
	TBC by sample/shop drawing
	Garden, Walkways & Lighting — Walkways

	WF-01 / GL-01 / LS-01
	[image: ] Warm white paint
[image: ] Clear glass
	Special finish / equipment
	Built-in rendered planters painted to match the façade, plus fibreglass pots at the entrance.
	TBC by sample/shop drawing
	Garden, Walkways & Lighting — Planters

	LT-01 / LS-01
	[image: ] 2700K LED
[image: ] Planting
	Special finish / equipment
	Eight tree uplights, bollards along the pedestrian route and step lights, all 2700 K on one dusk-to-midnight circuit.
	2700 K
	Garden, Walkways & Lighting — Lighting

	TL-01 / WF-01
	[image: ] Marble-look porcelain
[image: ] Warm white paint
	Special finish / equipment
	Rendered boundary wall with a porcelain-clad gate frame; dark powder-coated aluminium sliding vehicle gate and matching pedestrian gate.
	TBC by sample/shop drawing
	Garden, Walkways & Lighting — Boundary & gates

	ST-04 / TL-01
	[image: ] Limestone
[image: ] Marble-look porcelain
	Outdoor paving
	Limestone-look exterior porcelain, R11 anti-slip. Supplier/Product Code to be selected.
	600×600 / 900×600 mm · 20–30 mm
	Garden, Walkways & Lighting — paths, terraces and hard landscape

	ST-04 / WF-01
	[image: ] Limestone
[image: ] Warm white paint
	Outdoor walls
	Natural beige limestone cladding with exterior acrylic render, warm sand, matt. Supplier/Product Code to be selected.
	30 mm stone · render 15 mm
	Garden, Walkways & Lighting — façades, boundary and feature walls

	MT-01
	[image: ] Brushed brass
	Outdoor metal
	Dark bronze powder-coated aluminium (gates, pergola, frames, trims). Supplier/Product Code to be selected.
	—
	Garden, Walkways & Lighting — all exterior metalwork

	JN-02
	[image: ] Natural oak / wood
	Outdoor timber
	Composite wood-effect decking, teak tone. Supplier/Product Code to be selected.
	140×21 mm boards
	Garden, Walkways & Lighting — decks, cladding and slatted screens

	MT-01 / LT-01
	[image: ] Brushed brass
[image: ] 2700K LED
	Outdoor lighting
	2700K IP65 bollards, step lights, uplights and linear wall-washers, dark bronze. Supplier/Product Code to be selected.
	—
	Garden, Walkways & Lighting — per lighting layout

	ST-04 / WF-01 / LS-01
	[image: ] Limestone
[image: ] Warm white paint
	Softscape
	Natural lawn, olive / palm feature trees, low hedges, raised planters in render / limestone, drip irrigation. Supplier/Product Code to be selected.
	—
	Garden, Walkways & Lighting — planting beds and lawn


Status: Approved design unless marked TBC. Reference codes are project schedule identifiers only.
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